From 4b1216203d83ff57820312dafb9a0b3500f03f80 Mon Sep 17 00:00:00 2001
From: Martin Sperl <kernel@martin.sperl.org>
Date: Tue, 22 Dec 2015 20:13:08 +0000
Subject: [PATCH 255/381] clk: bcm2835: added missing clock register
 definitions

Added missing CTRL and DIV clock register definitions for:
PCM, SLIM, TCNT, TEC, TD0, TD1

Register information taken from:
https://rawgit.com/msperl/rpi-registers/master/rpi-registers.html#CM
which extracted the information from the header files shared by
Broadcom/rpi foundation in this file:
http://www.broadcom.com/docs/support/videocore/Brcm_Android_ICS_Graphics_Stack.tar.gz

Signed-off-by: Martin Sperl <kernel@martin.sperl.org>
Reviewed-by: Eric Anholt <eric@anholt.net>
Signed-off-by: Stephen Boyd <sboyd@codeaurora.org>
(cherry picked from commit 2103a2156119b30f5924af2a1094227954be4617)
---
 drivers/clk/bcm/clk-bcm2835.c | 13 +++++++++++++
 1 file changed, 13 insertions(+)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -88,10 +88,23 @@
 #define CM_HSMDIV		0x08c
 #define CM_OTPCTL		0x090
 #define CM_OTPDIV		0x094
+#define CM_PCMCTL		0x098
+#define CM_PCMDIV		0x09c
 #define CM_PWMCTL		0x0a0
 #define CM_PWMDIV		0x0a4
+#define CM_SLIMCTL		0x0a8
+#define CM_SLIMDIV		0x0ac
 #define CM_SMICTL		0x0b0
 #define CM_SMIDIV		0x0b4
+/* no definition for 0x0b8  and 0x0bc */
+#define CM_TCNTCTL		0x0c0
+#define CM_TCNTDIV		0x0c4
+#define CM_TECCTL		0x0c8
+#define CM_TECDIV		0x0cc
+#define CM_TD0CTL		0x0d0
+#define CM_TD0DIV		0x0d4
+#define CM_TD1CTL		0x0d8
+#define CM_TD1DIV		0x0dc
 #define CM_TSENSCTL		0x0e0
 #define CM_TSENSDIV		0x0e4
 #define CM_TIMERCTL		0x0e8
