/dts-v1/;

#include "bcm6345.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Broadcom BCM96345GW2 reference board";
	compatible = "brcm,bcm96345gw2", "brcm,bcm6345";

	chosen {
		bootargs = "root=/dev/mtdblock2 rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
	};
};
