From 6d490f62a4c7f11c552591bdd08eda3636aa0db9 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Tue, 7 Jun 2016 15:06:15 -0700
Subject: [PATCH 3/3] bgmac: Maintain some netdev statistics

Add a few netdev statistics to report transmitted and received bytes and
packets and a few obvious errors.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/broadcom/bgmac.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -246,6 +246,8 @@ err_dma_head:
 
 err_drop:
 	dev_kfree_skb(skb);
+	net_dev->stats.tx_dropped++;
+	net_dev->stats.tx_errors++;
 	return NETDEV_TX_OK;
 }
 
@@ -284,6 +286,8 @@ static void bgmac_dma_tx_free(struct bgm
 				       DMA_TO_DEVICE);
 
 		if (slot->skb) {
+			bgmac->net_dev->stats.tx_bytes += slot->skb->len;
+			bgmac->net_dev->stats.tx_packets++;
 			bytes_compl += slot->skb->len;
 			pkts_compl++;
 
@@ -464,6 +468,7 @@ static int bgmac_dma_rx_read(struct bgma
 				bgmac_err(bgmac, "Found poisoned packet at slot %d, DMA issue!\n",
 					  ring->start);
 				put_page(virt_to_head_page(buf));
+				bgmac->net_dev->stats.rx_errors++;
 				break;
 			}
 
@@ -471,6 +476,8 @@ static int bgmac_dma_rx_read(struct bgma
 				bgmac_err(bgmac, "Found oversized packet at slot %d, DMA issue!\n",
 					  ring->start);
 				put_page(virt_to_head_page(buf));
+				bgmac->net_dev->stats.rx_length_errors++;
+				bgmac->net_dev->stats.rx_errors++;
 				break;
 			}
 
@@ -481,6 +488,7 @@ static int bgmac_dma_rx_read(struct bgma
 			if (unlikely(!skb)) {
 				bgmac_err(bgmac, "build_skb failed\n");
 				put_page(virt_to_head_page(buf));
+				bgmac->net_dev->stats.rx_errors++;
 				break;
 			}
 			skb_put(skb, BGMAC_RX_FRAME_OFFSET +
@@ -490,6 +498,8 @@ static int bgmac_dma_rx_read(struct bgma
 
 			skb_checksum_none_assert(skb);
 			skb->protocol = eth_type_trans(skb, bgmac->net_dev);
+			bgmac->net_dev->stats.rx_bytes += len;
+			bgmac->net_dev->stats.rx_packets++;
 			napi_gro_receive(&bgmac->napi, skb);
 			handled++;
 		} while (0);
