#!/bin/sh
#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/ipq806x.sh

board_config_update

board=$(ipq806x_board_name)

case "$board" in
c2600)
	ucidef_set_led_usbdev "usb1" "USB 1" "usb_2:blue" "2-1"
	ucidef_set_led_usbdev "usb2" "USB 2" "usb_4:blue" "4-1"
	ucidef_set_led_netdev "wan" "WAN" "wan:blue" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "lan:blue" "br-lan"
	ucidef_set_led_default "general" "general" "ledgnr:blue" "1"
	;;
d7800 |\
r7500 |\
r7800)
	ucidef_set_led_usbdev "usb1" "USB 1" "${board}:white:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB 2" "${board}:white:usb3" "3-1"
	ucidef_set_led_netdev "wan" "WAN" "${board}:white:wan" "eth0"
	ucidef_set_led_ide "esata" "eSATA" "${board}:amber:esata"
	ucidef_set_led_default "wps" "WPS" "${board}:white:wps" "0"
	ucidef_set_led_default "rfkill" "rfkill" "${board}:white:rfkill" "0"
	;;
ea8500)
	ucidef_set_led_wlan "wifi" "WIFI" "ea8500:green:wifi" "phy0radio"
	ucidef_set_led_default "wps" "WPS" "ea8500:green:wps" "0"
	;;
*)
	;;
esac

board_config_flush

exit 0
