From c1f2dd85b1d53093fdf7af80ece7517ffed00f3a Mon Sep 17 00:00:00 2001
From: Remi Pommarel <repk@triplefau.lt>
Date: Sun, 6 Dec 2015 17:22:48 +0100
Subject: [PATCH 254/381] clk: bcm2835: Add PWM clock support

Register the pwm clock for bcm2835.

Signed-off-by: Remi Pommarel <repk@triplefau.lt>
Reviewed-by: Eric Anholt <eric@anholt.net>
Signed-off-by: Michael Turquette <mturquette@baylibre.com>
(cherry picked from commit cfbab8fbab9c330aca963095a439c451ac97c0dd)
---
 drivers/clk/bcm/clk-bcm2835.c       | 13 +++++++++++++
 include/dt-bindings/clock/bcm2835.h |  3 ++-
 2 files changed, 15 insertions(+), 1 deletion(-)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -807,6 +807,16 @@ static const struct bcm2835_clock_data b
 	.frac_bits = 8,
 };
 
+static const struct bcm2835_clock_data bcm2835_clock_pwm_data = {
+	.name = "pwm",
+	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),
+	.parents = bcm2835_clock_per_parents,
+	.ctl_reg = CM_PWMCTL,
+	.div_reg = CM_PWMDIV,
+	.int_bits = 12,
+	.frac_bits = 12,
+};
+
 struct bcm2835_pll {
 	struct clk_hw hw;
 	struct bcm2835_cprman *cprman;
@@ -1601,6 +1611,9 @@ static int bcm2835_clk_probe(struct plat
 				  cprman->regs + CM_PERIICTL, CM_GATE_BIT,
 				  0, &cprman->regs_lock);
 
+	clks[BCM2835_CLOCK_PWM] =
+		bcm2835_register_clock(cprman, &bcm2835_clock_pwm_data);
+
 	return of_clk_add_provider(dev->of_node, of_clk_src_onecell_get,
 				   &cprman->onecell);
 }
--- a/include/dt-bindings/clock/bcm2835.h
+++ b/include/dt-bindings/clock/bcm2835.h
@@ -43,5 +43,6 @@
 #define BCM2835_CLOCK_TSENS		27
 #define BCM2835_CLOCK_EMMC		28
 #define BCM2835_CLOCK_PERI_IMAGE	29
+#define BCM2835_CLOCK_PWM		30
 
-#define BCM2835_CLOCK_COUNT		30
+#define BCM2835_CLOCK_COUNT		31
