From 3abeeb47bad351f535efdf176cd623ac8ff7cfe3 Mon Sep 17 00:00:00 2001
From: Eric Nelson <eric@nelint.com>
Date: Sat, 3 Oct 2015 08:18:50 -0700
Subject: [PATCH 372/381] [media] rc-core: define a default timeout for drivers

A default timeout value of 125 ms should work for all decoders.

Declare a constant to help standardize its' use.

Signed-off-by: Eric Nelson <eric@nelint.com>
Signed-off-by: Mauro Carvalho Chehab <mchehab@osg.samsung.com>
---
 include/media/rc-core.h | 1 +
 1 file changed, 1 insertion(+)

--- a/include/media/rc-core.h
+++ b/include/media/rc-core.h
@@ -239,6 +239,7 @@ static inline void init_ir_raw_event(str
 	memset(ev, 0, sizeof(*ev));
 }
 
+#define IR_DEFAULT_TIMEOUT	MS_TO_NS(125)
 #define IR_MAX_DURATION         500000000	/* 500 ms */
 #define US_TO_NS(usec)		((usec) * 1000)
 #define MS_TO_US(msec)		((msec) * 1000)
