From cc64a36830bcae96e5df48d69f69057a8df539f2 Mon Sep 17 00:00:00 2001
From: Mario Kleiner <mario.kleiner.de@gmail.com>
Date: Fri, 6 May 2016 19:26:05 +0200
Subject: [PATCH 343/381] drm/vc4: Fix get_vblank_counter with proper no-op for
 Linux 4.4+

get_vblank_counter hooked up to drm_vblank_count() which alway was
non-sensical but didn't hurt in the past. Since Linux 4.4 it
triggers a WARN_ON_ONCE in drm_update_vblank_count on first vblank
irq disable, so fix it by hooking to drm_vblank_no_hw_counter().

Tested against Raspian kernel 4.4.8 tree on RPi 2B.

Signed-off-by: Mario Kleiner <mario.kleiner.de@gmail.com>
Cc: Eric Anholt <eric@anholt.net>
Signed-off-by: Eric Anholt <eric@anholt.net>
---
 drivers/gpu/drm/vc4/vc4_drv.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/gpu/drm/vc4/vc4_drv.c
+++ b/drivers/gpu/drm/vc4/vc4_drv.c
@@ -102,7 +102,7 @@ static struct drm_driver vc4_drm_driver
 
 	.enable_vblank = vc4_enable_vblank,
 	.disable_vblank = vc4_disable_vblank,
-	.get_vblank_counter = drm_vblank_count,
+	.get_vblank_counter = drm_vblank_no_hw_counter,
 
 #if defined(CONFIG_DEBUG_FS)
 	.debugfs_init = vc4_debugfs_init,
