From 0d2dc82a9fe4a2325df235180812065bcb47c3a6 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 19 Apr 2016 14:23:30 -0700
Subject: [PATCH 271/381] bcm2708: Add RASPBERRYPI_POWER to the defconfigs.

This will be used by the GPU driver for powering on HDMI at boot time
and for 3D hang reset.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/configs/bcm2709_defconfig | 2 ++
 arch/arm/configs/bcmrpi_defconfig  | 2 ++
 2 files changed, 4 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -71,6 +71,7 @@ CONFIG_NEON=y
 CONFIG_KERNEL_MODE_NEON=y
 CONFIG_BINFMT_MISC=m
 # CONFIG_SUSPEND is not set
+CONFIG_PM=y
 CONFIG_NET=y
 CONFIG_PACKET=y
 CONFIG_UNIX=y
@@ -1116,6 +1117,7 @@ CONFIG_FB_TFT_FBTFT_DEVICE=m
 CONFIG_MAILBOX=y
 CONFIG_BCM2835_MBOX=y
 # CONFIG_IOMMU_SUPPORT is not set
+CONFIG_RASPBERRYPI_POWER=y
 CONFIG_EXTCON=m
 CONFIG_EXTCON_ARIZONA=m
 CONFIG_IIO=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -64,6 +64,7 @@ CONFIG_CPU_FREQ_GOV_CONSERVATIVE=y
 CONFIG_VFP=y
 CONFIG_BINFMT_MISC=m
 # CONFIG_SUSPEND is not set
+CONFIG_PM=y
 CONFIG_NET=y
 CONFIG_PACKET=y
 CONFIG_UNIX=y
@@ -1123,6 +1124,7 @@ CONFIG_FB_TFT_FBTFT_DEVICE=m
 CONFIG_MAILBOX=y
 CONFIG_BCM2835_MBOX=y
 # CONFIG_IOMMU_SUPPORT is not set
+CONFIG_RASPBERRYPI_POWER=y
 CONFIG_EXTCON=m
 CONFIG_EXTCON_ARIZONA=m
 CONFIG_IIO=m
