From 8269ed007349714e9ef0e3408a68159d763145dd Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 8 Jan 2016 08:33:17 +0100
Subject: [PATCH 043/102] mfd: mt6397: int_con and int_status may vary in
 location

MT6323 has the INT_CON and INT_STATUS located at a different position.
Make the registers locations configurable.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/mfd/mt6397-core.c       |   27 +++++++++++++++++----------
 include/linux/mfd/mt6397/core.h |    2 ++
 2 files changed, 19 insertions(+), 10 deletions(-)

--- a/drivers/mfd/mt6397-core.c
+++ b/drivers/mfd/mt6397-core.c
@@ -69,8 +69,10 @@ static void mt6397_irq_sync_unlock(struc
 {
 	struct mt6397_chip *mt6397 = irq_data_get_irq_chip_data(data);
 
-	regmap_write(mt6397->regmap, MT6397_INT_CON0, mt6397->irq_masks_cur[0]);
-	regmap_write(mt6397->regmap, MT6397_INT_CON1, mt6397->irq_masks_cur[1]);
+	regmap_write(mt6397->regmap, mt6397->int_con[0],
+		     mt6397->irq_masks_cur[0]);
+	regmap_write(mt6397->regmap, mt6397->int_con[1],
+		     mt6397->irq_masks_cur[1]);
 
 	mutex_unlock(&mt6397->irqlock);
 }
@@ -147,8 +149,8 @@ static irqreturn_t mt6397_irq_thread(int
 {
 	struct mt6397_chip *mt6397 = data;
 
-	mt6397_irq_handle_reg(mt6397, MT6397_INT_STATUS0, 0);
-	mt6397_irq_handle_reg(mt6397, MT6397_INT_STATUS1, 16);
+	mt6397_irq_handle_reg(mt6397, mt6397->int_status[0], 0);
+	mt6397_irq_handle_reg(mt6397, mt6397->int_status[1], 16);
 
 	return IRQ_HANDLED;
 }
@@ -177,8 +179,8 @@ static int mt6397_irq_init(struct mt6397
 	mutex_init(&mt6397->irqlock);
 
 	/* Mask all interrupt sources */
-	regmap_write(mt6397->regmap, MT6397_INT_CON0, 0x0);
-	regmap_write(mt6397->regmap, MT6397_INT_CON1, 0x0);
+	regmap_write(mt6397->regmap, mt6397->int_con[0], 0x0);
+	regmap_write(mt6397->regmap, mt6397->int_con[1], 0x0);
 
 	mt6397->irq_domain = irq_domain_add_linear(mt6397->dev->of_node,
 		MT6397_IRQ_NR, &mt6397_irq_domain_ops, mt6397);
@@ -203,8 +205,8 @@ static int mt6397_irq_suspend(struct dev
 {
 	struct mt6397_chip *chip = dev_get_drvdata(dev);
 
-	regmap_write(chip->regmap, MT6397_INT_CON0, chip->wake_mask[0]);
-	regmap_write(chip->regmap, MT6397_INT_CON1, chip->wake_mask[1]);
+	regmap_write(chip->regmap, chip->int_con[0], chip->wake_mask[0]);
+	regmap_write(chip->regmap, chip->int_con[1], chip->wake_mask[1]);
 
 	enable_irq_wake(chip->irq);
 
@@ -215,8 +217,8 @@ static int mt6397_irq_resume(struct devi
 {
 	struct mt6397_chip *chip = dev_get_drvdata(dev);
 
-	regmap_write(chip->regmap, MT6397_INT_CON0, chip->irq_masks_cur[0]);
-	regmap_write(chip->regmap, MT6397_INT_CON1, chip->irq_masks_cur[1]);
+	regmap_write(chip->regmap, chip->int_con[0], chip->irq_masks_cur[0]);
+	regmap_write(chip->regmap, chip->int_con[1], chip->irq_masks_cur[1]);
 
 	disable_irq_wake(chip->irq);
 
@@ -237,6 +239,11 @@ static int mt6397_probe(struct platform_
 		return -ENOMEM;
 
 	mt6397->dev = &pdev->dev;
+	mt6397->int_con[0] = MT6397_INT_CON0;
+	mt6397->int_con[1] = MT6397_INT_CON1;
+	mt6397->int_status[0] = MT6397_INT_STATUS0;
+	mt6397->int_status[1] = MT6397_INT_STATUS1;
+
 	/*
 	 * mt6397 MFD is child device of soc pmic wrapper.
 	 * Regmap is set from its parent.
--- a/include/linux/mfd/mt6397/core.h
+++ b/include/linux/mfd/mt6397/core.h
@@ -60,6 +60,8 @@ struct mt6397_chip {
 	u16 wake_mask[2];
 	u16 irq_masks_cur[2];
 	u16 irq_masks_cache[2];
+	u16 int_con[2];
+	u16 int_status[2];
 };
 
 #endif /* __MFD_MT6397_CORE_H__ */
