/*
 * Copyright (C) 2014-15 Synopsys, Inc. (www.synopsys.com)
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

/include/ "skeleton.dtsi"

/ {
	model = "Synopsys ARC HS38 nSIM simulator";
	compatible = "snps,nsim_hs";
	interrupt-parent = <&core_intc>;

	chosen {
		bootargs = "earlycon=arc_uart,mmio32,0xc0fc1000,115200n8 console=ttyARC0,115200n8";
	};

	aliases {
		serial0 = &arcuart0;
	};

	fpga {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;

		/* child and parent address space 1:1 mapped */
		ranges;

		core_intc: core-interrupt-controller {
			compatible = "snps,archs-intc";
			interrupt-controller;
			#interrupt-cells = <1>;
		};

		idu_intc: idu-interrupt-controller {
			compatible = "snps,archs-idu-intc";
			interrupt-controller;
			interrupt-parent = <&core_intc>;

			/*
			 * <hwirq  distribution>
			 * distribution: 0=RR; 1=cpu0, 2=cpu1, 4=cpu2, 8=cpu3
			 */
			#interrupt-cells = <2>;

			/*
			 * upstream irqs to core intc - downstream these are
			 * "COMMON" irq 0,1..
			 */
			interrupts = <24 25 26 27 28 29 30 31>;
		};

		arcuart0: serial@c0fc1000 {
			compatible = "snps,arc-uart";
			reg = <0xc0fc1000 0x100>;
			interrupt-parent = <&idu_intc>;
			interrupts = <0 0>;
			clock-frequency = <80000000>;
			current-speed = <115200>;
			status = "okay";
		};

		arcpct0: pct {
			compatible = "snps,archs-pct";
			#interrupt-cells = <1>;
			interrupts = <20>;
		};
	};
};
