From 8e5424e69f62b365bcb158c6d4b28b7e1c100664 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Thu, 7 Apr 2016 12:44:24 +0100
Subject: [PATCH 235/381] config: Enable CONFIG_IPV6_ROUTER_PREF for networks
 with multiple routers

---
 arch/arm/configs/bcm2709_defconfig | 1 +
 arch/arm/configs/bcmrpi_defconfig  | 1 +
 2 files changed, 2 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -101,6 +101,7 @@ CONFIG_INET_XFRM_MODE_TUNNEL=m
 CONFIG_INET_XFRM_MODE_BEET=m
 CONFIG_INET_LRO=m
 CONFIG_INET_DIAG=m
+CONFIG_IPV6_ROUTER_PREF=y
 CONFIG_INET6_AH=m
 CONFIG_INET6_ESP=m
 CONFIG_INET6_IPCOMP=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -95,6 +95,7 @@ CONFIG_INET_XFRM_MODE_TUNNEL=m
 CONFIG_INET_XFRM_MODE_BEET=m
 CONFIG_INET_LRO=m
 CONFIG_INET_DIAG=m
+CONFIG_IPV6_ROUTER_PREF=y
 CONFIG_INET6_AH=m
 CONFIG_INET6_ESP=m
 CONFIG_INET6_IPCOMP=m
