From 5869509197e8b3b6080f212a22e7d10310fc0a9b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Noralf=20Tr=C3=B8nnes?= <noralf@tronnes.org>
Date: Sat, 15 Aug 2015 20:47:07 +0200
Subject: [PATCH 052/381] bcm2835: Match with BCM2708 Device Trees
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Noralf Trønnes <noralf@tronnes.org>
---
 arch/arm/boot/dts/bcm2835-rpi-b-plus.dts | 132 ++++++++++++++++++---
 arch/arm/boot/dts/bcm2835-rpi-b.dts      | 115 ++++++++++++++++--
 arch/arm/boot/dts/bcm2835.dtsi           | 195 +++----------------------------
 3 files changed, 237 insertions(+), 205 deletions(-)

--- a/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
@@ -1,30 +1,128 @@
 /dts-v1/;
-#include "bcm2835-rpi.dtsi"
+#include "bcm2835.dtsi"
 
 / {
 	compatible = "raspberrypi,model-b-plus", "brcm,bcm2835";
 	model = "Raspberry Pi Model B+";
-
-	leds {
-		act {
-			gpios = <&gpio 47 0>;
-		};
-
-		pwr {
-			label = "PWR";
-			gpios = <&gpio 35 0>;
-			default-state = "keep";
-			linux,default-trigger = "default-on";
-		};
-	};
 };
 
 &gpio {
-	pinctrl-0 = <&gpioout &alt0 &i2s_alt0 &alt3>;
+	spi0_pins: spi0_pins {
+		brcm,pins = <7 8 9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
 
-	/* I2S interface */
-	i2s_alt0: i2s_alt0 {
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
 		brcm,pins = <18 19 20 21>;
-		brcm,function = <BCM2835_FSEL_ALT0>;
+		brcm,function = <4>; /* alt0 */
+	};
+};
+
+&mmc {
+	status = "okay";
+	bus-width = <4>;
+};
+
+&fb {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&gpio 35 0>;
+	};
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		uart1_clkrate = <&uart1>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
 	};
 };
--- a/arch/arm/boot/dts/bcm2835-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b.dts
@@ -1,17 +1,118 @@
 /dts-v1/;
-#include "bcm2835-rpi.dtsi"
+#include "bcm2835.dtsi"
 
 / {
 	compatible = "raspberrypi,model-b", "brcm,bcm2835";
 	model = "Raspberry Pi Model B";
+};
 
-	leds {
-		act {
-			gpios = <&gpio 16 1>;
-		};
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <7 8 9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <28 29 30 31>;
+		brcm,function = <6>; /* alt2 */
 	};
 };
 
-&gpio {
-	pinctrl-0 = <&gpioout &alt0 &alt3>;
+&mmc {
+	status = "okay";
+	bus-width = <4>;
+};
+
+&fb {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 16 1>;
+	};
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		uart1_clkrate = <&uart1>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
 };
--- a/arch/arm/boot/dts/bcm2835.dtsi
+++ b/arch/arm/boot/dts/bcm2835.dtsi
@@ -1,206 +1,39 @@
-#include <dt-bindings/pinctrl/bcm2835.h>
-#include <dt-bindings/clock/bcm2835.h>
-#include "skeleton.dtsi"
+#include "bcm2708_common.dtsi"
 
 / {
 	compatible = "brcm,bcm2835";
 	model = "BCM2835";
-	interrupt-parent = <&intc>;
 
 	chosen {
-		bootargs = "earlyprintk console=ttyAMA0";
+		bootargs = "";
 	};
 
 	soc {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <1>;
-		ranges = <0x7e000000 0x20000000 0x02000000>;
+		ranges = <0x7e000000 0x20000000 0x01000000>;
 		dma-ranges = <0x40000000 0x00000000 0x20000000>;
 
 		timer@7e003000 {
 			compatible = "brcm,bcm2835-system-timer";
 			reg = <0x7e003000 0x1000>;
 			interrupts = <1 0>, <1 1>, <1 2>, <1 3>;
-			/* This could be a reference to BCM2835_CLOCK_TIMER,
-			 * but we don't have the driver using the common clock
-			 * support yet.
-			 */
 			clock-frequency = <1000000>;
 		};
 
-		dma: dma@7e007000 {
-			compatible = "brcm,bcm2835-dma";
-			reg = <0x7e007000 0xf00>;
-			interrupts = <1 16>,
-				     <1 17>,
-				     <1 18>,
-				     <1 19>,
-				     <1 20>,
-				     <1 21>,
-				     <1 22>,
-				     <1 23>,
-				     <1 24>,
-				     <1 25>,
-				     <1 26>,
-				     <1 27>,
-				     <1 28>;
-
-			#dma-cells = <1>;
-			brcm,dma-channel-mask = <0x7f35>;
-		};
-
-		intc: interrupt-controller@7e00b200 {
-			compatible = "brcm,bcm2835-armctrl-ic";
-			reg = <0x7e00b200 0x200>;
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		watchdog@7e100000 {
-			compatible = "brcm,bcm2835-pm-wdt";
-			reg = <0x7e100000 0x28>;
-		};
-
-		clocks: cprman@7e101000 {
-			compatible = "brcm,bcm2835-cprman";
-			#clock-cells = <1>;
-			reg = <0x7e101000 0x2000>;
-
-			/* CPRMAN derives everything from the platform's
-			 * oscillator.
-			 */
-			clocks = <&clk_osc>;
-		};
-
-		rng@7e104000 {
-			compatible = "brcm,bcm2835-rng";
-			reg = <0x7e104000 0x10>;
-		};
-
-		mailbox: mailbox@7e00b800 {
-			compatible = "brcm,bcm2835-mbox";
-			reg = <0x7e00b880 0x40>;
-			interrupts = <0 1>;
-			#mbox-cells = <0>;
-		};
-
-		gpio: gpio@7e200000 {
-			compatible = "brcm,bcm2835-gpio";
-			reg = <0x7e200000 0xb4>;
-			/*
-			 * The GPIO IP block is designed for 3 banks of GPIOs.
-			 * Each bank has a GPIO interrupt for itself.
-			 * There is an overall "any bank" interrupt.
-			 * In order, these are GIC interrupts 17, 18, 19, 20.
-			 * Since the BCM2835 only has 2 banks, the 2nd bank
-			 * interrupt output appears to be mirrored onto the
-			 * 3rd bank's interrupt signal.
-			 * So, a bank0 interrupt shows up on 17, 20, and
-			 * a bank1 interrupt shows up on 18, 19, 20!
-			 */
-			interrupts = <2 17>, <2 18>, <2 19>, <2 20>;
-
-			gpio-controller;
-			#gpio-cells = <2>;
-
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		uart0: uart@7e201000 {
-			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
-			reg = <0x7e201000 0x1000>;
-			interrupts = <2 25>;
-			clocks = <&clocks BCM2835_CLOCK_UART>,
-				 <&clocks BCM2835_CLOCK_VPU>;
-			clock-names = "uartclk", "apb_pclk";
-			arm,primecell-periphid = <0x00241011>;
-		};
-
-		i2s: i2s@7e203000 {
-			compatible = "brcm,bcm2835-i2s";
-			reg = <0x7e203000 0x24>,
-			      <0x7e101098 0x08>;
-
-			dmas = <&dma 2>,
-			       <&dma 3>;
-			dma-names = "tx", "rx";
-			status = "disabled";
-		};
-
-		spi: spi@7e204000 {
-			compatible = "brcm,bcm2835-spi";
-			reg = <0x7e204000 0x1000>;
-			interrupts = <2 22>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		i2c0: i2c@7e205000 {
-			compatible = "brcm,bcm2835-i2c";
-			reg = <0x7e205000 0x1000>;
-			interrupts = <2 21>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		sdhci: sdhci@7e300000 {
-			compatible = "brcm,bcm2835-sdhci";
-			reg = <0x7e300000 0x100>;
-			interrupts = <2 30>;
-			clocks = <&clocks BCM2835_CLOCK_EMMC>;
-			status = "disabled";
-		};
-
-		i2c1: i2c@7e804000 {
-			compatible = "brcm,bcm2835-i2c";
-			reg = <0x7e804000 0x1000>;
-			interrupts = <2 21>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		i2c2: i2c@7e805000 {
-			compatible = "brcm,bcm2835-i2c";
-			reg = <0x7e805000 0x1000>;
-			interrupts = <2 21>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		usb@7e980000 {
-			compatible = "brcm,bcm2835-usb";
-			reg = <0x7e980000 0x10000>;
-			interrupts = <1 9>;
-		};
-
 		arm-pmu {
 			compatible = "arm,arm1176-pmu";
 		};
-	};
 
-	clocks {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <0>;
-
-		/* The oscillator is the root of the clock tree. */
-		clk_osc: clock@3 {
-			compatible = "fixed-clock";
-			reg = <3>;
-			#clock-cells = <0>;
-			clock-output-names = "osc";
-			clock-frequency = <19200000>;
+		aux_enable: aux_enable@0x7e215004 {
+			compatible = "bcrm,bcm2835-aux-enable";
+			reg = <0x7e215004 0x04>;
 		};
-
 	};
 };
+
+&intc {
+	compatible = "brcm,bcm2835-armctrl-ic";
+};
+
+&watchdog {
+	status = "okay";
+};
