From 2f681005c89b65de1a2aa1426a41cc7b9e243c74 Mon Sep 17 00:00:00 2001
From: Florian Meier <florian.meier@koalo.de>
Date: Fri, 22 Nov 2013 19:21:34 +0100
Subject: [PATCH 064/381] ASoC: Add support for Rpi-DAC

---
 sound/soc/bcm/Kconfig       |   7 +++
 sound/soc/bcm/Makefile      |   2 +
 sound/soc/bcm/rpi-dac.c     | 118 ++++++++++++++++++++++++++++++++++++++++++++
 sound/soc/codecs/Kconfig    |   9 ++++
 sound/soc/codecs/Makefile   |   2 +
 sound/soc/codecs/pcm1794a.c |  69 ++++++++++++++++++++++++++
 6 files changed, 207 insertions(+)
 create mode 100644 sound/soc/bcm/rpi-dac.c
 create mode 100644 sound/soc/codecs/pcm1794a.c

--- a/sound/soc/bcm/Kconfig
+++ b/sound/soc/bcm/Kconfig
@@ -14,3 +14,10 @@ config SND_BCM2708_SOC_HIFIBERRY_DAC
         select SND_SOC_PCM5102A
         help
          Say Y or M if you want to add support for HifiBerry DAC.
+
+config SND_BCM2708_SOC_RPI_DAC
+        tristate "Support for RPi-DAC"
+        depends on SND_BCM2708_SOC_I2S || SND_BCM2835_SOC_I2S
+        select SND_SOC_PCM1794A
+        help
+         Say Y or M if you want to add support for RPi-DAC.
--- a/sound/soc/bcm/Makefile
+++ b/sound/soc/bcm/Makefile
@@ -5,5 +5,7 @@ obj-$(CONFIG_SND_BCM2835_SOC_I2S) += snd
 
 # BCM2708 Machine Support
 snd-soc-hifiberry-dac-objs := hifiberry_dac.o
+snd-soc-rpi-dac-objs := rpi-dac.o
 
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC) += snd-soc-hifiberry-dac.o
+obj-$(CONFIG_SND_BCM2708_SOC_RPI_DAC) += snd-soc-rpi-dac.o
--- /dev/null
+++ b/sound/soc/bcm/rpi-dac.c
@@ -0,0 +1,118 @@
+/*
+ * ASoC Driver for RPi-DAC.
+ *
+ * Author:	Florian Meier <florian.meier@koalo.de>
+ *		Copyright 2013
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ */
+
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <sound/core.h>
+#include <sound/pcm.h>
+#include <sound/pcm_params.h>
+#include <sound/soc.h>
+#include <sound/jack.h>
+
+static int snd_rpi_rpi_dac_init(struct snd_soc_pcm_runtime *rtd)
+{
+	return 0;
+}
+
+static int snd_rpi_rpi_dac_hw_params(struct snd_pcm_substream *substream,
+				       struct snd_pcm_hw_params *params)
+{
+	struct snd_soc_pcm_runtime *rtd = substream->private_data;
+	struct snd_soc_dai *cpu_dai = rtd->cpu_dai;
+
+	return snd_soc_dai_set_bclk_ratio(cpu_dai, 32*2);
+}
+
+/* machine stream operations */
+static struct snd_soc_ops snd_rpi_rpi_dac_ops = {
+	.hw_params = snd_rpi_rpi_dac_hw_params,
+};
+
+static struct snd_soc_dai_link snd_rpi_rpi_dac_dai[] = {
+{
+	.name		= "RPi-DAC",
+	.stream_name	= "RPi-DAC HiFi",
+	.cpu_dai_name	= "bcm2708-i2s.0",
+	.codec_dai_name	= "pcm1794a-hifi",
+	.platform_name	= "bcm2708-i2s.0",
+	.codec_name	= "pcm1794a-codec",
+	.dai_fmt	= SND_SOC_DAIFMT_I2S | SND_SOC_DAIFMT_NB_NF |
+				SND_SOC_DAIFMT_CBS_CFS,
+	.ops		= &snd_rpi_rpi_dac_ops,
+	.init		= snd_rpi_rpi_dac_init,
+},
+};
+
+/* audio machine driver */
+static struct snd_soc_card snd_rpi_rpi_dac = {
+	.name         = "snd_rpi_rpi_dac",
+	.dai_link     = snd_rpi_rpi_dac_dai,
+	.num_links    = ARRAY_SIZE(snd_rpi_rpi_dac_dai),
+};
+
+static int snd_rpi_rpi_dac_probe(struct platform_device *pdev)
+{
+	int ret = 0;
+
+	snd_rpi_rpi_dac.dev = &pdev->dev;
+	
+	if (pdev->dev.of_node) {
+		struct device_node *i2s_node;
+		struct snd_soc_dai_link *dai = &snd_rpi_rpi_dac_dai[0];
+		i2s_node = of_parse_phandle(pdev->dev.of_node, "i2s-controller", 0);
+
+		if (i2s_node) {
+			dai->cpu_dai_name = NULL;
+			dai->cpu_of_node = i2s_node;
+			dai->platform_name = NULL;
+			dai->platform_of_node = i2s_node;
+		}
+	}
+	
+	ret = snd_soc_register_card(&snd_rpi_rpi_dac);
+	if (ret)
+		dev_err(&pdev->dev, "snd_soc_register_card() failed: %d\n", ret);
+
+	return ret;
+}
+
+static int snd_rpi_rpi_dac_remove(struct platform_device *pdev)
+{
+	return snd_soc_unregister_card(&snd_rpi_rpi_dac);
+}
+
+static const struct of_device_id snd_rpi_rpi_dac_of_match[] = {
+	{ .compatible = "rpi,rpi-dac", },
+	{},
+};
+MODULE_DEVICE_TABLE(of, snd_rpi_rpi_dac_of_match);
+
+static struct platform_driver snd_rpi_rpi_dac_driver = {
+        .driver = {
+                .name   = "snd-rpi-dac",
+                .owner  = THIS_MODULE,
+                .of_match_table = snd_rpi_rpi_dac_of_match,
+        },
+        .probe          = snd_rpi_rpi_dac_probe,
+        .remove         = snd_rpi_rpi_dac_remove,
+};
+
+module_platform_driver(snd_rpi_rpi_dac_driver);
+
+MODULE_AUTHOR("Florian Meier <florian.meier@koalo.de>");
+MODULE_DESCRIPTION("ASoC Driver for RPi-DAC");
+MODULE_LICENSE("GPL v2");
--- a/sound/soc/codecs/Kconfig
+++ b/sound/soc/codecs/Kconfig
@@ -90,6 +90,7 @@ config SND_SOC_ALL_CODECS
 	select SND_SOC_RT286 if I2C
 	select SND_SOC_RT298 if I2C
 	select SND_SOC_PCM5102A if I2C
+	select SND_SOC_PCM1794A if I2C
 	select SND_SOC_RT5631 if I2C
 	select SND_SOC_RT5640 if I2C
 	select SND_SOC_RT5645 if I2C
@@ -550,6 +551,14 @@ config SND_SOC_RT298
 	tristate
 	depends on I2C
 
+config SND_SOC_RT298
+	tristate
+	depends on I2C
+
+config SND_SOC_PCM1794A
+	tristate
+	depends on I2C
+
 config SND_SOC_PCM5102A
 	tristate
 	depends on I2C
--- a/sound/soc/codecs/Makefile
+++ b/sound/soc/codecs/Makefile
@@ -85,6 +85,7 @@ snd-soc-rl6231-objs := rl6231.o
 snd-soc-rl6347a-objs := rl6347a.o
 snd-soc-rt286-objs := rt286.o
 snd-soc-rt298-objs := rt298.o
+snd-soc-pcm1794a-objs := pcm1794a.o
 snd-soc-pcm5102a-objs := pcm5102a.o
 snd-soc-rt5631-objs := rt5631.o
 snd-soc-rt5640-objs := rt5640.o
@@ -281,6 +282,7 @@ obj-$(CONFIG_SND_SOC_RL6231)	+= snd-soc-
 obj-$(CONFIG_SND_SOC_RL6347A)	+= snd-soc-rl6347a.o
 obj-$(CONFIG_SND_SOC_RT286)	+= snd-soc-rt286.o
 obj-$(CONFIG_SND_SOC_RT298)	+= snd-soc-rt298.o
+obj-$(CONFIG_SND_SOC_PCM1794A)	+= snd-soc-pcm1794a.o
 obj-$(CONFIG_SND_SOC_PCM5102A)	+= snd-soc-pcm5102a.o
 obj-$(CONFIG_SND_SOC_RT5631)	+= snd-soc-rt5631.o
 obj-$(CONFIG_SND_SOC_RT5640)	+= snd-soc-rt5640.o
--- /dev/null
+++ b/sound/soc/codecs/pcm1794a.c
@@ -0,0 +1,69 @@
+/*
+ * Driver for the PCM1794A codec
+ *
+ * Author:	Florian Meier <florian.meier@koalo.de>
+ *		Copyright 2013
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ */
+
+
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <sound/soc.h>
+
+static struct snd_soc_dai_driver pcm1794a_dai = {
+	.name = "pcm1794a-hifi",
+	.playback = {
+		.channels_min = 2,
+		.channels_max = 2,
+		.rates = SNDRV_PCM_RATE_8000_192000,
+		.formats = SNDRV_PCM_FMTBIT_S16_LE |
+			   SNDRV_PCM_FMTBIT_S24_LE
+	},
+};
+
+static struct snd_soc_codec_driver soc_codec_dev_pcm1794a;
+
+static int pcm1794a_probe(struct platform_device *pdev)
+{
+	return snd_soc_register_codec(&pdev->dev, &soc_codec_dev_pcm1794a,
+			&pcm1794a_dai, 1);
+}
+
+static int pcm1794a_remove(struct platform_device *pdev)
+{
+	snd_soc_unregister_codec(&pdev->dev);
+	return 0;
+}
+
+static const struct of_device_id pcm1794a_of_match[] = {
+	{ .compatible = "ti,pcm1794a", },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, pcm1794a_of_match);
+
+static struct platform_driver pcm1794a_codec_driver = {
+	.probe 		= pcm1794a_probe,
+	.remove 	= pcm1794a_remove,
+	.driver		= {
+		.name	= "pcm1794a-codec",
+		.owner	= THIS_MODULE,
+		.of_match_table = of_match_ptr(pcm1794a_of_match),
+	},
+};
+
+module_platform_driver(pcm1794a_codec_driver);
+
+MODULE_DESCRIPTION("ASoC PCM1794A codec driver");
+MODULE_AUTHOR("Florian Meier <florian.meier@koalo.de>");
+MODULE_LICENSE("GPL v2");
