--- a/arch/arm/mach-cns3xxx/laguna.c
+++ b/arch/arm/mach-cns3xxx/laguna.c
@@ -21,6 +21,7 @@
 #include <linux/kernel.h>
 #include <linux/compiler.h>
 #include <linux/io.h>
+#include <linux/irq.h>
 #include <linux/gpio.h>
 #include <linux/dma-mapping.h>
 #include <linux/serial_core.h>
@@ -872,6 +873,47 @@ static int laguna_register_gpio(struct g
 	return ret;
 }
 
+/* allow disabling of external isolated PCIe IRQs */
+static int cns3xxx_pciextirq = 1;
+static int __init cns3xxx_pciextirq_disable(char *s)
+{
+      cns3xxx_pciextirq = 0;
+      return 1;
+}
+__setup("noextirq", cns3xxx_pciextirq_disable);
+
+static int __init laguna_pcie_init_irq(void)
+{
+	u32 __iomem *mem = (void __iomem *)(CNS3XXX_GPIOB_BASE_VIRT + 0x0004);
+	u32 reg = (__raw_readl(mem) >> 26) & 0xf;
+	int irqs[] = {
+		IRQ_CNS3XXX_EXTERNAL_PIN0,
+		IRQ_CNS3XXX_EXTERNAL_PIN1,
+		IRQ_CNS3XXX_EXTERNAL_PIN2,
+		154,
+	};
+
+	if (!machine_is_gw2388())
+		return 0;
+
+	/* Verify GPIOB[26:29] == 0001b indicating support for ext irqs */
+	if (cns3xxx_pciextirq && reg != 1)
+		cns3xxx_pciextirq = 0;
+
+	if (cns3xxx_pciextirq) {
+		printk("laguna: using isolated PCI interrupts:"
+		       " irq%d/irq%d/irq%d/irq%d\n",
+		       irqs[0], irqs[1], irqs[2], irqs[3]);
+		cns3xxx_pcie_set_irqs(0, irqs);
+	} else {
+		printk("laguna: using shared PCI interrupts: irq%d\n",
+		       IRQ_CNS3XXX_PCIE0_DEVICE);
+	}
+
+	return 0;
+}
+subsys_initcall(laguna_pcie_init_irq);
+
 static int __init laguna_model_setup(void)
 {
 	u32 __iomem *mem;
@@ -883,8 +925,33 @@ static int __init laguna_model_setup(voi
 	printk("Running on Gateworks Laguna %s\n", laguna_info.model);
 	cns3xxx_gpio_init( 0, 32, CNS3XXX_GPIOA_BASE_VIRT, IRQ_CNS3XXX_GPIOA,
 		NR_IRQS_CNS3XXX);
-	cns3xxx_gpio_init(32, 32, CNS3XXX_GPIOB_BASE_VIRT, IRQ_CNS3XXX_GPIOB,
-		NR_IRQS_CNS3XXX + 32);
+
+	/*
+	 * If pcie external interrupts are supported and desired
+	 * configure IRQ types and configure pin function.
+	 * Note that cns3xxx_pciextirq is enabled by default, but can be
+	 * unset via the 'noextirq' kernel param or by laguna_pcie_init() if
+	 * the baseboard model does not support this hardware feature.
+	 */
+	if (cns3xxx_pciextirq) {
+		mem = (void __iomem *)(CNS3XXX_MISC_BASE_VIRT + 0x0018);
+		reg = __raw_readl(mem);
+		/* GPIO26 is gpio, EXT_INT[0:2] not gpio func */
+		reg &= ~0x3c000000;
+		reg |= 0x38000000;
+		__raw_writel(reg, mem);
+
+		cns3xxx_gpio_init(32, 32, CNS3XXX_GPIOB_BASE_VIRT,
+				  IRQ_CNS3XXX_GPIOB, NR_IRQS_CNS3XXX + 32);
+
+		irq_set_irq_type(154, IRQ_TYPE_LEVEL_LOW);
+		irq_set_irq_type(93, IRQ_TYPE_LEVEL_HIGH);
+		irq_set_irq_type(94, IRQ_TYPE_LEVEL_HIGH);
+		irq_set_irq_type(95, IRQ_TYPE_LEVEL_HIGH);
+	} else {
+		cns3xxx_gpio_init(32, 32, CNS3XXX_GPIOB_BASE_VIRT,
+				  IRQ_CNS3XXX_GPIOB, NR_IRQS_CNS3XXX + 32);
+	}
 
 	if (strncmp(laguna_info.model, "GW", 2) == 0) {
 		if (laguna_info.config_bitmap & ETH0_LOAD)
--- a/arch/arm/mach-cns3xxx/pcie.c
+++ b/arch/arm/mach-cns3xxx/pcie.c
@@ -18,6 +18,7 @@
 #include <linux/io.h>
 #include <linux/ioport.h>
 #include <linux/interrupt.h>
+#include <linux/irq.h>
 #include <linux/ptrace.h>
 #include <asm/mach/map.h>
 #include "cns3xxx.h"
@@ -27,7 +28,7 @@ struct cns3xxx_pcie {
 	void __iomem *host_regs; /* PCI config registers for host bridge */
 	void __iomem *cfg0_regs; /* PCI Type 0 config registers */
 	void __iomem *cfg1_regs; /* PCI Type 1 config registers */
-	unsigned int irqs[2];
+	unsigned int irqs[5];
 	struct resource res_io;
 	struct resource res_mem;
 	int port;
@@ -95,7 +96,7 @@ static inline int check_master_abort(str
 		void __iomem *host_base;
 		u32 sreg, ereg;
 
-		host_base = (void __iomem *) cnspci->cfg_bases[CNS3XXX_HOST_TYPE].virtual;
+		host_base = (void __iomem *) cnspci->host_regs;
 		sreg = __raw_readw(host_base + 0x6) & 0xF900;
 		ereg = __raw_readl(host_base + 0x104); // Uncorrectable Error Status Reg
 
@@ -209,7 +210,7 @@ static struct pci_ops cns3xxx_pcie_ops =
 static int cns3xxx_pcie_map_irq(const struct pci_dev *dev, u8 slot, u8 pin)
 {
 	struct cns3xxx_pcie *cnspci = pdev_to_cnspci(dev);
-	int irq = cnspci->irqs[!!dev->bus->number];
+	int irq = cnspci->irqs[!!dev->bus->number + pin - 1];
 
 	pr_info("PCIe map irq: %04d:%02x:%02x.%02x slot %d, pin %d, irq: %d\n",
 		pci_domain_nr(dev->bus), dev->bus->number, PCI_SLOT(dev->devfn),
@@ -235,7 +236,13 @@ static struct cns3xxx_pcie cns3xxx_pcie[
 			.end = CNS3XXX_PCIE0_HOST_BASE - 1, /* 176 MiB */
 			.flags = IORESOURCE_MEM,
 		},
-		.irqs = { IRQ_CNS3XXX_PCIE0_RC, IRQ_CNS3XXX_PCIE0_DEVICE, },
+		.irqs = {
+			IRQ_CNS3XXX_PCIE0_RC,
+			IRQ_CNS3XXX_PCIE0_DEVICE,
+			IRQ_CNS3XXX_PCIE0_DEVICE,
+			IRQ_CNS3XXX_PCIE0_DEVICE,
+			IRQ_CNS3XXX_PCIE0_DEVICE,
+		},
 		.port = 0,
 	},
 	[1] = {
@@ -254,7 +261,13 @@ static struct cns3xxx_pcie cns3xxx_pcie[
 			.end = CNS3XXX_PCIE1_HOST_BASE - 1, /* 176 MiB */
 			.flags = IORESOURCE_MEM,
 		},
-		.irqs = { IRQ_CNS3XXX_PCIE1_RC, IRQ_CNS3XXX_PCIE1_DEVICE, },
+		.irqs = {
+			IRQ_CNS3XXX_PCIE1_RC,
+			IRQ_CNS3XXX_PCIE1_DEVICE,
+			IRQ_CNS3XXX_PCIE1_DEVICE,
+			IRQ_CNS3XXX_PCIE1_DEVICE,
+			IRQ_CNS3XXX_PCIE1_DEVICE,
+		},
 		.port = 1,
 	},
 };
@@ -346,6 +359,14 @@ static int cns3xxx_pcie_abort_handler(un
 	return 0;
 }
 
+void __init cns3xxx_pcie_set_irqs(int bus, int *irqs)
+{
+	int i;
+
+	for (i = 0; i < 4; i++)
+		cns3xxx_pcie[bus].irqs[i + 1] = irqs[i];
+}
+
 void __init cns3xxx_pcie_init_late(void)
 {
 	int i;
--- a/arch/arm/mach-cns3xxx/core.h
+++ b/arch/arm/mach-cns3xxx/core.h
@@ -18,8 +18,10 @@ extern void cns3xxx_timer_init(void);
 
 #ifdef CONFIG_PCI
 extern void __init cns3xxx_pcie_init_late(void);
+extern void __init cns3xxx_pcie_set_irqs(int bus, int *irqs);
 #else
 static inline void __init cns3xxx_pcie_init_late(void) {}
+static inline void cns3xxx_pcie_set_irqs(int bus, int *irqs) {}
 #endif
 
 void __init cns3xxx_map_io(void);
