From 775d5392d5ba612dc856f05fef318b3fd0687f81 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Tue, 26 Mar 2013 17:26:38 +0000
Subject: [PATCH 058/381] Allow mac address to be set in smsc95xx

Signed-off-by: popcornmix <popcornmix@gmail.com>
---
 drivers/net/usb/smsc95xx.c | 56 ++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 56 insertions(+)

--- a/drivers/net/usb/smsc95xx.c
+++ b/drivers/net/usb/smsc95xx.c
@@ -59,6 +59,7 @@
 #define SUSPEND_SUSPEND3		(0x08)
 #define SUSPEND_ALLMODES		(SUSPEND_SUSPEND0 | SUSPEND_SUSPEND1 | \
 					 SUSPEND_SUSPEND2 | SUSPEND_SUSPEND3)
+#define MAC_ADDR_LEN                    (6)
 
 struct smsc95xx_priv {
 	u32 mac_cr;
@@ -74,6 +75,10 @@ static bool turbo_mode = false;
 module_param(turbo_mode, bool, 0644);
 MODULE_PARM_DESC(turbo_mode, "Enable multiple frames per Rx transaction");
 
+static char *macaddr = ":";
+module_param(macaddr, charp, 0);
+MODULE_PARM_DESC(macaddr, "MAC address");
+
 static int __must_check __smsc95xx_read_reg(struct usbnet *dev, u32 index,
 					    u32 *data, int in_pm)
 {
@@ -763,8 +768,59 @@ static int smsc95xx_ioctl(struct net_dev
 	return generic_mii_ioctl(&dev->mii, if_mii(rq), cmd, NULL);
 }
 
+/* Check the macaddr module parameter for a MAC address */
+static int smsc95xx_is_macaddr_param(struct usbnet *dev, u8 *dev_mac)
+{
+       int i, j, got_num, num;
+       u8 mtbl[MAC_ADDR_LEN];
+
+       if (macaddr[0] == ':')
+               return 0;
+
+       i = 0;
+       j = 0;
+       num = 0;
+       got_num = 0;
+       while (j < MAC_ADDR_LEN) {
+               if (macaddr[i] && macaddr[i] != ':') {
+                       got_num++;
+                       if ('0' <= macaddr[i] && macaddr[i] <= '9')
+                               num = num * 16 + macaddr[i] - '0';
+                       else if ('A' <= macaddr[i] && macaddr[i] <= 'F')
+                               num = num * 16 + 10 + macaddr[i] - 'A';
+                       else if ('a' <= macaddr[i] && macaddr[i] <= 'f')
+                               num = num * 16 + 10 + macaddr[i] - 'a';
+                       else
+                               break;
+                       i++;
+               } else if (got_num == 2) {
+                       mtbl[j++] = (u8) num;
+                       num = 0;
+                       got_num = 0;
+                       i++;
+               } else {
+                       break;
+               }
+       }
+
+       if (j == MAC_ADDR_LEN) {
+               netif_dbg(dev, ifup, dev->net, "Overriding MAC address with: "
+               "%02x:%02x:%02x:%02x:%02x:%02x\n", mtbl[0], mtbl[1], mtbl[2],
+                                               mtbl[3], mtbl[4], mtbl[5]);
+               for (i = 0; i < MAC_ADDR_LEN; i++)
+                       dev_mac[i] = mtbl[i];
+               return 1;
+       } else {
+               return 0;
+       }
+}
+
 static void smsc95xx_init_mac_address(struct usbnet *dev)
 {
+       /* Check module parameters */
+       if (smsc95xx_is_macaddr_param(dev, dev->net->dev_addr))
+               return;
+
 	/* try reading mac address from EEPROM */
 	if (smsc95xx_read_eeprom(dev, EEPROM_MAC_OFFSET, ETH_ALEN,
 			dev->net->dev_addr) == 0) {
