From 1fc5799ca5f6f2cc31f5b076d780e111de011cc3 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 15 Apr 2016 10:48:39 +0100
Subject: [PATCH 244/381] boomberry-dac: Adjust for ALSA API change

As of 4.4, snd_soc_limit_volume now takes a struct snd_soc_card *
rather than a struct snd_soc_codec *.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 sound/soc/bcm/boomberry-dac.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/sound/soc/bcm/boomberry-dac.c
+++ b/sound/soc/bcm/boomberry-dac.c
@@ -40,9 +40,8 @@ static int snd_rpi_boomberry_dac_init(st
 	{
 		int ret;
 		struct snd_soc_card *card = rtd->card;
-		struct snd_soc_codec *codec = rtd->codec;
 
-		ret = snd_soc_limit_volume(codec, "Digital Playback Volume", 207);
+		ret = snd_soc_limit_volume(card, "Digital Playback Volume", 207);
 		if (ret < 0)
 			dev_warn(card->dev, "Failed to set volume limit: %d\n", ret);
 	}
