--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -508,4 +508,12 @@ config LEDS_VERSATILE
 comment "LED Triggers"
 source "drivers/leds/trigger/Kconfig"
 
+config LEDS_TRIGGER_ADM5120_SWITCH
+	tristate "LED ADM5120 Switch Port Status Trigger"
+	depends on LEDS_TRIGGERS && ADM5120
+	help
+	  This allows LEDs to be controlled by the port states of
+	  the ADM5120 built-in Ethernet Switch
+	  If unsure, say N.
+
 endif # NEW_LEDS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -65,3 +65,4 @@ obj-$(CONFIG_LEDS_TRIGGERS)		+= trigger/
 obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
 obj-$(CONFIG_LEDS_TRIGGER_NETDEV)	+= ledtrig-netdev.o
 obj-$(CONFIG_LEDS_TRIGGER_USBDEV)	+= ledtrig-usbdev.o
+obj-$(CONFIG_LEDS_TRIGGER_ADM5120_SWITCH) += ledtrig-adm5120-switch.o
