From 34db3e8f383a79ea01a1fee31270e779956ec939 Mon Sep 17 00:00:00 2001
From: Martin Sperl <kernel@martin.sperl.org>
Date: Mon, 29 Feb 2016 12:51:42 +0000
Subject: [PATCH 262/381] clk: bcm2835: reorganize bcm2835_clock_array
 assignment

Reorganize bcm2835_clock_array so that there is no more
need for separate bcm2835_*_data structures to be defined.
Instead the required structures are generated inline via
helper macros.

To allow this to also work for pll alone it was required that
the parent_pll was changed from a pointer to bcm2835_pll_data
to the name of the pll instead.

Signed-off-by: Martin Sperl <kernel@martin.sperl.org>
Signed-off-by: Eric Anholt <eric@anholt.net>
Reviewed-by: Eric Anholt <eric@anholt.net>
(cherry picked from commit 3b15afefbef9b5952e3d68ad73d93f981b9faca8)
---
 drivers/clk/bcm/clk-bcm2835.c | 852 +++++++++++++++++++-----------------------
 1 file changed, 393 insertions(+), 459 deletions(-)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -418,115 +418,10 @@ static const struct bcm2835_pll_ana_bits
 	.fb_prediv_mask = BIT(11),
 };
 
-/*
- * PLLA is the auxiliary PLL, used to drive the CCP2 (Compact Camera
- * Port 2) transmitter clock.
- *
- * It is in the PX LDO power domain, which is on when the AUDIO domain
- * is on.
- */
-static const struct bcm2835_pll_data bcm2835_plla_data = {
-	.name = "plla",
-	.cm_ctrl_reg = CM_PLLA,
-	.a2w_ctrl_reg = A2W_PLLA_CTRL,
-	.frac_reg = A2W_PLLA_FRAC,
-	.ana_reg_base = A2W_PLLA_ANA0,
-	.reference_enable_mask = A2W_XOSC_CTRL_PLLA_ENABLE,
-	.lock_mask = CM_LOCK_FLOCKA,
-
-	.ana = &bcm2835_ana_default,
-
-	.min_rate = 600000000u,
-	.max_rate = 2400000000u,
-	.max_fb_rate = BCM2835_MAX_FB_RATE,
-};
-
-/* PLLB is used for the ARM's clock. */
-static const struct bcm2835_pll_data bcm2835_pllb_data = {
-	.name = "pllb",
-	.cm_ctrl_reg = CM_PLLB,
-	.a2w_ctrl_reg = A2W_PLLB_CTRL,
-	.frac_reg = A2W_PLLB_FRAC,
-	.ana_reg_base = A2W_PLLB_ANA0,
-	.reference_enable_mask = A2W_XOSC_CTRL_PLLB_ENABLE,
-	.lock_mask = CM_LOCK_FLOCKB,
-
-	.ana = &bcm2835_ana_default,
-
-	.min_rate = 600000000u,
-	.max_rate = 3000000000u,
-	.max_fb_rate = BCM2835_MAX_FB_RATE,
-};
-
-/*
- * PLLC is the core PLL, used to drive the core VPU clock.
- *
- * It is in the PX LDO power domain, which is on when the AUDIO domain
- * is on.
-*/
-static const struct bcm2835_pll_data bcm2835_pllc_data = {
-	.name = "pllc",
-	.cm_ctrl_reg = CM_PLLC,
-	.a2w_ctrl_reg = A2W_PLLC_CTRL,
-	.frac_reg = A2W_PLLC_FRAC,
-	.ana_reg_base = A2W_PLLC_ANA0,
-	.reference_enable_mask = A2W_XOSC_CTRL_PLLC_ENABLE,
-	.lock_mask = CM_LOCK_FLOCKC,
-
-	.ana = &bcm2835_ana_default,
-
-	.min_rate = 600000000u,
-	.max_rate = 3000000000u,
-	.max_fb_rate = BCM2835_MAX_FB_RATE,
-};
-
-/*
- * PLLD is the display PLL, used to drive DSI display panels.
- *
- * It is in the PX LDO power domain, which is on when the AUDIO domain
- * is on.
- */
-static const struct bcm2835_pll_data bcm2835_plld_data = {
-	.name = "plld",
-	.cm_ctrl_reg = CM_PLLD,
-	.a2w_ctrl_reg = A2W_PLLD_CTRL,
-	.frac_reg = A2W_PLLD_FRAC,
-	.ana_reg_base = A2W_PLLD_ANA0,
-	.reference_enable_mask = A2W_XOSC_CTRL_DDR_ENABLE,
-	.lock_mask = CM_LOCK_FLOCKD,
-
-	.ana = &bcm2835_ana_default,
-
-	.min_rate = 600000000u,
-	.max_rate = 2400000000u,
-	.max_fb_rate = BCM2835_MAX_FB_RATE,
-};
-
-/*
- * PLLH is used to supply the pixel clock or the AUX clock for the TV
- * encoder.
- *
- * It is in the HDMI power domain.
- */
-static const struct bcm2835_pll_data bcm2835_pllh_data = {
-	"pllh",
-	.cm_ctrl_reg = CM_PLLH,
-	.a2w_ctrl_reg = A2W_PLLH_CTRL,
-	.frac_reg = A2W_PLLH_FRAC,
-	.ana_reg_base = A2W_PLLH_ANA0,
-	.reference_enable_mask = A2W_XOSC_CTRL_PLLC_ENABLE,
-	.lock_mask = CM_LOCK_FLOCKH,
-
-	.ana = &bcm2835_ana_pllh,
-
-	.min_rate = 600000000u,
-	.max_rate = 3000000000u,
-	.max_fb_rate = BCM2835_MAX_FB_RATE,
-};
-
 struct bcm2835_pll_divider_data {
 	const char *name;
-	const struct bcm2835_pll_data *source_pll;
+	const char *source_pll;
+
 	u32 cm_reg;
 	u32 a2w_reg;
 
@@ -535,124 +430,6 @@ struct bcm2835_pll_divider_data {
 	u32 fixed_divider;
 };
 
-static const struct bcm2835_pll_divider_data bcm2835_plla_core_data = {
-	.name = "plla_core",
-	.source_pll = &bcm2835_plla_data,
-	.cm_reg = CM_PLLA,
-	.a2w_reg = A2W_PLLA_CORE,
-	.load_mask = CM_PLLA_LOADCORE,
-	.hold_mask = CM_PLLA_HOLDCORE,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_plla_per_data = {
-	.name = "plla_per",
-	.source_pll = &bcm2835_plla_data,
-	.cm_reg = CM_PLLA,
-	.a2w_reg = A2W_PLLA_PER,
-	.load_mask = CM_PLLA_LOADPER,
-	.hold_mask = CM_PLLA_HOLDPER,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllb_arm_data = {
-	.name = "pllb_arm",
-	.source_pll = &bcm2835_pllb_data,
-	.cm_reg = CM_PLLB,
-	.a2w_reg = A2W_PLLB_ARM,
-	.load_mask = CM_PLLB_LOADARM,
-	.hold_mask = CM_PLLB_HOLDARM,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllc_core0_data = {
-	.name = "pllc_core0",
-	.source_pll = &bcm2835_pllc_data,
-	.cm_reg = CM_PLLC,
-	.a2w_reg = A2W_PLLC_CORE0,
-	.load_mask = CM_PLLC_LOADCORE0,
-	.hold_mask = CM_PLLC_HOLDCORE0,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllc_core1_data = {
-	.name = "pllc_core1", .source_pll = &bcm2835_pllc_data,
-	.cm_reg = CM_PLLC, A2W_PLLC_CORE1,
-	.load_mask = CM_PLLC_LOADCORE1,
-	.hold_mask = CM_PLLC_HOLDCORE1,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllc_core2_data = {
-	.name = "pllc_core2",
-	.source_pll = &bcm2835_pllc_data,
-	.cm_reg = CM_PLLC,
-	.a2w_reg = A2W_PLLC_CORE2,
-	.load_mask = CM_PLLC_LOADCORE2,
-	.hold_mask = CM_PLLC_HOLDCORE2,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllc_per_data = {
-	.name = "pllc_per",
-	.source_pll = &bcm2835_pllc_data,
-	.cm_reg = CM_PLLC,
-	.a2w_reg = A2W_PLLC_PER,
-	.load_mask = CM_PLLC_LOADPER,
-	.hold_mask = CM_PLLC_HOLDPER,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_plld_core_data = {
-	.name = "plld_core",
-	.source_pll = &bcm2835_plld_data,
-	.cm_reg = CM_PLLD,
-	.a2w_reg = A2W_PLLD_CORE,
-	.load_mask = CM_PLLD_LOADCORE,
-	.hold_mask = CM_PLLD_HOLDCORE,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_plld_per_data = {
-	.name = "plld_per",
-	.source_pll = &bcm2835_plld_data,
-	.cm_reg = CM_PLLD,
-	.a2w_reg = A2W_PLLD_PER,
-	.load_mask = CM_PLLD_LOADPER,
-	.hold_mask = CM_PLLD_HOLDPER,
-	.fixed_divider = 1,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllh_rcal_data = {
-	.name = "pllh_rcal",
-	.source_pll = &bcm2835_pllh_data,
-	.cm_reg = CM_PLLH,
-	.a2w_reg = A2W_PLLH_RCAL,
-	.load_mask = CM_PLLH_LOADRCAL,
-	.hold_mask = 0,
-	.fixed_divider = 10,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllh_aux_data = {
-	.name = "pllh_aux",
-	.source_pll = &bcm2835_pllh_data,
-	.cm_reg = CM_PLLH,
-	.a2w_reg = A2W_PLLH_AUX,
-	.load_mask = CM_PLLH_LOADAUX,
-	.hold_mask = 0,
-	.fixed_divider = 10,
-};
-
-static const struct bcm2835_pll_divider_data bcm2835_pllh_pix_data = {
-	.name = "pllh_pix",
-	.source_pll = &bcm2835_pllh_data,
-	.cm_reg = CM_PLLH,
-	.a2w_reg = A2W_PLLH_PIX,
-	.load_mask = CM_PLLH_LOADPIX,
-	.hold_mask = 0,
-	.fixed_divider = 10,
-};
-
 struct bcm2835_clock_data {
 	const char *name;
 
@@ -671,188 +448,6 @@ struct bcm2835_clock_data {
 	bool is_mash_clock;
 };
 
-static const char *const bcm2835_clock_per_parents[] = {
-	"gnd",
-	"xosc",
-	"testdebug0",
-	"testdebug1",
-	"plla_per",
-	"pllc_per",
-	"plld_per",
-	"pllh_aux",
-};
-
-static const char *const bcm2835_clock_vpu_parents[] = {
-	"gnd",
-	"xosc",
-	"testdebug0",
-	"testdebug1",
-	"plla_core",
-	"pllc_core0",
-	"plld_core",
-	"pllh_aux",
-	"pllc_core1",
-	"pllc_core2",
-};
-
-static const char *const bcm2835_clock_osc_parents[] = {
-	"gnd",
-	"xosc",
-	"testdebug0",
-	"testdebug1"
-};
-
-/*
- * Used for a 1Mhz clock for the system clocksource, and also used by
- * the watchdog timer and the camera pulse generator.
- */
-static const struct bcm2835_clock_data bcm2835_clock_timer_data = {
-	.name = "timer",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_osc_parents),
-	.parents = bcm2835_clock_osc_parents,
-	.ctl_reg = CM_TIMERCTL,
-	.div_reg = CM_TIMERDIV,
-	.int_bits = 6,
-	.frac_bits = 12,
-};
-
-/* One Time Programmable Memory clock.  Maximum 10Mhz. */
-static const struct bcm2835_clock_data bcm2835_clock_otp_data = {
-	.name = "otp",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_osc_parents),
-	.parents = bcm2835_clock_osc_parents,
-	.ctl_reg = CM_OTPCTL,
-	.div_reg = CM_OTPDIV,
-	.int_bits = 4,
-	.frac_bits = 0,
-};
-
-/*
- * VPU clock.  This doesn't have an enable bit, since it drives the
- * bus for everything else, and is special so it doesn't need to be
- * gated for rate changes.  It is also known as "clk_audio" in various
- * hardware documentation.
- */
-static const struct bcm2835_clock_data bcm2835_clock_vpu_data = {
-	.name = "vpu",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_vpu_parents),
-	.parents = bcm2835_clock_vpu_parents,
-	.ctl_reg = CM_VPUCTL,
-	.div_reg = CM_VPUDIV,
-	.int_bits = 12,
-	.frac_bits = 8,
-	.is_vpu_clock = true,
-};
-
-static const struct bcm2835_clock_data bcm2835_clock_v3d_data = {
-	.name = "v3d",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_vpu_parents),
-	.parents = bcm2835_clock_vpu_parents,
-	.ctl_reg = CM_V3DCTL,
-	.div_reg = CM_V3DDIV,
-	.int_bits = 4,
-	.frac_bits = 8,
-};
-
-static const struct bcm2835_clock_data bcm2835_clock_isp_data = {
-	.name = "isp",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_vpu_parents),
-	.parents = bcm2835_clock_vpu_parents,
-	.ctl_reg = CM_ISPCTL,
-	.div_reg = CM_ISPDIV,
-	.int_bits = 4,
-	.frac_bits = 8,
-};
-
-static const struct bcm2835_clock_data bcm2835_clock_h264_data = {
-	.name = "h264",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_vpu_parents),
-	.parents = bcm2835_clock_vpu_parents,
-	.ctl_reg = CM_H264CTL,
-	.div_reg = CM_H264DIV,
-	.int_bits = 4,
-	.frac_bits = 8,
-};
-
-/* TV encoder clock.  Only operating frequency is 108Mhz.  */
-static const struct bcm2835_clock_data bcm2835_clock_vec_data = {
-	.name = "vec",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),
-	.parents = bcm2835_clock_per_parents,
-	.ctl_reg = CM_VECCTL,
-	.div_reg = CM_VECDIV,
-	.int_bits = 4,
-	.frac_bits = 0,
-};
-
-static const struct bcm2835_clock_data bcm2835_clock_uart_data = {
-	.name = "uart",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),
-	.parents = bcm2835_clock_per_parents,
-	.ctl_reg = CM_UARTCTL,
-	.div_reg = CM_UARTDIV,
-	.int_bits = 10,
-	.frac_bits = 12,
-};
-
-/* HDMI state machine */
-static const struct bcm2835_clock_data bcm2835_clock_hsm_data = {
-	.name = "hsm",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),
-	.parents = bcm2835_clock_per_parents,
-	.ctl_reg = CM_HSMCTL,
-	.div_reg = CM_HSMDIV,
-	.int_bits = 4,
-	.frac_bits = 8,
-};
-
-/*
- * Secondary SDRAM clock.  Used for low-voltage modes when the PLL in
- * the SDRAM controller can't be used.
- */
-static const struct bcm2835_clock_data bcm2835_clock_sdram_data = {
-	.name = "sdram",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_vpu_parents),
-	.parents = bcm2835_clock_vpu_parents,
-	.ctl_reg = CM_SDCCTL,
-	.div_reg = CM_SDCDIV,
-	.int_bits = 6,
-	.frac_bits = 0,
-};
-
-/* Clock for the temperature sensor.  Generally run at 2Mhz, max 5Mhz. */
-static const struct bcm2835_clock_data bcm2835_clock_tsens_data = {
-	.name = "tsens",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_osc_parents),
-	.parents = bcm2835_clock_osc_parents,
-	.ctl_reg = CM_TSENSCTL,
-	.div_reg = CM_TSENSDIV,
-	.int_bits = 5,
-	.frac_bits = 0,
-};
-
-/* Arasan EMMC clock */
-static const struct bcm2835_clock_data bcm2835_clock_emmc_data = {
-	.name = "emmc",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),
-	.parents = bcm2835_clock_per_parents,
-	.ctl_reg = CM_EMMCCTL,
-	.div_reg = CM_EMMCDIV,
-	.int_bits = 4,
-	.frac_bits = 8,
-};
-
-static const struct bcm2835_clock_data bcm2835_clock_pwm_data = {
-	.name = "pwm",
-	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),
-	.parents = bcm2835_clock_per_parents,
-	.ctl_reg = CM_PWMCTL,
-	.div_reg = CM_PWMDIV,
-	.int_bits = 12,
-	.frac_bits = 12,
-	.is_mash_clock = true,
-};
-
 struct bcm2835_gate_data {
 	const char *name;
 	const char *parent;
@@ -860,18 +455,6 @@ struct bcm2835_gate_data {
 	u32 ctl_reg;
 };
 
-/*
- * CM_PERIICTL (and CM_PERIACTL, CM_SYSCTL and CM_VPUCTL if
- * you have the debug bit set in the power manager, which we
- * don't bother exposing) are individual gates off of the
- * non-stop vpu clock.
- */
-static const struct bcm2835_gate_data bcm2835_clock_peri_image_data = {
-	.name = "peri_image",
-	.parent = "vpu",
-	.ctl_reg = CM_PERIICTL,
-};
-
 struct bcm2835_pll {
 	struct clk_hw hw;
 	struct bcm2835_cprman *cprman;
@@ -1594,7 +1177,7 @@ bcm2835_register_pll_divider(struct bcm2
 
 	memset(&init, 0, sizeof(init));
 
-	init.parent_names = &data->source_pll->name;
+	init.parent_names = &data->source_pll;
 	init.num_parents = 1;
 	init.name = divider_name;
 	init.ops = &bcm2835_pll_divider_clk_ops;
@@ -1693,50 +1276,401 @@ struct bcm2835_clk_desc {
 	const void *data;
 };
 
-#define _REGISTER(f, d) { .clk_register = (bcm2835_clk_register)f, \
-			  .data = d }
-#define REGISTER_PLL(d)		_REGISTER(&bcm2835_register_pll, d)
-#define REGISTER_PLL_DIV(d)	_REGISTER(&bcm2835_register_pll_divider, d)
-#define REGISTER_CLK(d)		_REGISTER(&bcm2835_register_clock, d)
-#define REGISTER_GATE(d)	_REGISTER(&bcm2835_register_gate, d)
+/* assignment helper macros for different clock types */
+#define _REGISTER(f, ...) { .clk_register = (bcm2835_clk_register)f, \
+			    .data = __VA_ARGS__ }
+#define REGISTER_PLL(...)	_REGISTER(&bcm2835_register_pll,	\
+					  &(struct bcm2835_pll_data)	\
+					  {__VA_ARGS__})
+#define REGISTER_PLL_DIV(...)	_REGISTER(&bcm2835_register_pll_divider, \
+					  &(struct bcm2835_pll_divider_data) \
+					  {__VA_ARGS__})
+#define REGISTER_CLK(...)	_REGISTER(&bcm2835_register_clock,	\
+					  &(struct bcm2835_clock_data)	\
+					  {__VA_ARGS__})
+#define REGISTER_GATE(...)	_REGISTER(&bcm2835_register_gate,	\
+					  &(struct bcm2835_gate_data)	\
+					  {__VA_ARGS__})
+
+/* parent mux arrays plus helper macros */
+
+/* main oscillator parent mux */
+static const char *const bcm2835_clock_osc_parents[] = {
+	"gnd",
+	"xosc",
+	"testdebug0",
+	"testdebug1"
+};
+
+#define REGISTER_OSC_CLK(...)	REGISTER_CLK(				\
+	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_osc_parents),	\
+	.parents = bcm2835_clock_osc_parents,				\
+	__VA_ARGS__)
+
+/* main peripherial parent mux */
+static const char *const bcm2835_clock_per_parents[] = {
+	"gnd",
+	"xosc",
+	"testdebug0",
+	"testdebug1",
+	"plla_per",
+	"pllc_per",
+	"plld_per",
+	"pllh_aux",
+};
+
+#define REGISTER_PER_CLK(...)	REGISTER_CLK(				\
+	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_per_parents),	\
+	.parents = bcm2835_clock_per_parents,				\
+	__VA_ARGS__)
+
+/* main vpu parent mux */
+static const char *const bcm2835_clock_vpu_parents[] = {
+	"gnd",
+	"xosc",
+	"testdebug0",
+	"testdebug1",
+	"plla_core",
+	"pllc_core0",
+	"plld_core",
+	"pllh_aux",
+	"pllc_core1",
+	"pllc_core2",
+};
+
+#define REGISTER_VPU_CLK(...)	REGISTER_CLK(				\
+	.num_mux_parents = ARRAY_SIZE(bcm2835_clock_vpu_parents),	\
+	.parents = bcm2835_clock_vpu_parents,				\
+	__VA_ARGS__)
 
+/*
+ * the real definition of all the pll, pll_dividers and clocks
+ * these make use of the above REGISTER_* macros
+ */
 static const struct bcm2835_clk_desc clk_desc_array[] = {
-	/* register PLL */
-	[BCM2835_PLLA]		= REGISTER_PLL(&bcm2835_plla_data),
-	[BCM2835_PLLB]		= REGISTER_PLL(&bcm2835_pllb_data),
-	[BCM2835_PLLC]		= REGISTER_PLL(&bcm2835_pllc_data),
-	[BCM2835_PLLD]		= REGISTER_PLL(&bcm2835_plld_data),
-	[BCM2835_PLLH]		= REGISTER_PLL(&bcm2835_pllh_data),
-	/* the PLL dividers */
-	[BCM2835_PLLA_CORE]	= REGISTER_PLL_DIV(&bcm2835_plla_core_data),
-	[BCM2835_PLLA_PER]	= REGISTER_PLL_DIV(&bcm2835_plla_per_data),
-	[BCM2835_PLLC_CORE0]	= REGISTER_PLL_DIV(&bcm2835_pllc_core0_data),
-	[BCM2835_PLLC_CORE1]	= REGISTER_PLL_DIV(&bcm2835_pllc_core1_data),
-	[BCM2835_PLLC_CORE2]	= REGISTER_PLL_DIV(&bcm2835_pllc_core2_data),
-	[BCM2835_PLLC_PER]	= REGISTER_PLL_DIV(&bcm2835_pllc_per_data),
-	[BCM2835_PLLD_CORE]	= REGISTER_PLL_DIV(&bcm2835_plld_core_data),
-	[BCM2835_PLLD_PER]	= REGISTER_PLL_DIV(&bcm2835_plld_per_data),
-	[BCM2835_PLLH_RCAL]	= REGISTER_PLL_DIV(&bcm2835_pllh_rcal_data),
-	[BCM2835_PLLH_AUX]	= REGISTER_PLL_DIV(&bcm2835_pllh_aux_data),
-	[BCM2835_PLLH_PIX]	= REGISTER_PLL_DIV(&bcm2835_pllh_pix_data),
+	/* the PLL + PLL dividers */
+
+	/*
+	 * PLLA is the auxiliary PLL, used to drive the CCP2
+	 * (Compact Camera Port 2) transmitter clock.
+	 *
+	 * It is in the PX LDO power domain, which is on when the
+	 * AUDIO domain is on.
+	 */
+	[BCM2835_PLLA]		= REGISTER_PLL(
+		.name = "plla",
+		.cm_ctrl_reg = CM_PLLA,
+		.a2w_ctrl_reg = A2W_PLLA_CTRL,
+		.frac_reg = A2W_PLLA_FRAC,
+		.ana_reg_base = A2W_PLLA_ANA0,
+		.reference_enable_mask = A2W_XOSC_CTRL_PLLA_ENABLE,
+		.lock_mask = CM_LOCK_FLOCKA,
+
+		.ana = &bcm2835_ana_default,
+
+		.min_rate = 600000000u,
+		.max_rate = 2400000000u,
+		.max_fb_rate = BCM2835_MAX_FB_RATE),
+	[BCM2835_PLLA_CORE]	= REGISTER_PLL_DIV(
+		.name = "plla_core",
+		.source_pll = "plla",
+		.cm_reg = CM_PLLA,
+		.a2w_reg = A2W_PLLA_CORE,
+		.load_mask = CM_PLLA_LOADCORE,
+		.hold_mask = CM_PLLA_HOLDCORE,
+		.fixed_divider = 1),
+	[BCM2835_PLLA_PER]	= REGISTER_PLL_DIV(
+		.name = "plla_per",
+		.source_pll = "plla",
+		.cm_reg = CM_PLLA,
+		.a2w_reg = A2W_PLLA_PER,
+		.load_mask = CM_PLLA_LOADPER,
+		.hold_mask = CM_PLLA_HOLDPER,
+		.fixed_divider = 1),
+
+	/* PLLB is used for the ARM's clock. */
+	[BCM2835_PLLB]		= REGISTER_PLL(
+		.name = "pllb",
+		.cm_ctrl_reg = CM_PLLB,
+		.a2w_ctrl_reg = A2W_PLLB_CTRL,
+		.frac_reg = A2W_PLLB_FRAC,
+		.ana_reg_base = A2W_PLLB_ANA0,
+		.reference_enable_mask = A2W_XOSC_CTRL_PLLB_ENABLE,
+		.lock_mask = CM_LOCK_FLOCKB,
+
+		.ana = &bcm2835_ana_default,
+
+		.min_rate = 600000000u,
+		.max_rate = 3000000000u,
+		.max_fb_rate = BCM2835_MAX_FB_RATE),
+	[BCM2835_PLLB_ARM]	= REGISTER_PLL_DIV(
+		.name = "pllb_arm",
+		.source_pll = "pllb",
+		.cm_reg = CM_PLLB,
+		.a2w_reg = A2W_PLLB_ARM,
+		.load_mask = CM_PLLB_LOADARM,
+		.hold_mask = CM_PLLB_HOLDARM,
+		.fixed_divider = 1),
+
+	/*
+	 * PLLC is the core PLL, used to drive the core VPU clock.
+	 *
+	 * It is in the PX LDO power domain, which is on when the
+	 * AUDIO domain is on.
+	 */
+	[BCM2835_PLLC]		= REGISTER_PLL(
+		.name = "pllc",
+		.cm_ctrl_reg = CM_PLLC,
+		.a2w_ctrl_reg = A2W_PLLC_CTRL,
+		.frac_reg = A2W_PLLC_FRAC,
+		.ana_reg_base = A2W_PLLC_ANA0,
+		.reference_enable_mask = A2W_XOSC_CTRL_PLLC_ENABLE,
+		.lock_mask = CM_LOCK_FLOCKC,
+
+		.ana = &bcm2835_ana_default,
+
+		.min_rate = 600000000u,
+		.max_rate = 3000000000u,
+		.max_fb_rate = BCM2835_MAX_FB_RATE),
+	[BCM2835_PLLC_CORE0]	= REGISTER_PLL_DIV(
+		.name = "pllc_core0",
+		.source_pll = "pllc",
+		.cm_reg = CM_PLLC,
+		.a2w_reg = A2W_PLLC_CORE0,
+		.load_mask = CM_PLLC_LOADCORE0,
+		.hold_mask = CM_PLLC_HOLDCORE0,
+		.fixed_divider = 1),
+	[BCM2835_PLLC_CORE1]	= REGISTER_PLL_DIV(
+		.name = "pllc_core1",
+		.source_pll = "pllc",
+		.cm_reg = CM_PLLC,
+		.a2w_reg = A2W_PLLC_CORE1,
+		.load_mask = CM_PLLC_LOADCORE1,
+		.hold_mask = CM_PLLC_HOLDCORE1,
+		.fixed_divider = 1),
+	[BCM2835_PLLC_CORE2]	= REGISTER_PLL_DIV(
+		.name = "pllc_core2",
+		.source_pll = "pllc",
+		.cm_reg = CM_PLLC,
+		.a2w_reg = A2W_PLLC_CORE2,
+		.load_mask = CM_PLLC_LOADCORE2,
+		.hold_mask = CM_PLLC_HOLDCORE2,
+		.fixed_divider = 1),
+	[BCM2835_PLLC_PER]	= REGISTER_PLL_DIV(
+		.name = "pllc_per",
+		.source_pll = "pllc",
+		.cm_reg = CM_PLLC,
+		.a2w_reg = A2W_PLLC_PER,
+		.load_mask = CM_PLLC_LOADPER,
+		.hold_mask = CM_PLLC_HOLDPER,
+		.fixed_divider = 1),
+
+	/*
+	 * PLLD is the display PLL, used to drive DSI display panels.
+	 *
+	 * It is in the PX LDO power domain, which is on when the
+	 * AUDIO domain is on.
+	 */
+	[BCM2835_PLLD]		= REGISTER_PLL(
+		.name = "plld",
+		.cm_ctrl_reg = CM_PLLD,
+		.a2w_ctrl_reg = A2W_PLLD_CTRL,
+		.frac_reg = A2W_PLLD_FRAC,
+		.ana_reg_base = A2W_PLLD_ANA0,
+		.reference_enable_mask = A2W_XOSC_CTRL_DDR_ENABLE,
+		.lock_mask = CM_LOCK_FLOCKD,
+
+		.ana = &bcm2835_ana_default,
+
+		.min_rate = 600000000u,
+		.max_rate = 2400000000u,
+		.max_fb_rate = BCM2835_MAX_FB_RATE),
+	[BCM2835_PLLD_CORE]	= REGISTER_PLL_DIV(
+		.name = "plld_core",
+		.source_pll = "plld",
+		.cm_reg = CM_PLLD,
+		.a2w_reg = A2W_PLLD_CORE,
+		.load_mask = CM_PLLD_LOADCORE,
+		.hold_mask = CM_PLLD_HOLDCORE,
+		.fixed_divider = 1),
+	[BCM2835_PLLD_PER]	= REGISTER_PLL_DIV(
+		.name = "plld_per",
+		.source_pll = "plld",
+		.cm_reg = CM_PLLD,
+		.a2w_reg = A2W_PLLD_PER,
+		.load_mask = CM_PLLD_LOADPER,
+		.hold_mask = CM_PLLD_HOLDPER,
+		.fixed_divider = 1),
+
+	/*
+	 * PLLH is used to supply the pixel clock or the AUX clock for the
+	 * TV encoder.
+	 *
+	 * It is in the HDMI power domain.
+	 */
+	[BCM2835_PLLH]		= REGISTER_PLL(
+		"pllh",
+		.cm_ctrl_reg = CM_PLLH,
+		.a2w_ctrl_reg = A2W_PLLH_CTRL,
+		.frac_reg = A2W_PLLH_FRAC,
+		.ana_reg_base = A2W_PLLH_ANA0,
+		.reference_enable_mask = A2W_XOSC_CTRL_PLLC_ENABLE,
+		.lock_mask = CM_LOCK_FLOCKH,
+
+		.ana = &bcm2835_ana_pllh,
+
+		.min_rate = 600000000u,
+		.max_rate = 3000000000u,
+		.max_fb_rate = BCM2835_MAX_FB_RATE),
+	[BCM2835_PLLH_RCAL]	= REGISTER_PLL_DIV(
+		.name = "pllh_rcal",
+		.source_pll = "pllh",
+		.cm_reg = CM_PLLH,
+		.a2w_reg = A2W_PLLH_RCAL,
+		.load_mask = CM_PLLH_LOADRCAL,
+		.hold_mask = 0,
+		.fixed_divider = 10),
+	[BCM2835_PLLH_AUX]	= REGISTER_PLL_DIV(
+		.name = "pllh_aux",
+		.source_pll = "pllh",
+		.cm_reg = CM_PLLH,
+		.a2w_reg = A2W_PLLH_AUX,
+		.load_mask = CM_PLLH_LOADAUX,
+		.hold_mask = 0,
+		.fixed_divider = 10),
+	[BCM2835_PLLH_PIX]	= REGISTER_PLL_DIV(
+		.name = "pllh_pix",
+		.source_pll = "pllh",
+		.cm_reg = CM_PLLH,
+		.a2w_reg = A2W_PLLH_PIX,
+		.load_mask = CM_PLLH_LOADPIX,
+		.hold_mask = 0,
+		.fixed_divider = 10),
+
 	/* the clocks */
-	[BCM2835_CLOCK_TIMER]	= REGISTER_CLK(&bcm2835_clock_timer_data),
-	[BCM2835_CLOCK_OTP]	= REGISTER_CLK(&bcm2835_clock_otp_data),
-	[BCM2835_CLOCK_TSENS]	= REGISTER_CLK(&bcm2835_clock_tsens_data),
-	[BCM2835_CLOCK_VPU]	= REGISTER_CLK(&bcm2835_clock_vpu_data),
-	[BCM2835_CLOCK_V3D]	= REGISTER_CLK(&bcm2835_clock_v3d_data),
-	[BCM2835_CLOCK_ISP]	= REGISTER_CLK(&bcm2835_clock_isp_data),
-	[BCM2835_CLOCK_H264]	= REGISTER_CLK(&bcm2835_clock_h264_data),
-	[BCM2835_CLOCK_V3D]	= REGISTER_CLK(&bcm2835_clock_v3d_data),
-	[BCM2835_CLOCK_SDRAM]	= REGISTER_CLK(&bcm2835_clock_sdram_data),
-	[BCM2835_CLOCK_UART]	= REGISTER_CLK(&bcm2835_clock_uart_data),
-	[BCM2835_CLOCK_VEC]	= REGISTER_CLK(&bcm2835_clock_vec_data),
-	[BCM2835_CLOCK_HSM]	= REGISTER_CLK(&bcm2835_clock_hsm_data),
-	[BCM2835_CLOCK_EMMC]	= REGISTER_CLK(&bcm2835_clock_emmc_data),
-	[BCM2835_CLOCK_PWM]	= REGISTER_CLK(&bcm2835_clock_pwm_data),
+
+	/* clocks with oscillator parent mux */
+
+	/* One Time Programmable Memory clock.  Maximum 10Mhz. */
+	[BCM2835_CLOCK_OTP]	= REGISTER_OSC_CLK(
+		.name = "otp",
+		.ctl_reg = CM_OTPCTL,
+		.div_reg = CM_OTPDIV,
+		.int_bits = 4,
+		.frac_bits = 0),
+	/*
+	 * Used for a 1Mhz clock for the system clocksource, and also used
+	 * bythe watchdog timer and the camera pulse generator.
+	 */
+	[BCM2835_CLOCK_TIMER]	= REGISTER_OSC_CLK(
+		.name = "timer",
+		.ctl_reg = CM_TIMERCTL,
+		.div_reg = CM_TIMERDIV,
+		.int_bits = 6,
+		.frac_bits = 12),
+	/*
+	 * Clock for the temperature sensor.
+	 * Generally run at 2Mhz, max 5Mhz.
+	 */
+	[BCM2835_CLOCK_TSENS]	= REGISTER_OSC_CLK(
+		.name = "tsens",
+		.ctl_reg = CM_TSENSCTL,
+		.div_reg = CM_TSENSDIV,
+		.int_bits = 5,
+		.frac_bits = 0),
+
+	/* clocks with vpu parent mux */
+	[BCM2835_CLOCK_H264]	= REGISTER_VPU_CLK(
+		.name = "h264",
+		.ctl_reg = CM_H264CTL,
+		.div_reg = CM_H264DIV,
+		.int_bits = 4,
+		.frac_bits = 8),
+	[BCM2835_CLOCK_ISP]	= REGISTER_VPU_CLK(
+		.name = "isp",
+		.ctl_reg = CM_ISPCTL,
+		.div_reg = CM_ISPDIV,
+		.int_bits = 4,
+		.frac_bits = 8),
+	/*
+	 * Secondary SDRAM clock.  Used for low-voltage modes when the PLL
+	 * in the SDRAM controller can't be used.
+	 */
+	[BCM2835_CLOCK_SDRAM]	= REGISTER_VPU_CLK(
+		.name = "sdram",
+		.ctl_reg = CM_SDCCTL,
+		.div_reg = CM_SDCDIV,
+		.int_bits = 6,
+		.frac_bits = 0),
+	[BCM2835_CLOCK_V3D]	= REGISTER_VPU_CLK(
+		.name = "v3d",
+		.ctl_reg = CM_V3DCTL,
+		.div_reg = CM_V3DDIV,
+		.int_bits = 4,
+		.frac_bits = 8),
+	/*
+	 * VPU clock.  This doesn't have an enable bit, since it drives
+	 * the bus for everything else, and is special so it doesn't need
+	 * to be gated for rate changes.  It is also known as "clk_audio"
+	 * in various hardware documentation.
+	 */
+	[BCM2835_CLOCK_VPU]	= REGISTER_VPU_CLK(
+		.name = "vpu",
+		.ctl_reg = CM_VPUCTL,
+		.div_reg = CM_VPUDIV,
+		.int_bits = 12,
+		.frac_bits = 8,
+		.is_vpu_clock = true),
+
+	/* clocks with per parent mux */
+
+	/* Arasan EMMC clock */
+	[BCM2835_CLOCK_EMMC]	= REGISTER_PER_CLK(
+		.name = "emmc",
+		.ctl_reg = CM_EMMCCTL,
+		.div_reg = CM_EMMCDIV,
+		.int_bits = 4,
+		.frac_bits = 8),
+	/* HDMI state machine */
+	[BCM2835_CLOCK_HSM]	= REGISTER_PER_CLK(
+		.name = "hsm",
+		.ctl_reg = CM_HSMCTL,
+		.div_reg = CM_HSMDIV,
+		.int_bits = 4,
+		.frac_bits = 8),
+	[BCM2835_CLOCK_PWM]	= REGISTER_PER_CLK(
+		.name = "pwm",
+		.ctl_reg = CM_PWMCTL,
+		.div_reg = CM_PWMDIV,
+		.int_bits = 12,
+		.frac_bits = 12,
+		.is_mash_clock = true),
+	[BCM2835_CLOCK_UART]	= REGISTER_PER_CLK(
+		.name = "uart",
+		.ctl_reg = CM_UARTCTL,
+		.div_reg = CM_UARTDIV,
+		.int_bits = 10,
+		.frac_bits = 12),
+	/* TV encoder clock.  Only operating frequency is 108Mhz.  */
+	[BCM2835_CLOCK_VEC]	= REGISTER_PER_CLK(
+		.name = "vec",
+		.ctl_reg = CM_VECCTL,
+		.div_reg = CM_VECDIV,
+		.int_bits = 4,
+		.frac_bits = 0),
+
 	/* the gates */
+
+	/*
+	 * CM_PERIICTL (and CM_PERIACTL, CM_SYSCTL and CM_VPUCTL if
+	 * you have the debug bit set in the power manager, which we
+	 * don't bother exposing) are individual gates off of the
+	 * non-stop vpu clock.
+	 */
 	[BCM2835_CLOCK_PERI_IMAGE] = REGISTER_GATE(
-		&bcm2835_clock_peri_image_data),
+		.name = "peri_image",
+		.parent = "vpu",
+		.ctl_reg = CM_PERIICTL),
 };
 
 static int bcm2835_clk_probe(struct platform_device *pdev)
