From f7121d2b19ddad33a09408a2c5923bfd95da8533 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 6 Jan 2016 20:06:49 +0100
Subject: [PATCH 017/102] clk: add hifsys reset

Hi,

small patch to add hifsys reset bits. Maybe you could add it to the next
version of your patch series. i have teste scpsys and clk on mt7623 today
and it works well.

thanks,
	John

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/clk/mediatek/clk-mt2701.c                    |    2 ++
 include/dt-bindings/reset-controller/mt2701-resets.h |    9 +++++++++
 2 files changed, 11 insertions(+)

--- a/drivers/clk/mediatek/clk-mt2701.c
+++ b/drivers/clk/mediatek/clk-mt2701.c
@@ -1000,6 +1000,8 @@ static void __init mtk_hifsys_init(struc
 	if (r)
 		pr_err("%s(): could not register clock provider: %d\n",
 			__func__, r);
+
+	mtk_register_reset_controller(node, 1, 0x34);
 }
 CLK_OF_DECLARE(mtk_hifsys, "mediatek,mt2701-hifsys", mtk_hifsys_init);
 
--- a/include/dt-bindings/reset-controller/mt2701-resets.h
+++ b/include/dt-bindings/reset-controller/mt2701-resets.h
@@ -71,4 +71,13 @@
 #define MT2701_TOPRGU_CONN_MCU_RST		12
 #define MT2701_TOPRGU_BDP_DISP_RST		13
 
+/* HIFSYS resets */
+#define MT2701_HIFSYS_UHOST0_RST		3
+#define MT2701_HIFSYS_UHOST1_RST		4
+#define MT2701_HIFSYS_UPHY0_RST			21
+#define MT2701_HIFSYS_UPHY1_RST			22
+#define MT2701_HIFSYS_PCIE0_RST			24
+#define MT2701_HIFSYS_PCIE1_RST			25
+#define MT2701_HIFSYS_PCIE2_RST			26
+
 #endif  /* _DT_BINDINGS_RESET_CONTROLLER_MT2701 */
