--- a/arch/arm/boot/dts/qcom-ipq8064-ap148.dts
+++ b/arch/arm/boot/dts/qcom-ipq8064-ap148.dts
@@ -4,6 +4,11 @@
 	model = "Qualcomm IPQ8064/AP148";
 	compatible = "qcom,ipq8064-ap148", "qcom,ipq8064";
 
+	memory@0 {
+		reg = <0x42000000 0x1e000000>;
+		device_type = "memory";
+	};
+
 	reserved-memory {
 		#address-cells = <1>;
 		#size-cells = <1>;
