/*
 * Copyright (C) 2014, 2015 Synopsys, Inc. (www.synopsys.com)
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

/*
 * Device tree for AXC003 CPU card: HS38x2 (Dual Core) with IDU intc
 */

/ {
	compatible = "snps,arc";
	clock-frequency = <90000000>;
	#address-cells = <1>;
	#size-cells = <1>;

	cpu_card {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;

		ranges = <0x00000000 0xf0000000 0x10000000>;

		cpu_intc: archs-intc@cpu {
			compatible = "snps,archs-intc";
			interrupt-controller;
			#interrupt-cells = <1>;
		};

		idu_intc: idu-interrupt-controller {
			compatible = "snps,archs-idu-intc";
			interrupt-controller;
			interrupt-parent = <&cpu_intc>;

			/*
			 * <hwirq  distribution>
			 * distribution: 0=RR; 1=cpu0, 2=cpu1, 4=cpu2, 8=cpu3
			 */
			#interrupt-cells = <2>;

			/*
			 * upstream irqs to core intc - downstream these are
			 * "COMMON" irq 0,1..
			 */
			interrupts = <24 25>;
		};

		/*
		 * this GPIO block ORs all interrupts on CPU card (creg,..)
		 * to uplink only 1 IRQ to ARC core intc
		 */
		dw-apb-gpio@0x2000 {
			compatible = "snps,dw-apb-gpio";
			reg = < 0x2000 0x80 >;
			#address-cells = <1>;
			#size-cells = <0>;

			ictl_intc: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <30>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupt-parent = <&idu_intc>;

				/*
				 * cmn irq 1 -> cpu irq 25
				 * Distribute to cpu0 only
				 */
				interrupts = <1 1>;
			};
		};

		debug_uart: dw-apb-uart@0x5000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x5000 0x100>;
			clock-frequency = <33333000>;
			interrupt-parent = <&ictl_intc>;
			interrupts = <2 4>;
			baud = <115200>;
			reg-shift = <2>;
			reg-io-width = <4>;
		};

		arcpct0: pct {
			compatible = "snps,archs-pct";
			#interrupt-cells = <1>;
			interrupt-parent = <&cpu_intc>;
			interrupts = <20>;
		};
	};

	/*
	 * This INTC is actually connected to DW APB GPIO
	 * which acts as a wire between MB INTC and CPU INTC.
	 * GPIO INTC is configured in platform init code
	 * and here we mimic direct connection from MB INTC to
	 * CPU INTC, thus we set "interrupts = <0 1>" instead of
	 * "interrupts = <12>"
	 *
	 * This intc actually resides on MB, but we move it here to
	 * avoid duplicating the MB dtsi file given that IRQ from
	 * this intc to cpu intc are different for axs101 and axs103
	 */
	mb_intc: dw-apb-ictl@0xe0012000 {
		#interrupt-cells = <1>;
		compatible = "snps,dw-apb-ictl";
		reg = < 0xe0012000 0x200 >;
		interrupt-controller;
		interrupt-parent = <&idu_intc>;
		interrupts = <0 1>;	/* cmn irq 0 -> cpu irq 24
					   distribute to cpu0 only */
	};

	memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x80000000 0x40000000>;
		device_type = "memory";
		reg = <0x80000000 0x20000000>;	/* 512MiB */
	};
};
