From a6dd2b7d0cf90158755da4949006feebde8c9fe5 Mon Sep 17 00:00:00 2001
From: wm4 <wm4@nowhere>
Date: Wed, 13 Jan 2016 19:43:12 +0100
Subject: [PATCH 129/381] bcm2835: implement channel map API

Report all layouts supported by the HDMI protocol to userspace.
Make the videocore set the correct layout according to the
userspace request.

Some code taken from patch_hdmi.c. In particular, the HDMI channel
layout table was copied without changes - with the idea in mind that
hopefully it can be shared one day. Or at least updating it will be
simpler.

In my tests, everything appears to work, except when outputting
FL FR RL RR. Then my receiver outputs RL on both the RL and RR
speakers, while RR is never heard.
---
 sound/arm/bcm2835-ctl.c   | 276 ++++++++++++++++++++++++++++++++++++++++++++++
 sound/arm/bcm2835-pcm.c   |  22 +++-
 sound/arm/bcm2835-vchiq.c |  13 +++
 sound/arm/bcm2835.h       |   4 +
 4 files changed, 311 insertions(+), 4 deletions(-)

--- a/sound/arm/bcm2835-ctl.c
+++ b/sound/arm/bcm2835-ctl.c
@@ -300,6 +300,281 @@ static struct snd_kcontrol_new snd_bcm28
 	},
 };
 
+struct cea_channel_speaker_allocation {
+	int ca_index;
+	int speakers[8];
+};
+
+#define FL	SNDRV_CHMAP_FL
+#define FR	SNDRV_CHMAP_FR
+#define RL	SNDRV_CHMAP_RL
+#define RR	SNDRV_CHMAP_RR
+#define LFE	SNDRV_CHMAP_LFE
+#define FC	SNDRV_CHMAP_FC
+#define RLC	SNDRV_CHMAP_RLC
+#define RRC	SNDRV_CHMAP_RRC
+#define RC	SNDRV_CHMAP_RC
+#define FLC	SNDRV_CHMAP_FLC
+#define FRC	SNDRV_CHMAP_FRC
+#define FLH	SNDRV_CHMAP_TFL
+#define FRH	SNDRV_CHMAP_TFR
+#define FLW	SNDRV_CHMAP_FLW
+#define FRW	SNDRV_CHMAP_FRW
+#define TC	SNDRV_CHMAP_TC
+#define FCH	SNDRV_CHMAP_TFC
+
+/*
+ * CEA-861 channel maps
+ *
+ * Stolen from sound/pci/hda/patch_hdmi.c
+ * (unlike the source, this uses SNDRV_* constants directly, as by the
+ *  map_tables array in patch_hdmi.c)
+ * Unknown entries use 0, which unfortunately is SNDRV_CHMAP_UNKNOWN instead
+ * of SNDRV_CHMAP_NA.
+ */
+static struct cea_channel_speaker_allocation channel_allocations[] = {
+/*			  channel:   7     6    5    4    3     2    1    0  */
+{ .ca_index = 0x00,  .speakers = {   0,    0,   0,   0,   0,    0,  FR,  FL } },
+				 /* 2.1 */
+{ .ca_index = 0x01,  .speakers = {   0,    0,   0,   0,   0,  LFE,  FR,  FL } },
+				 /* Dolby Surround */
+{ .ca_index = 0x02,  .speakers = {   0,    0,   0,   0,  FC,    0,  FR,  FL } },
+				 /* surround40 */
+{ .ca_index = 0x08,  .speakers = {   0,    0,  RR,  RL,   0,    0,  FR,  FL } },
+				 /* surround41 */
+{ .ca_index = 0x09,  .speakers = {   0,    0,  RR,  RL,   0,  LFE,  FR,  FL } },
+				 /* surround50 */
+{ .ca_index = 0x0a,  .speakers = {   0,    0,  RR,  RL,  FC,    0,  FR,  FL } },
+				 /* surround51 */
+{ .ca_index = 0x0b,  .speakers = {   0,    0,  RR,  RL,  FC,  LFE,  FR,  FL } },
+				 /* 6.1 */
+{ .ca_index = 0x0f,  .speakers = {   0,   RC,  RR,  RL,  FC,  LFE,  FR,  FL } },
+				 /* surround71 */
+{ .ca_index = 0x13,  .speakers = { RRC,  RLC,  RR,  RL,  FC,  LFE,  FR,  FL } },
+
+{ .ca_index = 0x03,  .speakers = {   0,    0,   0,   0,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x04,  .speakers = {   0,    0,   0,  RC,   0,    0,  FR,  FL } },
+{ .ca_index = 0x05,  .speakers = {   0,    0,   0,  RC,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x06,  .speakers = {   0,    0,   0,  RC,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x07,  .speakers = {   0,    0,   0,  RC,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x0c,  .speakers = {   0,   RC,  RR,  RL,   0,    0,  FR,  FL } },
+{ .ca_index = 0x0d,  .speakers = {   0,   RC,  RR,  RL,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x0e,  .speakers = {   0,   RC,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x10,  .speakers = { RRC,  RLC,  RR,  RL,   0,    0,  FR,  FL } },
+{ .ca_index = 0x11,  .speakers = { RRC,  RLC,  RR,  RL,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x12,  .speakers = { RRC,  RLC,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x14,  .speakers = { FRC,  FLC,   0,   0,   0,    0,  FR,  FL } },
+{ .ca_index = 0x15,  .speakers = { FRC,  FLC,   0,   0,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x16,  .speakers = { FRC,  FLC,   0,   0,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x17,  .speakers = { FRC,  FLC,   0,   0,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x18,  .speakers = { FRC,  FLC,   0,  RC,   0,    0,  FR,  FL } },
+{ .ca_index = 0x19,  .speakers = { FRC,  FLC,   0,  RC,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x1a,  .speakers = { FRC,  FLC,   0,  RC,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x1b,  .speakers = { FRC,  FLC,   0,  RC,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x1c,  .speakers = { FRC,  FLC,  RR,  RL,   0,    0,  FR,  FL } },
+{ .ca_index = 0x1d,  .speakers = { FRC,  FLC,  RR,  RL,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x1e,  .speakers = { FRC,  FLC,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x1f,  .speakers = { FRC,  FLC,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x20,  .speakers = {   0,  FCH,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x21,  .speakers = {   0,  FCH,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x22,  .speakers = {  TC,    0,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x23,  .speakers = {  TC,    0,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x24,  .speakers = { FRH,  FLH,  RR,  RL,   0,    0,  FR,  FL } },
+{ .ca_index = 0x25,  .speakers = { FRH,  FLH,  RR,  RL,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x26,  .speakers = { FRW,  FLW,  RR,  RL,   0,    0,  FR,  FL } },
+{ .ca_index = 0x27,  .speakers = { FRW,  FLW,  RR,  RL,   0,  LFE,  FR,  FL } },
+{ .ca_index = 0x28,  .speakers = {  TC,   RC,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x29,  .speakers = {  TC,   RC,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x2a,  .speakers = { FCH,   RC,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x2b,  .speakers = { FCH,   RC,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x2c,  .speakers = {  TC,  FCH,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x2d,  .speakers = {  TC,  FCH,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x2e,  .speakers = { FRH,  FLH,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x2f,  .speakers = { FRH,  FLH,  RR,  RL,  FC,  LFE,  FR,  FL } },
+{ .ca_index = 0x30,  .speakers = { FRW,  FLW,  RR,  RL,  FC,    0,  FR,  FL } },
+{ .ca_index = 0x31,  .speakers = { FRW,  FLW,  RR,  RL,  FC,  LFE,  FR,  FL } },
+};
+
+static int snd_bcm2835_chmap_ctl_tlv(struct snd_kcontrol *kcontrol, int op_flag,
+				     unsigned int size, unsigned int __user *tlv)
+{
+	unsigned int __user *dst;
+	int count = 0;
+	int i;
+
+	if (size < 8)
+		return -ENOMEM;
+	if (put_user(SNDRV_CTL_TLVT_CONTAINER, tlv))
+		return -EFAULT;
+	size -= 8;
+	dst = tlv + 2;
+	for (i = 0; i < ARRAY_SIZE(channel_allocations); i++) {
+		struct cea_channel_speaker_allocation *ch = &channel_allocations[i];
+		int num_chs = 0;
+		int chs_bytes;
+		int c;
+
+		for (c = 0; c < 8; c++) {
+			if (ch->speakers[c])
+				num_chs++;
+		}
+
+		chs_bytes = num_chs * 4;
+		if (size < 8)
+			return -ENOMEM;
+		if (put_user(SNDRV_CTL_TLVT_CHMAP_FIXED, dst) ||
+		    put_user(chs_bytes, dst + 1))
+			return -EFAULT;
+		dst += 2;
+		size -= 8;
+		count += 8;
+		if (size < chs_bytes)
+			return -ENOMEM;
+		size -= chs_bytes;
+		count += chs_bytes;
+		for (c = 0; c < 8; c++) {
+			int sp = ch->speakers[7 - c];
+			if (sp) {
+				if (put_user(sp, dst))
+					return -EFAULT;
+				dst++;
+			}
+		}
+	}
+	if (put_user(count, tlv + 1))
+		return -EFAULT;
+	return 0;
+}
+
+static int snd_bcm2835_chmap_ctl_get(struct snd_kcontrol *kcontrol,
+				     struct snd_ctl_elem_value *ucontrol)
+{
+	struct snd_pcm_chmap *info = snd_kcontrol_chip(kcontrol);
+	bcm2835_chip_t *chip = info->private_data;
+	unsigned int idx = snd_ctl_get_ioffidx(kcontrol, &ucontrol->id);
+	struct snd_pcm_substream *substream = snd_pcm_chmap_substream(info, idx);
+	struct cea_channel_speaker_allocation *ch = NULL;
+	int cur = 0;
+	int i;
+
+	if (!substream || !substream->runtime)
+		return -ENODEV;
+
+	for (i = 0; i < ARRAY_SIZE(channel_allocations); i++) {
+		if (channel_allocations[i].ca_index == chip->cea_chmap)
+			ch = &channel_allocations[i];
+	}
+
+	/* If no layout was set yet, return a dummy. Apparently the userspace
+	 * API will be confused if we don't. */
+	if (!ch)
+		ch = &channel_allocations[0];
+
+	for (i = 0; i < 8; i++) {
+		if (ch->speakers[7 - i])
+			ucontrol->value.integer.value[cur++] = ch->speakers[7 - i];
+	}
+	while (cur < 8)
+		ucontrol->value.integer.value[cur++] = SNDRV_CHMAP_NA;
+	return 0;
+}
+
+static int snd_bcm2835_chmap_ctl_put(struct snd_kcontrol *kcontrol,
+				     struct snd_ctl_elem_value *ucontrol)
+{
+	struct snd_pcm_chmap *info = snd_kcontrol_chip(kcontrol);
+	bcm2835_chip_t *chip = info->private_data;
+	unsigned int idx = snd_ctl_get_ioffidx(kcontrol, &ucontrol->id);
+	struct snd_pcm_substream *substream = snd_pcm_chmap_substream(info, idx);
+	int i, prepared = 0, cea_chmap = -1;
+	int remap[8];
+
+	if (!substream || !substream->runtime)
+		return -ENODEV;
+
+	switch (substream->runtime->status->state) {
+	case SNDRV_PCM_STATE_OPEN:
+	case SNDRV_PCM_STATE_SETUP:
+		break;
+	case SNDRV_PCM_STATE_PREPARED:
+		prepared = 1;
+		break;
+	default:
+		return -EBUSY;
+	}
+
+	for (i = 0; i < ARRAY_SIZE(channel_allocations); i++) {
+		struct cea_channel_speaker_allocation *ch = &channel_allocations[i];
+		int matches = 1;
+		int cur = 0;
+		int x;
+		memset(remap, 0, sizeof(remap));
+		for (x = 0; x < substream->runtime->channels; x++) {
+			int sp = ucontrol->value.integer.value[x];
+			while (cur < 8 && !ch->speakers[7 - cur])
+				cur++;
+			if (cur >= 8) {
+				/* user has more channels than ch */
+				matches = 0;
+				break;
+			}
+			if (ch->speakers[7 - cur] != sp) {
+				matches = 0;
+				break;
+			}
+			remap[x] = cur;
+			cur++;
+		}
+		for (x = cur; x < 8; x++) {
+			if (ch->speakers[7 - x]) {
+				/* ch has more channels than user */
+				matches = 0;
+				break;
+			}
+		}
+		if (matches) {
+			cea_chmap = ch->ca_index;
+			break;
+		}
+	}
+
+	if (cea_chmap < 0)
+		return -EINVAL;
+
+	/* don't change the layout if another substream is active */
+	if (chip->opened != (1 << substream->number) && chip->cea_chmap != cea_chmap)
+		return -EBUSY; /* unsure whether this is a good error code */
+
+	chip->cea_chmap = cea_chmap;
+	for (i = 0; i < 8; i++)
+		chip->map_channels[i] = remap[i];
+	if (prepared)
+		snd_bcm2835_pcm_prepare_again(substream);
+	return 0;
+}
+
+static int snd_bcm2835_add_chmap_ctl(bcm2835_chip_t * chip)
+{
+	struct snd_pcm_chmap *chmap;
+	struct snd_kcontrol *kctl;
+	int err, i;
+
+	err = snd_pcm_add_chmap_ctls(chip->pcm,
+				     SNDRV_PCM_STREAM_PLAYBACK,
+				     NULL, 8, 0, &chmap);
+	if (err < 0)
+		return err;
+	/* override handlers */
+	chmap->private_data = chip;
+	kctl = chmap->kctl;
+	for (i = 0; i < kctl->count; i++)
+		kctl->vd[i].access |= SNDRV_CTL_ELEM_ACCESS_WRITE;
+	kctl->get = snd_bcm2835_chmap_ctl_get;
+	kctl->put = snd_bcm2835_chmap_ctl_put;
+	kctl->tlv.c = snd_bcm2835_chmap_ctl_tlv;
+	return 0;
+}
+
 int snd_bcm2835_new_ctl(bcm2835_chip_t * chip)
 {
 	int err;
@@ -313,6 +588,7 @@ int snd_bcm2835_new_ctl(bcm2835_chip_t *
 		if (err < 0)
 			return err;
 	}
+	snd_bcm2835_add_chmap_ctl(chip);
 	for (idx = 0; idx < ARRAY_SIZE(snd_bcm2835_spdif); idx++) {
 		err = snd_ctl_add(chip->card,
 				snd_ctl_new1(&snd_bcm2835_spdif[idx], chip));
--- a/sound/arm/bcm2835-pcm.c
+++ b/sound/arm/bcm2835-pcm.c
@@ -231,6 +231,9 @@ static int snd_bcm2835_playback_open_gen
 
 	chip->alsa_stream[idx] = alsa_stream;
 
+	if (!chip->opened)
+		chip->cea_chmap = -1;
+
 	chip->opened |= (1 << idx);
 	alsa_stream->open = 1;
 	alsa_stream->draining = 1;
@@ -341,8 +344,7 @@ static int snd_bcm2835_pcm_hw_free(struc
 	return snd_pcm_lib_free_pages(substream);
 }
 
-/* prepare callback */
-static int snd_bcm2835_pcm_prepare(struct snd_pcm_substream *substream)
+int snd_bcm2835_pcm_prepare_again(struct snd_pcm_substream *substream)
 {
 	bcm2835_chip_t *chip = snd_pcm_substream_chip(substream);
 	struct snd_pcm_runtime *runtime = substream->runtime;
@@ -350,8 +352,6 @@ static int snd_bcm2835_pcm_prepare(struc
 	int channels;
 	int err;
 
-	audio_info(" .. IN\n");
-
 	/* notify the vchiq that it should enter spdif passthrough mode by
 	 * setting channels=0 (see
 	 * https://github.com/raspberrypi/linux/issues/528) */
@@ -367,6 +367,20 @@ static int snd_bcm2835_pcm_prepare(struc
 		audio_error(" error setting hw params\n");
 	}
 
+	return err;
+}
+
+/* prepare callback */
+static int snd_bcm2835_pcm_prepare(struct snd_pcm_substream *substream)
+{
+	bcm2835_chip_t *chip = snd_pcm_substream_chip(substream);
+	struct snd_pcm_runtime *runtime = substream->runtime;
+	bcm2835_alsa_stream_t *alsa_stream = runtime->private_data;
+
+	audio_info(" .. IN\n");
+
+	snd_bcm2835_pcm_prepare_again(substream);
+
 	bcm2835_audio_setup(alsa_stream);
 
 	/* in preparation of the stream, set the controls (volume level) of the stream */
--- a/sound/arm/bcm2835-vchiq.c
+++ b/sound/arm/bcm2835-vchiq.c
@@ -570,6 +570,8 @@ int bcm2835_audio_set_params(bcm2835_als
 	VC_AUDIO_MSG_T m;
 	AUDIO_INSTANCE_T *instance = alsa_stream->instance;
 	int32_t success;
+	uint32_t chmap_value;
+	int i;
 	int ret;
 	LOG_DBG(" .. IN\n");
 
@@ -593,10 +595,21 @@ int bcm2835_audio_set_params(bcm2835_als
 
 	instance->result = -1;
 
+	if (alsa_stream->chip->cea_chmap >= 0) {
+		chmap_value = (unsigned)alsa_stream->chip->cea_chmap << 24;
+	} else {
+		chmap_value = 0; /* force stereo */
+		for (i = 0; i < 8; i++)
+			alsa_stream->chip->map_channels[i] = i;
+	}
+	for (i = 0; i < 8; i++)
+		chmap_value |= alsa_stream->chip->map_channels[i] << (i * 3);
+
 	m.type = VC_AUDIO_MSG_TYPE_CONFIG;
 	m.u.config.channels = channels;
 	m.u.config.samplerate = samplerate;
 	m.u.config.bps = bps;
+	m.u.config.channelmap = chmap_value;
 
 	/* Create the message available completion */
 	init_completion(&instance->msg_avail_comp);
--- a/sound/arm/bcm2835.h
+++ b/sound/arm/bcm2835.h
@@ -107,6 +107,8 @@ typedef struct bcm2835_chip {
 	int old_volume; /* stores the volume value whist muted */
 	int dest;
 	int mute;
+	int cea_chmap; /* currently requested Audio InfoFrame Data Byte 4 */
+	int map_channels[8];
 
 	unsigned int opened;
 	unsigned int spdif_status;
@@ -149,6 +151,8 @@ int snd_bcm2835_new_ctl(bcm2835_chip_t *
 int snd_bcm2835_new_pcm(bcm2835_chip_t * chip);
 int snd_bcm2835_new_spdif_pcm(bcm2835_chip_t * chip);
 
+int snd_bcm2835_pcm_prepare_again(struct snd_pcm_substream *substream);
+
 int bcm2835_audio_open(bcm2835_alsa_stream_t * alsa_stream);
 int bcm2835_audio_close(bcm2835_alsa_stream_t * alsa_stream);
 int bcm2835_audio_set_params(bcm2835_alsa_stream_t * alsa_stream,
