From dc02b5bdc0f962c1c9da85d98c11612e858280b3 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 15 Dec 2015 23:46:32 +0000
Subject: [PATCH 118/381] drm/vc4: Use "hpd-gpios" for HDMI GPIO, like what
 landed upstream.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
+++ b/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
@@ -68,7 +68,7 @@
 				      <0x7e808000 0x100>;
 				interrupts = <2 8>, <2 9>;
 				ddc = <&i2c2>;
-				hpd-gpio = <&gpio 46 GPIO_ACTIVE_HIGH>;
+				hpd-gpios = <&gpio 46 GPIO_ACTIVE_HIGH>;
 				clocks = <&cprman BCM2835_PLLH_PIX>,
 					 <&cprman BCM2835_CLOCK_HSM>;
 				clock-names = "pixel", "hdmi";
