From 5369ea497f871c261a8ceb49508999160fdd3fc7 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <6by9@users.noreply.github.com>
Date: Tue, 31 May 2016 10:38:31 +0100
Subject: [PATCH 365/381] BCM2835-V4L2: Increase minimum resolution to 32x32

https://github.com/raspberrypi/linux/issues/1498 showed
up that 16x16 is failing to work on the GPU for some reason.

GPU bug being tracked on
https://github.com/raspberrypi/firmware/issues/607
Workaround here by increasing minimum resolution via V4L2
to 32x32.

Signed-off-by: Dave Stevenson <6by9@users.noreply.github.com>
---
 drivers/media/platform/bcm2835/bcm2835-camera.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/media/platform/bcm2835/bcm2835-camera.c
+++ b/drivers/media/platform/bcm2835/bcm2835-camera.c
@@ -36,8 +36,8 @@
 
 #define BM2835_MMAL_VERSION "0.0.2"
 #define BM2835_MMAL_MODULE_NAME "bcm2835-v4l2"
-#define MIN_WIDTH 16
-#define MIN_HEIGHT 16
+#define MIN_WIDTH 32
+#define MIN_HEIGHT 32
 #define MIN_BUFFER_SIZE (80*1024)
 
 #define MAX_VIDEO_MODE_WIDTH 1280
