From ec7710516621d3131c7e025a73ab8354ec21f7f8 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 29 May 2015 11:48:59 +0100
Subject: [PATCH 182/381] Enable Dynamic Device Tree for bcmrpi_defconfig and
 bcm2709_defconfig

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/configs/bcm2709_defconfig | 2 +-
 arch/arm/configs/bcmrpi_defconfig  | 1 +
 2 files changed, 2 insertions(+), 1 deletion(-)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -403,6 +403,7 @@ CONFIG_MTD=m
 CONFIG_MTD_BLOCK=m
 CONFIG_MTD_NAND=m
 CONFIG_MTD_UBI=m
+CONFIG_OF_CONFIGFS=y
 CONFIG_ZRAM=m
 CONFIG_ZRAM_LZ4_COMPRESS=y
 CONFIG_BLK_DEV_LOOP=y
@@ -1161,7 +1162,6 @@ CONFIG_NTFS_FS=m
 CONFIG_NTFS_RW=y
 CONFIG_TMPFS=y
 CONFIG_TMPFS_POSIX_ACL=y
-CONFIG_CONFIGFS_FS=y
 CONFIG_ECRYPT_FS=m
 CONFIG_HFS_FS=m
 CONFIG_HFSPLUS_FS=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -396,6 +396,7 @@ CONFIG_MTD=m
 CONFIG_MTD_BLOCK=m
 CONFIG_MTD_NAND=m
 CONFIG_MTD_UBI=m
+CONFIG_OF_OVERLAY=y
 CONFIG_ZRAM=m
 CONFIG_ZRAM_LZ4_COMPRESS=y
 CONFIG_BLK_DEV_LOOP=y
