From a9d3c50f084d4d6d1063969c04bc8233fe1437c1 Mon Sep 17 00:00:00 2001
From: wm4 <wm4@nowhere>
Date: Tue, 19 Apr 2016 16:29:41 +0200
Subject: [PATCH 250/381] bcm2835: add fallback channel layouts if channel map
 API is not used

Should be more useful than just forcing stereo.

We can't match the exact legacy ALSA channel layouts, so this is a
"best effort" hack.

I'm not sure what happens if the application requests channel counts
that are not power-of-2s. The channel map API hopefully forces
applications which use the channel map API to request the correct
count by adding padding channels, but the bare API enforces
nothing. Possibly this could be added to rate_hw_constraint_channels
at a later point.
---
 sound/arm/bcm2835-vchiq.c | 11 ++++++++++-
 1 file changed, 10 insertions(+), 1 deletion(-)

--- a/sound/arm/bcm2835-vchiq.c
+++ b/sound/arm/bcm2835-vchiq.c
@@ -598,7 +598,16 @@ int bcm2835_audio_set_params(bcm2835_als
 	if (alsa_stream->chip->cea_chmap >= 0) {
 		chmap_value = (unsigned)alsa_stream->chip->cea_chmap << 24;
 	} else {
-		chmap_value = 0; /* force stereo */
+		/* fallback layouts for applications which do not use chmap API */
+		chmap_value = 0x00;
+		switch (channels) {
+		case 3: chmap_value = 0x01; break;
+		case 4: chmap_value = 0x03; break;
+		case 5: chmap_value = 0x07; break;
+		case 6: chmap_value = 0x0b; break;
+		case 7: chmap_value = 0x0f; break;
+		case 8: chmap_value = 0x13; break;
+		}
 		for (i = 0; i < 8; i++)
 			alsa_stream->chip->map_channels[i] = i;
 	}
