--- a/arch/arm/boot/dts/imx6qdl-gw53xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw53xx.dtsi
@@ -15,6 +15,7 @@
 	/* these are used by bootloader for disabling nodes */
 	aliases {
 		ethernet1 = &eth1;
+		sky2 = &eth1;
 		led0 = &led0;
 		led1 = &led1;
 		led2 = &led2;
--- a/arch/arm/boot/dts/imx6qdl-gw54xx.dtsi
+++ b/arch/arm/boot/dts/imx6qdl-gw54xx.dtsi
@@ -15,6 +15,7 @@
 	/* these are used by bootloader for disabling nodes */
 	aliases {
 		ethernet1 = &eth1;
+		sky2 = &eth1;
 		led0 = &led0;
 		led1 = &led1;
 		led2 = &led2;
