--- a/drivers/net/phy/phy_device.c
+++ b/drivers/net/phy/phy_device.c
@@ -674,6 +674,9 @@ void phy_detach(struct phy_device *phyde
 {
 	int i;
 
+	if (phydev->drv && phydev->drv->detach)
+		phydev->drv->detach(phydev);
+
 	if (phydev->bus->dev.driver)
 		module_put(phydev->bus->dev.driver->owner);
 
--- a/include/linux/phy.h
+++ b/include/linux/phy.h
@@ -507,6 +507,12 @@ struct phy_driver {
 	 */
 	int (*did_interrupt)(struct phy_device *phydev);
 
+	/*
+	 * Called before an ethernet device is detached
+	 * from the PHY.
+	 */
+	void (*detach)(struct phy_device *phydev);
+
 	/* Clears up any memory if needed */
 	void (*remove)(struct phy_device *phydev);
 
