--- a/drivers/mtd/nand/Kconfig
+++ b/drivers/mtd/nand/Kconfig
@@ -546,4 +546,12 @@ config MTD_NAND_HISI504
 	help
 	  Enables support for NAND controller on Hisilicon SoC Hip04.
 
+config MTD_NAND_OXNAS
+	tristate "Support for NAND on Plxtech NAS782X SoC"
+	depends on ARCH_OXNAS
+	select MTD_NAND_PLATFORM
+	help
+	  Enables support for NAND Flash chips on Plxtech NAS782X SoCs. NAND is attached
+	  to the STATIC Unit.
+
 endif # MTD_NAND
--- a/drivers/mtd/nand/Makefile
+++ b/drivers/mtd/nand/Makefile
@@ -46,6 +46,7 @@ obj-$(CONFIG_MTD_NAND_SOCRATES)		+= socr
 obj-$(CONFIG_MTD_NAND_TXX9NDFMC)	+= txx9ndfmc.o
 obj-$(CONFIG_MTD_NAND_NUC900)		+= nuc900_nand.o
 obj-$(CONFIG_MTD_NAND_MPC5121_NFC)	+= mpc5121_nfc.o
+obj-$(CONFIG_MTD_NAND_OXNAS)		+= oxnas_nand.o
 obj-$(CONFIG_MTD_NAND_VF610_NFC)	+= vf610_nfc.o
 obj-$(CONFIG_MTD_NAND_RICOH)		+= r852.o
 obj-$(CONFIG_MTD_NAND_JZ4740)		+= jz4740_nand.o
