From ea1121d3d44b53da76648d498bb1e02185f24198 Mon Sep 17 00:00:00 2001
From: Matthias Reichl <hias@horus.com>
Date: Sun, 11 Oct 2015 15:35:20 +0200
Subject: [PATCH 018/381] bcm2835-i2s: Register PCM device

Code ported from bcm2708-i2s driver in Raspberry Pi tree.

RPi commit ba46b4935a23aa2caac1855ead52a035d4776680 ("ASoC: Add
support for BCM2708")

This driver adds support for digital audio (I2S)
for the BCM2708 SoC that is used by the
Raspberry Pi. External audio codecs can be
connected to the Raspberry Pi via P5 header.

It relies on cyclic DMA engine support for BCM2708.

Signed-off-by: Florian Meier <florian.meier@koalo.de>

Signed-off-by: Matthias Reichl <hias@horus.com>
---
 sound/soc/bcm/bcm2835-i2s.c | 23 ++++++++++++++++++++++-
 1 file changed, 22 insertions(+), 1 deletion(-)

--- a/sound/soc/bcm/bcm2835-i2s.c
+++ b/sound/soc/bcm/bcm2835-i2s.c
@@ -799,6 +799,25 @@ static const struct snd_soc_component_dr
 	.name		= "bcm2835-i2s-comp",
 };
 
+static const struct snd_pcm_hardware bcm2835_pcm_hardware = {
+	.info			= SNDRV_PCM_INFO_INTERLEAVED |
+				  SNDRV_PCM_INFO_JOINT_DUPLEX,
+	.formats		= SNDRV_PCM_FMTBIT_S16_LE |
+				  SNDRV_PCM_FMTBIT_S24_LE |
+				  SNDRV_PCM_FMTBIT_S32_LE,
+	.period_bytes_min	= 32,
+	.period_bytes_max	= 64 * PAGE_SIZE,
+	.periods_min		= 2,
+	.periods_max		= 255,
+	.buffer_bytes_max	= 128 * PAGE_SIZE,
+};
+
+static const struct snd_dmaengine_pcm_config bcm2835_dmaengine_pcm_config = {
+	.prepare_slave_config = snd_dmaengine_pcm_prepare_slave_config,
+	.pcm_hardware = &bcm2835_pcm_hardware,
+	.prealloc_buffer_size = 256 * PAGE_SIZE,
+};
+
 static int bcm2835_i2s_probe(struct platform_device *pdev)
 {
 	struct bcm2835_i2s_dev *dev;
@@ -870,7 +889,9 @@ static int bcm2835_i2s_probe(struct plat
 		return ret;
 	}
 
-	ret = devm_snd_dmaengine_pcm_register(&pdev->dev, NULL, 0);
+	ret = devm_snd_dmaengine_pcm_register(&pdev->dev,
+			&bcm2835_dmaengine_pcm_config,
+			SND_DMAENGINE_PCM_FLAG_COMPAT);
 	if (ret) {
 		dev_err(&pdev->dev, "Could not register PCM: %d\n", ret);
 		return ret;
