From 97799edbda33efb8ebb20785bc7ad76c1b8a0aa9 Mon Sep 17 00:00:00 2001
From: Martin Sperl <kernel@martin.sperl.org>
Date: Mon, 29 Feb 2016 11:39:22 +0000
Subject: [PATCH 259/381] clk: bcm2835: clean up coding style issues

Fix all the checkpatch complaints for clk-bcm2835.c

Signed-off-by: Martin Sperl <kernel@martin.sperl.org>
Signed-off-by: Eric Anholt <eric@anholt.net>
(cherry picked from commit 6e1e60dacee7b32aef1468ea461b02e4c7a90a45)
---
 drivers/clk/bcm/clk-bcm2835.c | 8 ++------
 1 file changed, 2 insertions(+), 6 deletions(-)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -12,9 +12,6 @@
  * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
  * GNU General Public License for more details.
  *
- * You should have received a copy of the GNU General Public License
- * along with this program; if not, write to the Free Software
- * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
  */
 
 /**
@@ -299,7 +296,7 @@
 struct bcm2835_cprman {
 	struct device *dev;
 	void __iomem *regs;
-	spinlock_t regs_lock;
+	spinlock_t regs_lock; /* spinlock for all clocks */
 	const char *osc_name;
 
 	struct clk_onecell_data onecell;
@@ -1344,7 +1341,7 @@ static int bcm2835_clock_set_rate(struct
 }
 
 static int bcm2835_clock_determine_rate(struct clk_hw *hw,
-		struct clk_rate_request *req)
+					struct clk_rate_request *req)
 {
 	struct bcm2835_clock *clock = bcm2835_clock_from_hw(hw);
 	struct clk_hw *parent, *best_parent = NULL;
@@ -1402,7 +1399,6 @@ static u8 bcm2835_clock_get_parent(struc
 	return (src & CM_SRC_MASK) >> CM_SRC_SHIFT;
 }
 
-
 static const struct clk_ops bcm2835_clock_clk_ops = {
 	.is_prepared = bcm2835_clock_is_on,
 	.prepare = bcm2835_clock_on,
