From a369af5149e6eb442b22ce89b564dd7a76e03638 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Tue, 26 Apr 2016 19:05:01 +0200
Subject: [PATCH 072/102] mtd: backport v4.7-0day patches from Boris

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/mtd/Kconfig                 |    4 +-
 drivers/mtd/cmdlinepart.c           |    3 +-
 drivers/mtd/devices/m25p80.c        |   44 +--
 drivers/mtd/maps/physmap_of.c       |    6 +-
 drivers/mtd/mtdchar.c               |  123 ++++++--
 drivers/mtd/mtdconcat.c             |    2 +-
 drivers/mtd/mtdcore.c               |  428 ++++++++++++++++++++++++--
 drivers/mtd/mtdcore.h               |    7 +-
 drivers/mtd/mtdpart.c               |  161 ++++++----
 drivers/mtd/mtdswap.c               |   24 +-
 drivers/mtd/nand/Kconfig            |   21 +-
 drivers/mtd/nand/Makefile           |    2 +
 drivers/mtd/nand/nand_base.c        |  571 +++++++++++++++++++----------------
 drivers/mtd/nand/nand_bbt.c         |   34 +--
 drivers/mtd/nand/nand_bch.c         |   52 ++--
 drivers/mtd/nand/nand_ecc.c         |    6 +-
 drivers/mtd/nand/nand_ids.c         |    4 +-
 drivers/mtd/nand/nandsim.c          |   43 +--
 drivers/mtd/ofpart.c                |   53 ++--
 drivers/mtd/spi-nor/Kconfig         |   10 +-
 drivers/mtd/spi-nor/Makefile        |    1 +
 drivers/mtd/spi-nor/mtk-quadspi.c   |  485 +++++++++++++++++++++++++++++
 drivers/mtd/spi-nor/spi-nor.c       |  321 +++++++++++++-------
 drivers/mtd/tests/mtd_nandecctest.c |    2 +-
 drivers/mtd/tests/oobtest.c         |   49 ++-
 drivers/mtd/tests/pagetest.c        |    3 +-
 include/linux/mtd/bbm.h             |    1 -
 include/linux/mtd/fsmc.h            |   18 --
 include/linux/mtd/inftl.h           |    1 -
 include/linux/mtd/map.h             |    9 +-
 include/linux/mtd/mtd.h             |   80 ++++-
 include/linux/mtd/nand.h            |   94 ++++--
 include/linux/mtd/nand_bch.h        |   10 +-
 include/linux/mtd/nftl.h            |    1 -
 include/linux/mtd/onenand.h         |    2 -
 include/linux/mtd/partitions.h      |   27 +-
 include/linux/mtd/sh_flctl.h        |    4 +-
 include/linux/mtd/sharpsl.h         |    2 +-
 include/linux/mtd/spi-nor.h         |   23 +-
 include/uapi/mtd/mtd-abi.h          |    2 +-
 45 files changed, 2077 insertions(+), 748 deletions(-)
 create mode 100644 drivers/mtd/spi-nor/mtk-quadspi.c

--- a/drivers/mtd/Kconfig
+++ b/drivers/mtd/Kconfig
@@ -131,7 +131,7 @@ config MTD_CMDLINE_PARTS
 
 config MTD_AFS_PARTS
 	tristate "ARM Firmware Suite partition parsing"
-	depends on ARM
+	depends on (ARM || ARM64)
 	---help---
 	  The ARM Firmware Suite allows the user to divide flash devices into
 	  multiple 'images'. Each such image has a header containing its name
@@ -161,7 +161,7 @@ config MTD_AR7_PARTS
 
 config MTD_BCM63XX_PARTS
 	tristate "BCM63XX CFE partitioning support"
-	depends on BCM63XX
+	depends on BCM63XX || BMIPS_GENERIC || COMPILE_TEST
 	select CRC32
 	help
 	  This provides partions parsing for BCM63xx devices with CFE
--- a/drivers/mtd/cmdlinepart.c
+++ b/drivers/mtd/cmdlinepart.c
@@ -304,7 +304,7 @@ static int mtdpart_setup_real(char *s)
  * the first one in the chain if a NULL mtd_id is passed in.
  */
 static int parse_cmdline_partitions(struct mtd_info *master,
-				    struct mtd_partition **pparts,
+				    const struct mtd_partition **pparts,
 				    struct mtd_part_parser_data *data)
 {
 	unsigned long long offset;
@@ -382,7 +382,6 @@ static int __init mtdpart_setup(char *s)
 __setup("mtdparts=", mtdpart_setup);
 
 static struct mtd_part_parser cmdline_parser = {
-	.owner = THIS_MODULE,
 	.parse_fn = parse_cmdline_partitions,
 	.name = "cmdlinepart",
 };
--- a/drivers/mtd/devices/m25p80.c
+++ b/drivers/mtd/devices/m25p80.c
@@ -174,22 +174,6 @@ static int m25p80_read(struct spi_nor *n
 	return 0;
 }
 
-static int m25p80_erase(struct spi_nor *nor, loff_t offset)
-{
-	struct m25p *flash = nor->priv;
-
-	dev_dbg(nor->dev, "%dKiB at 0x%08x\n",
-		flash->spi_nor.mtd.erasesize / 1024, (u32)offset);
-
-	/* Set up command buffer. */
-	flash->command[0] = nor->erase_opcode;
-	m25p_addr2cmd(nor, offset, flash->command);
-
-	spi_write(flash->spi, flash->command, m25p_cmdsz(nor));
-
-	return 0;
-}
-
 /*
  * board specific setup should have ensured the SPI clock used here
  * matches what the READ command supports, at least until this driver
@@ -197,12 +181,11 @@ static int m25p80_erase(struct spi_nor *
  */
 static int m25p_probe(struct spi_device *spi)
 {
-	struct mtd_part_parser_data	ppdata;
 	struct flash_platform_data	*data;
 	struct m25p *flash;
 	struct spi_nor *nor;
 	enum read_mode mode = SPI_NOR_NORMAL;
-	char *flash_name = NULL;
+	char *flash_name;
 	int ret;
 
 	data = dev_get_platdata(&spi->dev);
@@ -216,12 +199,11 @@ static int m25p_probe(struct spi_device
 	/* install the hooks */
 	nor->read = m25p80_read;
 	nor->write = m25p80_write;
-	nor->erase = m25p80_erase;
 	nor->write_reg = m25p80_write_reg;
 	nor->read_reg = m25p80_read_reg;
 
 	nor->dev = &spi->dev;
-	nor->flash_node = spi->dev.of_node;
+	spi_nor_set_flash_node(nor, spi->dev.of_node);
 	nor->priv = flash;
 
 	spi_set_drvdata(spi, flash);
@@ -242,6 +224,8 @@ static int m25p_probe(struct spi_device
 	 */
 	if (data && data->type)
 		flash_name = data->type;
+	else if (!strcmp(spi->modalias, "spi-nor"))
+		flash_name = NULL; /* auto-detect */
 	else
 		flash_name = spi->modalias;
 
@@ -249,11 +233,8 @@ static int m25p_probe(struct spi_device
 	if (ret)
 		return ret;
 
-	ppdata.of_node = spi->dev.of_node;
-
-	return mtd_device_parse_register(&nor->mtd, NULL, &ppdata,
-			data ? data->parts : NULL,
-			data ? data->nr_parts : 0);
+	return mtd_device_register(&nor->mtd, data ? data->parts : NULL,
+				   data ? data->nr_parts : 0);
 }
 
 
@@ -279,14 +260,21 @@ static int m25p_remove(struct spi_device
  */
 static const struct spi_device_id m25p_ids[] = {
 	/*
+	 * Allow non-DT platform devices to bind to the "spi-nor" modalias, and
+	 * hack around the fact that the SPI core does not provide uevent
+	 * matching for .of_match_table
+	 */
+	{"spi-nor"},
+
+	/*
 	 * Entries not used in DTs that should be safe to drop after replacing
-	 * them with "nor-jedec" in platform data.
+	 * them with "spi-nor" in platform data.
 	 */
 	{"s25sl064a"},	{"w25x16"},	{"m25p10"},	{"m25px64"},
 
 	/*
-	 * Entries that were used in DTs without "nor-jedec" fallback and should
-	 * be kept for backward compatibility.
+	 * Entries that were used in DTs without "jedec,spi-nor" fallback and
+	 * should be kept for backward compatibility.
 	 */
 	{"at25df321a"},	{"at25df641"},	{"at26df081a"},
 	{"mr25h256"},
--- a/drivers/mtd/maps/physmap_of.c
+++ b/drivers/mtd/maps/physmap_of.c
@@ -128,7 +128,6 @@ static int of_flash_probe(struct platfor
 	int reg_tuple_size;
 	struct mtd_info **mtd_list = NULL;
 	resource_size_t res_size;
-	struct mtd_part_parser_data ppdata;
 	bool map_indirect;
 	const char *mtd_name = NULL;
 
@@ -272,8 +271,9 @@ static int of_flash_probe(struct platfor
 	if (err)
 		goto err_out;
 
-	ppdata.of_node = dp;
-	mtd_device_parse_register(info->cmtd, part_probe_types_def, &ppdata,
+	info->cmtd->dev.parent = &dev->dev;
+	mtd_set_of_node(info->cmtd, dp);
+	mtd_device_parse_register(info->cmtd, part_probe_types_def, NULL,
 			NULL, 0);
 
 	kfree(mtd_list);
--- a/drivers/mtd/mtdchar.c
+++ b/drivers/mtd/mtdchar.c
@@ -465,38 +465,111 @@ static int mtdchar_readoob(struct file *
 }
 
 /*
- * Copies (and truncates, if necessary) data from the larger struct,
- * nand_ecclayout, to the smaller, deprecated layout struct,
- * nand_ecclayout_user. This is necessary only to support the deprecated
- * API ioctl ECCGETLAYOUT while allowing all new functionality to use
- * nand_ecclayout flexibly (i.e. the struct may change size in new
- * releases without requiring major rewrites).
+ * Copies (and truncates, if necessary) OOB layout information to the
+ * deprecated layout struct, nand_ecclayout_user. This is necessary only to
+ * support the deprecated API ioctl ECCGETLAYOUT while allowing all new
+ * functionality to use mtd_ooblayout_ops flexibly (i.e. mtd_ooblayout_ops
+ * can describe any kind of OOB layout with almost zero overhead from a
+ * memory usage point of view).
  */
-static int shrink_ecclayout(const struct nand_ecclayout *from,
-		struct nand_ecclayout_user *to)
+static int shrink_ecclayout(struct mtd_info *mtd,
+			    struct nand_ecclayout_user *to)
 {
-	int i;
+	struct mtd_oob_region oobregion;
+	int i, section = 0, ret;
 
-	if (!from || !to)
+	if (!mtd || !to)
 		return -EINVAL;
 
 	memset(to, 0, sizeof(*to));
 
-	to->eccbytes = min((int)from->eccbytes, MTD_MAX_ECCPOS_ENTRIES);
-	for (i = 0; i < to->eccbytes; i++)
-		to->eccpos[i] = from->eccpos[i];
+	to->eccbytes = 0;
+	for (i = 0; i < MTD_MAX_ECCPOS_ENTRIES;) {
+		u32 eccpos;
+
+		ret = mtd_ooblayout_ecc(mtd, section, &oobregion);
+		if (ret < 0) {
+			if (ret != -ERANGE)
+				return ret;
+
+			break;
+		}
+
+		eccpos = oobregion.offset;
+		for (; i < MTD_MAX_ECCPOS_ENTRIES &&
+		       eccpos < oobregion.offset + oobregion.length; i++) {
+			to->eccpos[i] = eccpos++;
+			to->eccbytes++;
+		}
+	}
 
 	for (i = 0; i < MTD_MAX_OOBFREE_ENTRIES; i++) {
-		if (from->oobfree[i].length == 0 &&
-				from->oobfree[i].offset == 0)
+		ret = mtd_ooblayout_free(mtd, i, &oobregion);
+		if (ret < 0) {
+			if (ret != -ERANGE)
+				return ret;
+
 			break;
-		to->oobavail += from->oobfree[i].length;
-		to->oobfree[i] = from->oobfree[i];
+		}
+
+		to->oobfree[i].offset = oobregion.offset;
+		to->oobfree[i].length = oobregion.length;
+		to->oobavail += to->oobfree[i].length;
 	}
 
 	return 0;
 }
 
+static int get_oobinfo(struct mtd_info *mtd, struct nand_oobinfo *to)
+{
+	struct mtd_oob_region oobregion;
+	int i, section = 0, ret;
+
+	if (!mtd || !to)
+		return -EINVAL;
+
+	memset(to, 0, sizeof(*to));
+
+	to->eccbytes = 0;
+	for (i = 0; i < ARRAY_SIZE(to->eccpos);) {
+		u32 eccpos;
+
+		ret = mtd_ooblayout_ecc(mtd, section, &oobregion);
+		if (ret < 0) {
+			if (ret != -ERANGE)
+				return ret;
+
+			break;
+		}
+
+		if (oobregion.length + i > ARRAY_SIZE(to->eccpos))
+			return -EINVAL;
+
+		eccpos = oobregion.offset;
+		for (; eccpos < oobregion.offset + oobregion.length; i++) {
+			to->eccpos[i] = eccpos++;
+			to->eccbytes++;
+		}
+	}
+
+	for (i = 0; i < 8; i++) {
+		ret = mtd_ooblayout_free(mtd, i, &oobregion);
+		if (ret < 0) {
+			if (ret != -ERANGE)
+				return ret;
+
+			break;
+		}
+
+		to->oobfree[i][0] = oobregion.offset;
+		to->oobfree[i][1] = oobregion.length;
+	}
+
+	to->useecc = MTD_NANDECC_AUTOPLACE;
+
+	return 0;
+}
+
 static int mtdchar_blkpg_ioctl(struct mtd_info *mtd,
 			       struct blkpg_ioctl_arg *arg)
 {
@@ -815,16 +888,12 @@ static int mtdchar_ioctl(struct file *fi
 	{
 		struct nand_oobinfo oi;
 
-		if (!mtd->ecclayout)
+		if (!mtd->ooblayout)
 			return -EOPNOTSUPP;
-		if (mtd->ecclayout->eccbytes > ARRAY_SIZE(oi.eccpos))
-			return -EINVAL;
 
-		oi.useecc = MTD_NANDECC_AUTOPLACE;
-		memcpy(&oi.eccpos, mtd->ecclayout->eccpos, sizeof(oi.eccpos));
-		memcpy(&oi.oobfree, mtd->ecclayout->oobfree,
-		       sizeof(oi.oobfree));
-		oi.eccbytes = mtd->ecclayout->eccbytes;
+		ret = get_oobinfo(mtd, &oi);
+		if (ret)
+			return ret;
 
 		if (copy_to_user(argp, &oi, sizeof(struct nand_oobinfo)))
 			return -EFAULT;
@@ -913,14 +982,14 @@ static int mtdchar_ioctl(struct file *fi
 	{
 		struct nand_ecclayout_user *usrlay;
 
-		if (!mtd->ecclayout)
+		if (!mtd->ooblayout)
 			return -EOPNOTSUPP;
 
 		usrlay = kmalloc(sizeof(*usrlay), GFP_KERNEL);
 		if (!usrlay)
 			return -ENOMEM;
 
-		shrink_ecclayout(mtd->ecclayout, usrlay);
+		shrink_ecclayout(mtd, usrlay);
 
 		if (copy_to_user(argp, usrlay, sizeof(*usrlay)))
 			ret = -EFAULT;
--- a/drivers/mtd/mtdconcat.c
+++ b/drivers/mtd/mtdconcat.c
@@ -777,7 +777,7 @@ struct mtd_info *mtd_concat_create(struc
 
 	}
 
-	concat->mtd.ecclayout = subdev[0]->ecclayout;
+	mtd_set_ooblayout(&concat->mtd, subdev[0]->ooblayout);
 
 	concat->num_subdev = num_devs;
 	concat->mtd.name = name;
--- a/drivers/mtd/mtdcore.c
+++ b/drivers/mtd/mtdcore.c
@@ -32,6 +32,7 @@
 #include <linux/err.h>
 #include <linux/ioctl.h>
 #include <linux/init.h>
+#include <linux/of.h>
 #include <linux/proc_fs.h>
 #include <linux/idr.h>
 #include <linux/backing-dev.h>
@@ -446,6 +447,7 @@ int add_mtd_device(struct mtd_info *mtd)
 	mtd->dev.devt = MTD_DEVT(i);
 	dev_set_name(&mtd->dev, "mtd%d", i);
 	dev_set_drvdata(&mtd->dev, mtd);
+	of_node_get(mtd_get_of_node(mtd));
 	error = device_register(&mtd->dev);
 	if (error)
 		goto fail_added;
@@ -477,6 +479,7 @@ int add_mtd_device(struct mtd_info *mtd)
 	return 0;
 
 fail_added:
+	of_node_put(mtd_get_of_node(mtd));
 	idr_remove(&mtd_idr, i);
 fail_locked:
 	mutex_unlock(&mtd_table_mutex);
@@ -518,6 +521,7 @@ int del_mtd_device(struct mtd_info *mtd)
 		device_unregister(&mtd->dev);
 
 		idr_remove(&mtd_idr, mtd->index);
+		of_node_put(mtd_get_of_node(mtd));
 
 		module_put(THIS_MODULE);
 		ret = 0;
@@ -529,9 +533,10 @@ out_error:
 }
 
 static int mtd_add_device_partitions(struct mtd_info *mtd,
-				     struct mtd_partition *real_parts,
-				     int nbparts)
+				     struct mtd_partitions *parts)
 {
+	const struct mtd_partition *real_parts = parts->parts;
+	int nbparts = parts->nr_parts;
 	int ret;
 
 	if (nbparts == 0 || IS_ENABLED(CONFIG_MTD_PARTITIONED_MASTER)) {
@@ -600,29 +605,29 @@ int mtd_device_parse_register(struct mtd
 			      const struct mtd_partition *parts,
 			      int nr_parts)
 {
+	struct mtd_partitions parsed;
 	int ret;
-	struct mtd_partition *real_parts = NULL;
 
 	mtd_set_dev_defaults(mtd);
 
-	ret = parse_mtd_partitions(mtd, types, &real_parts, parser_data);
-	if (ret <= 0 && nr_parts && parts) {
-		real_parts = kmemdup(parts, sizeof(*parts) * nr_parts,
-				     GFP_KERNEL);
-		if (!real_parts)
-			ret = -ENOMEM;
-		else
-			ret = nr_parts;
-	}
-	/* Didn't come up with either parsed OR fallback partitions */
-	if (ret < 0) {
-		pr_info("mtd: failed to find partitions; one or more parsers reports errors (%d)\n",
+	memset(&parsed, 0, sizeof(parsed));
+
+	ret = parse_mtd_partitions(mtd, types, &parsed, parser_data);
+	if ((ret < 0 || parsed.nr_parts == 0) && parts && nr_parts) {
+		/* Fall back to driver-provided partitions */
+		parsed = (struct mtd_partitions){
+			.parts		= parts,
+			.nr_parts	= nr_parts,
+		};
+	} else if (ret < 0) {
+		/* Didn't come up with parsed OR fallback partitions */
+			pr_info("mtd: failed to find partitions; one or more parsers reports errors (%d)\n",
 			ret);
 		/* Don't abort on errors; we can still use unpartitioned MTD */
-		ret = 0;
+		memset(&parsed, 0, sizeof(parsed));
 	}
 
-	ret = mtd_add_device_partitions(mtd, real_parts, ret);
+	ret = mtd_add_device_partitions(mtd, &parsed);
 	if (ret)
 		goto out;
 
@@ -642,7 +647,8 @@ int mtd_device_parse_register(struct mtd
 	}
 
 out:
-	kfree(real_parts);
+	/* Cleanup any parsed partitions */
+	mtd_part_parser_cleanup(&parsed);
 	return ret;
 }
 EXPORT_SYMBOL_GPL(mtd_device_parse_register);
@@ -767,7 +773,6 @@ out:
 }
 EXPORT_SYMBOL_GPL(get_mtd_device);
 
-
 int __get_mtd_device(struct mtd_info *mtd)
 {
 	int err;
@@ -1001,6 +1006,366 @@ int mtd_read_oob(struct mtd_info *mtd, l
 }
 EXPORT_SYMBOL_GPL(mtd_read_oob);
 
+/**
+ * mtd_ooblayout_ecc - Get the OOB region definition of a specific ECC section
+ * @mtd: MTD device structure
+ * @section: ECC section. Depending on the layout you may have all the ECC
+ *	     bytes stored in a single contiguous section, or one section
+ *	     per ECC chunk (and sometime several sections for a single ECC
+ *	     ECC chunk)
+ * @oobecc: OOB region struct filled with the appropriate ECC position
+ *	    information
+ *
+ * This functions return ECC section information in the OOB area. I you want
+ * to get all the ECC bytes information, then you should call
+ * mtd_ooblayout_ecc(mtd, section++, oobecc) until it returns -ERANGE.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_ecc(struct mtd_info *mtd, int section,
+		      struct mtd_oob_region *oobecc)
+{
+	memset(oobecc, 0, sizeof(*oobecc));
+
+	if (!mtd || section < 0)
+		return -EINVAL;
+
+	if (!mtd->ooblayout || !mtd->ooblayout->ecc)
+		return -ENOTSUPP;
+
+	return mtd->ooblayout->ecc(mtd, section, oobecc);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_ecc);
+
+/**
+ * mtd_ooblayout_free - Get the OOB region definition of a specific free
+ *			section
+ * @mtd: MTD device structure
+ * @section: Free section you are interested in. Depending on the layout
+ *	     you may have all the free bytes stored in a single contiguous
+ *	     section, or one section per ECC chunk plus an extra section
+ *	     for the remaining bytes (or other funky layout).
+ * @oobfree: OOB region struct filled with the appropriate free position
+ *	     information
+ *
+ * This functions return free bytes position in the OOB area. I you want
+ * to get all the free bytes information, then you should call
+ * mtd_ooblayout_free(mtd, section++, oobfree) until it returns -ERANGE.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_free(struct mtd_info *mtd, int section,
+		       struct mtd_oob_region *oobfree)
+{
+	memset(oobfree, 0, sizeof(*oobfree));
+
+	if (!mtd || section < 0)
+		return -EINVAL;
+
+	if (!mtd->ooblayout || !mtd->ooblayout->free)
+		return -ENOTSUPP;
+
+	return mtd->ooblayout->free(mtd, section, oobfree);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_free);
+
+/**
+ * mtd_ooblayout_find_region - Find the region attached to a specific byte
+ * @mtd: mtd info structure
+ * @byte: the byte we are searching for
+ * @sectionp: pointer where the section id will be stored
+ * @oobregion: used to retrieve the ECC position
+ * @iter: iterator function. Should be either mtd_ooblayout_free or
+ *	  mtd_ooblayout_ecc depending on the region type you're searching for
+ *
+ * This functions returns the section id and oobregion information of a
+ * specific byte. For example, say you want to know where the 4th ECC byte is
+ * stored, you'll use:
+ *
+ * mtd_ooblayout_find_region(mtd, 3, &section, &oobregion, mtd_ooblayout_ecc);
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+static int mtd_ooblayout_find_region(struct mtd_info *mtd, int byte,
+				int *sectionp, struct mtd_oob_region *oobregion,
+				int (*iter)(struct mtd_info *,
+					    int section,
+					    struct mtd_oob_region *oobregion))
+{
+	int pos = 0, ret, section = 0;
+
+	memset(oobregion, 0, sizeof(*oobregion));
+
+	while (1) {
+		ret = iter(mtd, section, oobregion);
+		if (ret)
+			return ret;
+
+		if (pos + oobregion->length > byte)
+			break;
+
+		pos += oobregion->length;
+		section++;
+	}
+
+	/*
+	 * Adjust region info to make it start at the beginning at the
+	 * 'start' ECC byte.
+	 */
+	oobregion->offset += byte - pos;
+	oobregion->length -= byte - pos;
+	*sectionp = section;
+
+	return 0;
+}
+
+/**
+ * mtd_ooblayout_find_eccregion - Find the ECC region attached to a specific
+ *				  ECC byte
+ * @mtd: mtd info structure
+ * @eccbyte: the byte we are searching for
+ * @sectionp: pointer where the section id will be stored
+ * @oobregion: OOB region information
+ *
+ * Works like mtd_ooblayout_find_region() except it searches for a specific ECC
+ * byte.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_find_eccregion(struct mtd_info *mtd, int eccbyte,
+				 int *section,
+				 struct mtd_oob_region *oobregion)
+{
+	return mtd_ooblayout_find_region(mtd, eccbyte, section, oobregion,
+					 mtd_ooblayout_ecc);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_find_eccregion);
+
+/**
+ * mtd_ooblayout_get_bytes - Extract OOB bytes from the oob buffer
+ * @mtd: mtd info structure
+ * @buf: destination buffer to store OOB bytes
+ * @oobbuf: OOB buffer
+ * @start: first byte to retrieve
+ * @nbytes: number of bytes to retrieve
+ * @iter: section iterator
+ *
+ * Extract bytes attached to a specific category (ECC or free)
+ * from the OOB buffer and copy them into buf.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+static int mtd_ooblayout_get_bytes(struct mtd_info *mtd, u8 *buf,
+				const u8 *oobbuf, int start, int nbytes,
+				int (*iter)(struct mtd_info *,
+					    int section,
+					    struct mtd_oob_region *oobregion))
+{
+	struct mtd_oob_region oobregion = { };
+	int section = 0, ret;
+
+	ret = mtd_ooblayout_find_region(mtd, start, &section,
+					&oobregion, iter);
+
+	while (!ret) {
+		int cnt;
+
+		cnt = oobregion.length > nbytes ? nbytes : oobregion.length;
+		memcpy(buf, oobbuf + oobregion.offset, cnt);
+		buf += cnt;
+		nbytes -= cnt;
+
+		if (!nbytes)
+			break;
+
+		ret = iter(mtd, ++section, &oobregion);
+	}
+
+	return ret;
+}
+
+/**
+ * mtd_ooblayout_set_bytes - put OOB bytes into the oob buffer
+ * @mtd: mtd info structure
+ * @buf: source buffer to get OOB bytes from
+ * @oobbuf: OOB buffer
+ * @start: first OOB byte to set
+ * @nbytes: number of OOB bytes to set
+ * @iter: section iterator
+ *
+ * Fill the OOB buffer with data provided in buf. The category (ECC or free)
+ * is selected by passing the appropriate iterator.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+static int mtd_ooblayout_set_bytes(struct mtd_info *mtd, const u8 *buf,
+				u8 *oobbuf, int start, int nbytes,
+				int (*iter)(struct mtd_info *,
+					    int section,
+					    struct mtd_oob_region *oobregion))
+{
+	struct mtd_oob_region oobregion = { };
+	int section = 0, ret;
+
+	ret = mtd_ooblayout_find_region(mtd, start, &section,
+					&oobregion, iter);
+
+	while (!ret) {
+		int cnt;
+
+		cnt = oobregion.length > nbytes ? nbytes : oobregion.length;
+		memcpy(oobbuf + oobregion.offset, buf, cnt);
+		buf += cnt;
+		nbytes -= cnt;
+
+		if (!nbytes)
+			break;
+
+		ret = iter(mtd, ++section, &oobregion);
+	}
+
+	return ret;
+}
+
+/**
+ * mtd_ooblayout_count_bytes - count the number of bytes in a OOB category
+ * @mtd: mtd info structure
+ * @iter: category iterator
+ *
+ * Count the number of bytes in a given category.
+ *
+ * Returns a positive value on success, a negative error code otherwise.
+ */
+static int mtd_ooblayout_count_bytes(struct mtd_info *mtd,
+				int (*iter)(struct mtd_info *,
+					    int section,
+					    struct mtd_oob_region *oobregion))
+{
+	struct mtd_oob_region oobregion = { };
+	int section = 0, ret, nbytes = 0;
+
+	while (1) {
+		ret = iter(mtd, section++, &oobregion);
+		if (ret) {
+			if (ret == -ERANGE)
+				ret = nbytes;
+			break;
+		}
+
+		nbytes += oobregion.length;
+	}
+
+	return ret;
+}
+
+/**
+ * mtd_ooblayout_get_eccbytes - extract ECC bytes from the oob buffer
+ * @mtd: mtd info structure
+ * @eccbuf: destination buffer to store ECC bytes
+ * @oobbuf: OOB buffer
+ * @start: first ECC byte to retrieve
+ * @nbytes: number of ECC bytes to retrieve
+ *
+ * Works like mtd_ooblayout_get_bytes(), except it acts on ECC bytes.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_get_eccbytes(struct mtd_info *mtd, u8 *eccbuf,
+			       const u8 *oobbuf, int start, int nbytes)
+{
+	return mtd_ooblayout_get_bytes(mtd, eccbuf, oobbuf, start, nbytes,
+				       mtd_ooblayout_ecc);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_get_eccbytes);
+
+/**
+ * mtd_ooblayout_set_eccbytes - set ECC bytes into the oob buffer
+ * @mtd: mtd info structure
+ * @eccbuf: source buffer to get ECC bytes from
+ * @oobbuf: OOB buffer
+ * @start: first ECC byte to set
+ * @nbytes: number of ECC bytes to set
+ *
+ * Works like mtd_ooblayout_set_bytes(), except it acts on ECC bytes.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_set_eccbytes(struct mtd_info *mtd, const u8 *eccbuf,
+			       u8 *oobbuf, int start, int nbytes)
+{
+	return mtd_ooblayout_set_bytes(mtd, eccbuf, oobbuf, start, nbytes,
+				       mtd_ooblayout_ecc);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_set_eccbytes);
+
+/**
+ * mtd_ooblayout_get_databytes - extract data bytes from the oob buffer
+ * @mtd: mtd info structure
+ * @databuf: destination buffer to store ECC bytes
+ * @oobbuf: OOB buffer
+ * @start: first ECC byte to retrieve
+ * @nbytes: number of ECC bytes to retrieve
+ *
+ * Works like mtd_ooblayout_get_bytes(), except it acts on free bytes.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_get_databytes(struct mtd_info *mtd, u8 *databuf,
+				const u8 *oobbuf, int start, int nbytes)
+{
+	return mtd_ooblayout_get_bytes(mtd, databuf, oobbuf, start, nbytes,
+				       mtd_ooblayout_free);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_get_databytes);
+
+/**
+ * mtd_ooblayout_get_eccbytes - set data bytes into the oob buffer
+ * @mtd: mtd info structure
+ * @eccbuf: source buffer to get data bytes from
+ * @oobbuf: OOB buffer
+ * @start: first ECC byte to set
+ * @nbytes: number of ECC bytes to set
+ *
+ * Works like mtd_ooblayout_get_bytes(), except it acts on free bytes.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_set_databytes(struct mtd_info *mtd, const u8 *databuf,
+				u8 *oobbuf, int start, int nbytes)
+{
+	return mtd_ooblayout_set_bytes(mtd, databuf, oobbuf, start, nbytes,
+				       mtd_ooblayout_free);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_set_databytes);
+
+/**
+ * mtd_ooblayout_count_freebytes - count the number of free bytes in OOB
+ * @mtd: mtd info structure
+ *
+ * Works like mtd_ooblayout_count_bytes(), except it count free bytes.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_count_freebytes(struct mtd_info *mtd)
+{
+	return mtd_ooblayout_count_bytes(mtd, mtd_ooblayout_free);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_count_freebytes);
+
+/**
+ * mtd_ooblayout_count_freebytes - count the number of ECC bytes in OOB
+ * @mtd: mtd info structure
+ *
+ * Works like mtd_ooblayout_count_bytes(), except it count ECC bytes.
+ *
+ * Returns zero on success, a negative error code otherwise.
+ */
+int mtd_ooblayout_count_eccbytes(struct mtd_info *mtd)
+{
+	return mtd_ooblayout_count_bytes(mtd, mtd_ooblayout_ecc);
+}
+EXPORT_SYMBOL_GPL(mtd_ooblayout_count_eccbytes);
+
 /*
  * Method to access the protection register area, present in some flash
  * devices. The user data is one time programmable but the factory data is read
--- a/drivers/mtd/mtdcore.h
+++ b/drivers/mtd/mtdcore.h
@@ -10,10 +10,15 @@ int add_mtd_device(struct mtd_info *mtd)
 int del_mtd_device(struct mtd_info *mtd);
 int add_mtd_partitions(struct mtd_info *, const struct mtd_partition *, int);
 int del_mtd_partitions(struct mtd_info *);
+
+struct mtd_partitions;
+
 int parse_mtd_partitions(struct mtd_info *master, const char * const *types,
-			 struct mtd_partition **pparts,
+			 struct mtd_partitions *pparts,
 			 struct mtd_part_parser_data *data);
 
+void mtd_part_parser_cleanup(struct mtd_partitions *parts);
+
 int __init init_mtdchar(void);
 void __exit cleanup_mtdchar(void);
 
--- a/drivers/mtd/mtdpart.c
+++ b/drivers/mtd/mtdpart.c
@@ -55,9 +55,12 @@ static void mtd_partition_split(struct m
 
 /*
  * Given a pointer to the MTD object in the mtd_part structure, we can retrieve
- * the pointer to that structure with this macro.
+ * the pointer to that structure.
  */
-#define PART(x)  ((struct mtd_part *)(x))
+static inline struct mtd_part *mtd_to_part(const struct mtd_info *mtd)
+{
+	return container_of(mtd, struct mtd_part, mtd);
+}
 
 
 /*
@@ -68,7 +71,7 @@ static void mtd_partition_split(struct m
 static int part_read(struct mtd_info *mtd, loff_t from, size_t len,
 		size_t *retlen, u_char *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	struct mtd_ecc_stats stats;
 	int res;
 
@@ -87,7 +90,7 @@ static int part_read(struct mtd_info *mt
 static int part_point(struct mtd_info *mtd, loff_t from, size_t len,
 		size_t *retlen, void **virt, resource_size_t *phys)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 
 	return part->master->_point(part->master, from + part->offset, len,
 				    retlen, virt, phys);
@@ -95,7 +98,7 @@ static int part_point(struct mtd_info *m
 
 static int part_unpoint(struct mtd_info *mtd, loff_t from, size_t len)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 
 	return part->master->_unpoint(part->master, from + part->offset, len);
 }
@@ -105,7 +108,7 @@ static unsigned long part_get_unmapped_a
 					    unsigned long offset,
 					    unsigned long flags)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 
 	offset += part->offset;
 	return part->master->_get_unmapped_area(part->master, len, offset,
@@ -115,7 +118,7 @@ static unsigned long part_get_unmapped_a
 static int part_read_oob(struct mtd_info *mtd, loff_t from,
 		struct mtd_oob_ops *ops)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	int res;
 
 	if (from >= mtd->size)
@@ -130,10 +133,7 @@ static int part_read_oob(struct mtd_info
 	if (ops->oobbuf) {
 		size_t len, pages;
 
-		if (ops->mode == MTD_OPS_AUTO_OOB)
-			len = mtd->oobavail;
-		else
-			len = mtd->oobsize;
+		len = mtd_oobavail(mtd, ops);
 		pages = mtd_div_by_ws(mtd->size, mtd);
 		pages -= mtd_div_by_ws(from, mtd);
 		if (ops->ooboffs + ops->ooblen > pages * len)
@@ -153,7 +153,7 @@ static int part_read_oob(struct mtd_info
 static int part_read_user_prot_reg(struct mtd_info *mtd, loff_t from,
 		size_t len, size_t *retlen, u_char *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_read_user_prot_reg(part->master, from, len,
 						 retlen, buf);
 }
@@ -161,7 +161,7 @@ static int part_read_user_prot_reg(struc
 static int part_get_user_prot_info(struct mtd_info *mtd, size_t len,
 				   size_t *retlen, struct otp_info *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_get_user_prot_info(part->master, len, retlen,
 						 buf);
 }
@@ -169,7 +169,7 @@ static int part_get_user_prot_info(struc
 static int part_read_fact_prot_reg(struct mtd_info *mtd, loff_t from,
 		size_t len, size_t *retlen, u_char *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_read_fact_prot_reg(part->master, from, len,
 						 retlen, buf);
 }
@@ -177,7 +177,7 @@ static int part_read_fact_prot_reg(struc
 static int part_get_fact_prot_info(struct mtd_info *mtd, size_t len,
 				   size_t *retlen, struct otp_info *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_get_fact_prot_info(part->master, len, retlen,
 						 buf);
 }
@@ -185,7 +185,7 @@ static int part_get_fact_prot_info(struc
 static int part_write(struct mtd_info *mtd, loff_t to, size_t len,
 		size_t *retlen, const u_char *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_write(part->master, to + part->offset, len,
 				    retlen, buf);
 }
@@ -193,7 +193,7 @@ static int part_write(struct mtd_info *m
 static int part_panic_write(struct mtd_info *mtd, loff_t to, size_t len,
 		size_t *retlen, const u_char *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_panic_write(part->master, to + part->offset, len,
 					  retlen, buf);
 }
@@ -201,7 +201,7 @@ static int part_panic_write(struct mtd_i
 static int part_write_oob(struct mtd_info *mtd, loff_t to,
 		struct mtd_oob_ops *ops)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 
 	if (to >= mtd->size)
 		return -EINVAL;
@@ -213,7 +213,7 @@ static int part_write_oob(struct mtd_inf
 static int part_write_user_prot_reg(struct mtd_info *mtd, loff_t from,
 		size_t len, size_t *retlen, u_char *buf)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_write_user_prot_reg(part->master, from, len,
 						  retlen, buf);
 }
@@ -221,21 +221,21 @@ static int part_write_user_prot_reg(stru
 static int part_lock_user_prot_reg(struct mtd_info *mtd, loff_t from,
 		size_t len)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_lock_user_prot_reg(part->master, from, len);
 }
 
 static int part_writev(struct mtd_info *mtd, const struct kvec *vecs,
 		unsigned long count, loff_t to, size_t *retlen)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_writev(part->master, vecs, count,
 				     to + part->offset, retlen);
 }
 
 static int part_erase(struct mtd_info *mtd, struct erase_info *instr)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	int ret;
 
 
@@ -299,7 +299,7 @@ static int part_erase(struct mtd_info *m
 void mtd_erase_callback(struct erase_info *instr)
 {
 	if (instr->mtd->_erase == part_erase) {
-		struct mtd_part *part = PART(instr->mtd);
+		struct mtd_part *part = mtd_to_part(instr->mtd);
 		size_t wrlen = 0;
 
 		if (instr->mtd->flags & MTD_ERASE_PARTIAL) {
@@ -330,13 +330,13 @@ EXPORT_SYMBOL_GPL(mtd_erase_callback);
 
 static int part_lock(struct mtd_info *mtd, loff_t ofs, uint64_t len)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_lock(part->master, ofs + part->offset, len);
 }
 
 static int part_unlock(struct mtd_info *mtd, loff_t ofs, uint64_t len)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 
 	ofs += part->offset;
 	if (mtd->flags & MTD_ERASE_PARTIAL) {
@@ -349,45 +349,45 @@ static int part_unlock(struct mtd_info *
 
 static int part_is_locked(struct mtd_info *mtd, loff_t ofs, uint64_t len)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_is_locked(part->master, ofs + part->offset, len);
 }
 
 static void part_sync(struct mtd_info *mtd)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	part->master->_sync(part->master);
 }
 
 static int part_suspend(struct mtd_info *mtd)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return part->master->_suspend(part->master);
 }
 
 static void part_resume(struct mtd_info *mtd)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	part->master->_resume(part->master);
 }
 
 static int part_block_isreserved(struct mtd_info *mtd, loff_t ofs)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	ofs += part->offset;
 	return part->master->_block_isreserved(part->master, ofs);
 }
 
 static int part_block_isbad(struct mtd_info *mtd, loff_t ofs)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	ofs += part->offset;
 	return part->master->_block_isbad(part->master, ofs);
 }
 
 static int part_block_markbad(struct mtd_info *mtd, loff_t ofs)
 {
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	int res;
 
 	ofs += part->offset;
@@ -397,6 +397,27 @@ static int part_block_markbad(struct mtd
 	return res;
 }
 
+static int part_ooblayout_ecc(struct mtd_info *mtd, int section,
+			      struct mtd_oob_region *oobregion)
+{
+	struct mtd_part *part = mtd_to_part(mtd);
+
+	return mtd_ooblayout_ecc(part->master, section, oobregion);
+}
+
+static int part_ooblayout_free(struct mtd_info *mtd, int section,
+			       struct mtd_oob_region *oobregion)
+{
+	struct mtd_part *part = mtd_to_part(mtd);
+
+	return mtd_ooblayout_free(part->master, section, oobregion);
+}
+
+static const struct mtd_ooblayout_ops part_ooblayout_ops = {
+	.ecc = part_ooblayout_ecc,
+	.free = part_ooblayout_free,
+};
+
 static inline void free_partition(struct mtd_part *p)
 {
 	kfree(p->mtd.name);
@@ -614,7 +635,7 @@ static struct mtd_part *allocate_partiti
 			slave->mtd.erasesize = slave->mtd.size;
 	}
 
-	slave->mtd.ecclayout = master->ecclayout;
+	mtd_set_ooblayout(&slave->mtd, &part_ooblayout_ops);
 	slave->mtd.ecc_step_size = master->ecc_step_size;
 	slave->mtd.ecc_strength = master->ecc_strength;
 	slave->mtd.bitflip_threshold = master->bitflip_threshold;
@@ -639,7 +660,7 @@ static ssize_t mtd_partition_offset_show
 		struct device_attribute *attr, char *buf)
 {
 	struct mtd_info *mtd = dev_get_drvdata(dev);
-	struct mtd_part *part = PART(mtd);
+	struct mtd_part *part = mtd_to_part(mtd);
 	return snprintf(buf, PAGE_SIZE, "%lld\n", part->offset);
 }
 
@@ -677,11 +698,10 @@ int mtd_add_partition(struct mtd_info *m
 	if (length <= 0)
 		return -EINVAL;
 
+	memset(&part, 0, sizeof(part));
 	part.name = name;
 	part.size = length;
 	part.offset = offset;
-	part.mask_flags = 0;
-	part.ecclayout = NULL;
 
 	new = allocate_partition(master, &part, -1, offset);
 	if (IS_ERR(new))
@@ -845,7 +865,7 @@ int add_mtd_partitions(struct mtd_info *
 static DEFINE_SPINLOCK(part_parser_lock);
 static LIST_HEAD(part_parsers);
 
-static struct mtd_part_parser *get_partition_parser(const char *name)
+static struct mtd_part_parser *mtd_part_parser_get(const char *name)
 {
 	struct mtd_part_parser *p, *ret = NULL;
 
@@ -862,7 +882,20 @@ static struct mtd_part_parser *get_parti
 	return ret;
 }
 
-#define put_partition_parser(p) do { module_put((p)->owner); } while (0)
+static inline void mtd_part_parser_put(const struct mtd_part_parser *p)
+{
+	module_put(p->owner);
+}
+
+/*
+ * Many partition parsers just expected the core to kfree() all their data in
+ * one chunk. Do that by default.
+ */
+static void mtd_part_parser_cleanup_default(const struct mtd_partition *pparts,
+					    int nr_parts)
+{
+	kfree(pparts);
+}
 
 static struct mtd_part_parser *
 get_partition_parser_by_type(enum mtd_parser_type type,
@@ -874,7 +907,7 @@ get_partition_parser_by_type(enum mtd_pa
 
 	p = list_prepare_entry(start, &part_parsers, list);
 	if (start)
-		put_partition_parser(start);
+		mtd_part_parser_put(start);
 
 	list_for_each_entry_continue(p, &part_parsers, list) {
 		if (p->type == type && try_module_get(p->owner)) {
@@ -888,13 +921,19 @@ get_partition_parser_by_type(enum mtd_pa
 	return ret;
 }
 
-void register_mtd_parser(struct mtd_part_parser *p)
-{
+int __register_mtd_parser(struct mtd_part_parser *p, struct module *owner)
+ {
+	p->owner = owner;
+
+	if (!p->cleanup)
+		p->cleanup = &mtd_part_parser_cleanup_default;
+
 	spin_lock(&part_parser_lock);
 	list_add(&p->list, &part_parsers);
 	spin_unlock(&part_parser_lock);
+	return 0;
 }
-EXPORT_SYMBOL_GPL(register_mtd_parser);
+EXPORT_SYMBOL_GPL(__register_mtd_parser);
 
 void deregister_mtd_parser(struct mtd_part_parser *p)
 {
@@ -954,7 +993,7 @@ static const char * const default_mtd_pa
  * parse_mtd_partitions - parse MTD partitions
  * @master: the master partition (describes whole MTD device)
  * @types: names of partition parsers to try or %NULL
- * @pparts: array of partitions found is returned here
+ * @pparts: info about partitions found is returned here
  * @data: MTD partition parser-specific data
  *
  * This function tries to find partition on MTD device @master. It uses MTD
@@ -966,45 +1005,42 @@ static const char * const default_mtd_pa
  *
  * This function may return:
  * o a negative error code in case of failure
- * o zero if no partitions were found
- * o a positive number of found partitions, in which case on exit @pparts will
- *   point to an array containing this number of &struct mtd_info objects.
+ * o zero otherwise, and @pparts will describe the partitions, number of
+ *   partitions, and the parser which parsed them. Caller must release
+ *   resources with mtd_part_parser_cleanup() when finished with the returned
+ *   data.
  */
 int parse_mtd_partitions(struct mtd_info *master, const char *const *types,
-			 struct mtd_partition **pparts,
+			 struct mtd_partitions *pparts,
 			 struct mtd_part_parser_data *data)
 {
 	struct mtd_part_parser *parser;
 	int ret, err = 0;
 	const char *const *types_of = NULL;
 
-	if (data && data->of_node) {
-		types_of = of_get_probes(data->of_node);
-		if (types_of != NULL)
-			types = types_of;
-	}
-
 	if (!types)
 		types = default_mtd_part_types;
 
 	for ( ; *types; types++) {
 		pr_debug("%s: parsing partitions %s\n", master->name, *types);
-		parser = get_partition_parser(*types);
+		parser = mtd_part_parser_get(*types);
 		if (!parser && !request_module("%s", *types))
-			parser = get_partition_parser(*types);
+			parser = mtd_part_parser_get(*types);
 		pr_debug("%s: got parser %s\n", master->name,
 			 parser ? parser->name : NULL);
 		if (!parser)
 			continue;
-		ret = (*parser->parse_fn)(master, pparts, data);
+		ret = (*parser->parse_fn)(master, &pparts->parts, data);
 		pr_debug("%s: parser %s: %i\n",
 			 master->name, parser->name, ret);
-		put_partition_parser(parser);
 		if (ret > 0) {
 			printk(KERN_NOTICE "%d %s partitions found on MTD device %s\n",
 			       ret, parser->name, master->name);
-			return ret;
+			pparts->nr_parts = ret;
+			pparts->parser = parser;
+			return 0;
 		}
+		mtd_part_parser_put(parser);
 		/*
 		 * Stash the first error we see; only report it if no parser
 		 * succeeds
@@ -1034,7 +1070,7 @@ int parse_mtd_partitions_by_type(struct
 		ret = (*parser->parse_fn)(master, pparts, data);
 
 		if (ret > 0) {
-			put_partition_parser(parser);
+			mtd_part_parser_put(parser);
 			printk(KERN_NOTICE
 			       "%d %s partitions found on MTD device %s\n",
 			       ret, parser->name, master->name);
@@ -1048,6 +1084,22 @@ int parse_mtd_partitions_by_type(struct
 }
 EXPORT_SYMBOL_GPL(parse_mtd_partitions_by_type);
 
+void mtd_part_parser_cleanup(struct mtd_partitions *parts)
+{
+	const struct mtd_part_parser *parser;
+
+	if (!parts)
+		return;
+
+	parser = parts->parser;
+	if (parser) {
+		if (parser->cleanup)
+			parser->cleanup(parts->parts, parts->nr_parts);
+
+		mtd_part_parser_put(parser);
+	}
+}
+
 int mtd_is_partition(const struct mtd_info *mtd)
 {
 	struct mtd_part *part;
@@ -1070,7 +1122,7 @@ struct mtd_info *mtdpart_get_master(cons
 	if (!mtd_is_partition(mtd))
 		return (struct mtd_info *)mtd;
 
-	return PART(mtd)->master;
+	return mtd_to_part(mtd)->master;
 }
 EXPORT_SYMBOL_GPL(mtdpart_get_master);
 
@@ -1079,7 +1131,7 @@ uint64_t mtdpart_get_offset(const struct
 	if (!mtd_is_partition(mtd))
 		return 0;
 
-	return PART(mtd)->offset;
+	return mtd_to_part(mtd)->offset;
 }
 EXPORT_SYMBOL_GPL(mtdpart_get_offset);
 
@@ -1089,6 +1141,6 @@ uint64_t mtd_get_device_size(const struc
 	if (!mtd_is_partition(mtd))
 		return mtd->size;
 
-	return PART(mtd)->master->size;
+	return mtd_to_part(mtd)->master->size;
 }
 EXPORT_SYMBOL_GPL(mtd_get_device_size);
--- a/drivers/mtd/mtdswap.c
+++ b/drivers/mtd/mtdswap.c
@@ -346,7 +346,7 @@ static int mtdswap_read_markers(struct m
 	if (mtd_can_have_bb(d->mtd) && mtd_block_isbad(d->mtd, offset))
 		return MTDSWAP_SCANNED_BAD;
 
-	ops.ooblen = 2 * d->mtd->ecclayout->oobavail;
+	ops.ooblen = 2 * d->mtd->oobavail;
 	ops.oobbuf = d->oob_buf;
 	ops.ooboffs = 0;
 	ops.datbuf = NULL;
@@ -359,7 +359,7 @@ static int mtdswap_read_markers(struct m
 
 	data = (struct mtdswap_oobdata *)d->oob_buf;
 	data2 = (struct mtdswap_oobdata *)
-		(d->oob_buf + d->mtd->ecclayout->oobavail);
+		(d->oob_buf + d->mtd->oobavail);
 
 	if (le16_to_cpu(data->magic) == MTDSWAP_MAGIC_CLEAN) {
 		eb->erase_count = le32_to_cpu(data->count);
@@ -933,7 +933,7 @@ static unsigned int mtdswap_eblk_passes(
 
 	ops.mode = MTD_OPS_AUTO_OOB;
 	ops.len = mtd->writesize;
-	ops.ooblen = mtd->ecclayout->oobavail;
+	ops.ooblen = mtd->oobavail;
 	ops.ooboffs = 0;
 	ops.datbuf = d->page_buf;
 	ops.oobbuf = d->oob_buf;
@@ -945,7 +945,7 @@ static unsigned int mtdswap_eblk_passes(
 		for (i = 0; i < mtd_pages; i++) {
 			patt = mtdswap_test_patt(test + i);
 			memset(d->page_buf, patt, mtd->writesize);
-			memset(d->oob_buf, patt, mtd->ecclayout->oobavail);
+			memset(d->oob_buf, patt, mtd->oobavail);
 			ret = mtd_write_oob(mtd, pos, &ops);
 			if (ret)
 				goto error;
@@ -964,7 +964,7 @@ static unsigned int mtdswap_eblk_passes(
 				if (p1[j] != patt)
 					goto error;
 
-			for (j = 0; j < mtd->ecclayout->oobavail; j++)
+			for (j = 0; j < mtd->oobavail; j++)
 				if (p2[j] != (unsigned char)patt)
 					goto error;
 
@@ -1387,7 +1387,7 @@ static int mtdswap_init(struct mtdswap_d
 	if (!d->page_buf)
 		goto page_buf_fail;
 
-	d->oob_buf = kmalloc(2 * mtd->ecclayout->oobavail, GFP_KERNEL);
+	d->oob_buf = kmalloc(2 * mtd->oobavail, GFP_KERNEL);
 	if (!d->oob_buf)
 		goto oob_buf_fail;
 
@@ -1417,7 +1417,6 @@ static void mtdswap_add_mtd(struct mtd_b
 	unsigned long part;
 	unsigned int eblocks, eavailable, bad_blocks, spare_cnt;
 	uint64_t swap_size, use_size, size_limit;
-	struct nand_ecclayout *oinfo;
 	int ret;
 
 	parts = &partitions[0];
@@ -1447,17 +1446,10 @@ static void mtdswap_add_mtd(struct mtd_b
 		return;
 	}
 
-	oinfo = mtd->ecclayout;
-	if (!oinfo) {
-		printk(KERN_ERR "%s: mtd%d does not have OOB\n",
-			MTDSWAP_PREFIX, mtd->index);
-		return;
-	}
-
-	if (!mtd->oobsize || oinfo->oobavail < MTDSWAP_OOBSIZE) {
+	if (!mtd->oobsize || mtd->oobavail < MTDSWAP_OOBSIZE) {
 		printk(KERN_ERR "%s: Not enough free bytes in OOB, "
 			"%d available, %zu needed.\n",
-			MTDSWAP_PREFIX, oinfo->oobavail, MTDSWAP_OOBSIZE);
+			MTDSWAP_PREFIX, mtd->oobavail, MTDSWAP_OOBSIZE);
 		return;
 	}
 
--- a/drivers/mtd/nand/Kconfig
+++ b/drivers/mtd/nand/Kconfig
@@ -55,7 +55,7 @@ config MTD_NAND_DENALI_PCI
 config MTD_NAND_DENALI_DT
 	tristate "Support Denali NAND controller as a DT device"
 	select MTD_NAND_DENALI
-	depends on HAS_DMA && HAVE_CLK
+	depends on HAS_DMA && HAVE_CLK && OF
 	help
 	  Enable the driver for NAND flash on platforms using a Denali NAND
 	  controller as a DT device.
@@ -74,6 +74,7 @@ config MTD_NAND_DENALI_SCRATCH_REG_ADDR
 config MTD_NAND_GPIO
 	tristate "GPIO assisted NAND Flash driver"
 	depends on GPIOLIB || COMPILE_TEST
+	depends on HAS_IOMEM
 	help
 	  This enables a NAND flash driver where control signals are
 	  connected to GPIO pins, and commands and data are communicated
@@ -310,6 +311,7 @@ config MTD_NAND_CAFE
 config MTD_NAND_CS553X
 	tristate "NAND support for CS5535/CS5536 (AMD Geode companion chip)"
 	depends on X86_32
+	depends on !UML && HAS_IOMEM
 	help
 	  The CS553x companion chips for the AMD Geode processor
 	  include NAND flash controllers with built-in hardware ECC
@@ -463,6 +465,7 @@ config MTD_NAND_MPC5121_NFC
 config MTD_NAND_VF610_NFC
 	tristate "Support for Freescale NFC for VF610/MPC5125"
 	depends on (SOC_VF610 || COMPILE_TEST)
+	depends on HAS_IOMEM
 	help
 	  Enables support for NAND Flash Controller on some Freescale
 	  processors like the VF610, MPC5125, MCF54418 or Kinetis K70.
@@ -480,7 +483,7 @@ config MTD_NAND_MXC
 
 config MTD_NAND_SH_FLCTL
 	tristate "Support for NAND on Renesas SuperH FLCTL"
-	depends on SUPERH || ARCH_SHMOBILE || COMPILE_TEST
+	depends on SUPERH || COMPILE_TEST
 	depends on HAS_IOMEM
 	depends on HAS_DMA
 	help
@@ -519,6 +522,13 @@ config MTD_NAND_JZ4740
 	help
 		Enables support for NAND Flash on JZ4740 SoC based boards.
 
+config MTD_NAND_JZ4780
+	tristate "Support for NAND on JZ4780 SoC"
+	depends on MACH_JZ4780 && JZ4780_NEMC
+	help
+	  Enables support for NAND Flash connected to the NEMC on JZ4780 SoC
+	  based boards, using the BCH controller for hardware error correction.
+
 config MTD_NAND_FSMC
 	tristate "Support for NAND on ST Micros FSMC"
 	depends on PLAT_SPEAR || ARCH_NOMADIK || ARCH_U8500 || MACH_U300
@@ -546,4 +556,11 @@ config MTD_NAND_HISI504
 	help
 	  Enables support for NAND controller on Hisilicon SoC Hip04.
 
+config MTD_NAND_QCOM
+	tristate "Support for NAND on QCOM SoCs"
+	depends on ARCH_QCOM
+	help
+	  Enables support for NAND flash chips on SoCs containing the EBI2 NAND
+	  controller. This controller is found on IPQ806x SoC.
+
 endif # MTD_NAND
--- a/drivers/mtd/nand/Makefile
+++ b/drivers/mtd/nand/Makefile
@@ -49,11 +49,13 @@ obj-$(CONFIG_MTD_NAND_MPC5121_NFC)	+= mp
 obj-$(CONFIG_MTD_NAND_VF610_NFC)	+= vf610_nfc.o
 obj-$(CONFIG_MTD_NAND_RICOH)		+= r852.o
 obj-$(CONFIG_MTD_NAND_JZ4740)		+= jz4740_nand.o
+obj-$(CONFIG_MTD_NAND_JZ4780)		+= jz4780_nand.o jz4780_bch.o
 obj-$(CONFIG_MTD_NAND_GPMI_NAND)	+= gpmi-nand/
 obj-$(CONFIG_MTD_NAND_XWAY)		+= xway_nand.o
 obj-$(CONFIG_MTD_NAND_BCM47XXNFLASH)	+= bcm47xxnflash/
 obj-$(CONFIG_MTD_NAND_SUNXI)		+= sunxi_nand.o
 obj-$(CONFIG_MTD_NAND_HISI504)	        += hisi504_nand.o
 obj-$(CONFIG_MTD_NAND_BRCMNAND)		+= brcmnand/
+obj-$(CONFIG_MTD_NAND_QCOM)		+= qcom_nandc.o
 
 nand-objs := nand_base.o nand_bbt.o nand_timings.o
--- a/drivers/mtd/nand/nand_base.c
+++ b/drivers/mtd/nand/nand_base.c
@@ -48,50 +48,6 @@
 #include <linux/mtd/partitions.h>
 #include <linux/of_mtd.h>
 
-/* Define default oob placement schemes for large and small page devices */
-static struct nand_ecclayout nand_oob_8 = {
-	.eccbytes = 3,
-	.eccpos = {0, 1, 2},
-	.oobfree = {
-		{.offset = 3,
-		 .length = 2},
-		{.offset = 6,
-		 .length = 2} }
-};
-
-static struct nand_ecclayout nand_oob_16 = {
-	.eccbytes = 6,
-	.eccpos = {0, 1, 2, 3, 6, 7},
-	.oobfree = {
-		{.offset = 8,
-		 . length = 8} }
-};
-
-static struct nand_ecclayout nand_oob_64 = {
-	.eccbytes = 24,
-	.eccpos = {
-		   40, 41, 42, 43, 44, 45, 46, 47,
-		   48, 49, 50, 51, 52, 53, 54, 55,
-		   56, 57, 58, 59, 60, 61, 62, 63},
-	.oobfree = {
-		{.offset = 2,
-		 .length = 38} }
-};
-
-static struct nand_ecclayout nand_oob_128 = {
-	.eccbytes = 48,
-	.eccpos = {
-		   80, 81, 82, 83, 84, 85, 86, 87,
-		   88, 89, 90, 91, 92, 93, 94, 95,
-		   96, 97, 98, 99, 100, 101, 102, 103,
-		   104, 105, 106, 107, 108, 109, 110, 111,
-		   112, 113, 114, 115, 116, 117, 118, 119,
-		   120, 121, 122, 123, 124, 125, 126, 127},
-	.oobfree = {
-		{.offset = 2,
-		 .length = 78} }
-};
-
 static int nand_get_device(struct mtd_info *mtd, int new_state);
 
 static int nand_do_write_oob(struct mtd_info *mtd, loff_t to,
@@ -103,10 +59,96 @@ static int nand_do_write_oob(struct mtd_
  */
 DEFINE_LED_TRIGGER(nand_led_trigger);
 
+/* Define default oob placement schemes for large and small page devices */
+static int nand_ooblayout_ecc_sp(struct mtd_info *mtd, int section,
+				 struct mtd_oob_region *oobregion)
+{
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nand_ecc_ctrl *ecc = &chip->ecc;
+
+	if (section > 1)
+		return -ERANGE;
+
+	if (!section) {
+		oobregion->offset = 0;
+		oobregion->length = 4;
+	} else {
+		oobregion->offset = 6;
+		oobregion->length = ecc->total - 4;
+	}
+
+	return 0;
+}
+
+static int nand_ooblayout_free_sp(struct mtd_info *mtd, int section,
+				  struct mtd_oob_region *oobregion)
+{
+	if (section > 1)
+		return -ERANGE;
+
+	if (mtd->oobsize == 16) {
+		if (section)
+			return -ERANGE;
+
+		oobregion->length = 8;
+		oobregion->offset = 8;
+	} else {
+		oobregion->length = 2;
+		if (!section)
+			oobregion->offset = 3;
+		else
+			oobregion->offset = 6;
+	}
+
+	return 0;
+}
+
+const struct mtd_ooblayout_ops nand_ooblayout_sp_ops = {
+	.ecc = nand_ooblayout_ecc_sp,
+	.free = nand_ooblayout_free_sp,
+};
+EXPORT_SYMBOL_GPL(nand_ooblayout_sp_ops);
+
+static int nand_ooblayout_ecc_lp(struct mtd_info *mtd, int section,
+				 struct mtd_oob_region *oobregion)
+{
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nand_ecc_ctrl *ecc = &chip->ecc;
+
+	if (section)
+		return -ERANGE;
+
+	oobregion->length = ecc->total;
+	oobregion->offset = mtd->oobsize - oobregion->length;
+
+	return 0;
+}
+
+static int nand_ooblayout_free_lp(struct mtd_info *mtd, int section,
+				  struct mtd_oob_region *oobregion)
+{
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nand_ecc_ctrl *ecc = &chip->ecc;
+
+	if (section)
+		return -ERANGE;
+
+	oobregion->length = mtd->oobsize - ecc->total - 2;
+	oobregion->offset = 2;
+
+	return 0;
+}
+
+const struct mtd_ooblayout_ops nand_ooblayout_lp_ops = {
+	.ecc = nand_ooblayout_ecc_lp,
+	.free = nand_ooblayout_free_lp,
+};
+EXPORT_SYMBOL_GPL(nand_ooblayout_lp_ops);
+
 static int check_offs_len(struct mtd_info *mtd,
 					loff_t ofs, uint64_t len)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	int ret = 0;
 
 	/* Start address must align on block boundary */
@@ -132,7 +174,7 @@ static int check_offs_len(struct mtd_inf
  */
 static void nand_release_device(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	/* Release the controller and the chip */
 	spin_lock(&chip->controller->lock);
@@ -150,7 +192,7 @@ static void nand_release_device(struct m
  */
 static uint8_t nand_read_byte(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	return readb(chip->IO_ADDR_R);
 }
 
@@ -163,7 +205,7 @@ static uint8_t nand_read_byte(struct mtd
  */
 static uint8_t nand_read_byte16(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	return (uint8_t) cpu_to_le16(readw(chip->IO_ADDR_R));
 }
 
@@ -175,7 +217,7 @@ static uint8_t nand_read_byte16(struct m
  */
 static u16 nand_read_word(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	return readw(chip->IO_ADDR_R);
 }
 
@@ -188,7 +230,7 @@ static u16 nand_read_word(struct mtd_inf
  */
 static void nand_select_chip(struct mtd_info *mtd, int chipnr)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	switch (chipnr) {
 	case -1:
@@ -211,7 +253,7 @@ static void nand_select_chip(struct mtd_
  */
 static void nand_write_byte(struct mtd_info *mtd, uint8_t byte)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	chip->write_buf(mtd, &byte, 1);
 }
@@ -225,7 +267,7 @@ static void nand_write_byte(struct mtd_i
  */
 static void nand_write_byte16(struct mtd_info *mtd, uint8_t byte)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	uint16_t word = byte;
 
 	/*
@@ -257,7 +299,7 @@ static void nand_write_byte16(struct mtd
  */
 static void nand_write_buf(struct mtd_info *mtd, const uint8_t *buf, int len)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	iowrite8_rep(chip->IO_ADDR_W, buf, len);
 }
@@ -272,7 +314,7 @@ static void nand_write_buf(struct mtd_in
  */
 static void nand_read_buf(struct mtd_info *mtd, uint8_t *buf, int len)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	ioread8_rep(chip->IO_ADDR_R, buf, len);
 }
@@ -287,7 +329,7 @@ static void nand_read_buf(struct mtd_inf
  */
 static void nand_write_buf16(struct mtd_info *mtd, const uint8_t *buf, int len)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	u16 *p = (u16 *) buf;
 
 	iowrite16_rep(chip->IO_ADDR_W, p, len >> 1);
@@ -303,7 +345,7 @@ static void nand_write_buf16(struct mtd_
  */
 static void nand_read_buf16(struct mtd_info *mtd, uint8_t *buf, int len)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	u16 *p = (u16 *) buf;
 
 	ioread16_rep(chip->IO_ADDR_R, p, len >> 1);
@@ -313,14 +355,13 @@ static void nand_read_buf16(struct mtd_i
  * nand_block_bad - [DEFAULT] Read bad block marker from the chip
  * @mtd: MTD device structure
  * @ofs: offset from device start
- * @getchip: 0, if the chip is already selected
  *
  * Check, if the block is bad.
  */
-static int nand_block_bad(struct mtd_info *mtd, loff_t ofs, int getchip)
+static int nand_block_bad(struct mtd_info *mtd, loff_t ofs)
 {
-	int page, chipnr, res = 0, i = 0;
-	struct nand_chip *chip = mtd->priv;
+	int page, res = 0, i = 0;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	u16 bad;
 
 	if (chip->bbt_options & NAND_BBT_SCANLASTPAGE)
@@ -328,15 +369,6 @@ static int nand_block_bad(struct mtd_inf
 
 	page = (int)(ofs >> chip->page_shift) & chip->pagemask;
 
-	if (getchip) {
-		chipnr = (int)(ofs >> chip->chip_shift);
-
-		nand_get_device(mtd, FL_READING);
-
-		/* Select the NAND device */
-		chip->select_chip(mtd, chipnr);
-	}
-
 	do {
 		if (chip->options & NAND_BUSWIDTH_16) {
 			chip->cmdfunc(mtd, NAND_CMD_READOOB,
@@ -361,11 +393,6 @@ static int nand_block_bad(struct mtd_inf
 		i++;
 	} while (!res && i < 2 && (chip->bbt_options & NAND_BBT_SCAN2NDPAGE));
 
-	if (getchip) {
-		chip->select_chip(mtd, -1);
-		nand_release_device(mtd);
-	}
-
 	return res;
 }
 
@@ -380,7 +407,7 @@ static int nand_block_bad(struct mtd_inf
  */
 static int nand_default_block_markbad(struct mtd_info *mtd, loff_t ofs)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	struct mtd_oob_ops ops;
 	uint8_t buf[2] = { 0, 0 };
 	int ret = 0, res, i = 0;
@@ -430,7 +457,7 @@ static int nand_default_block_markbad(st
 */
 static int nand_block_markbad_lowlevel(struct mtd_info *mtd, loff_t ofs)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	int res, ret = 0;
 
 	if (!(chip->bbt_options & NAND_BBT_NO_OOB_BBM)) {
@@ -471,7 +498,7 @@ static int nand_block_markbad_lowlevel(s
  */
 static int nand_check_wp(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	/* Broken xD cards report WP despite being writable */
 	if (chip->options & NAND_BROKEN_XD)
@@ -491,7 +518,7 @@ static int nand_check_wp(struct mtd_info
  */
 static int nand_block_isreserved(struct mtd_info *mtd, loff_t ofs)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	if (!chip->bbt)
 		return 0;
@@ -503,19 +530,17 @@ static int nand_block_isreserved(struct
  * nand_block_checkbad - [GENERIC] Check if a block is marked bad
  * @mtd: MTD device structure
  * @ofs: offset from device start
- * @getchip: 0, if the chip is already selected
  * @allowbbt: 1, if its allowed to access the bbt area
  *
  * Check, if the block is bad. Either by reading the bad block table or
  * calling of the scan function.
  */
-static int nand_block_checkbad(struct mtd_info *mtd, loff_t ofs, int getchip,
-			       int allowbbt)
+static int nand_block_checkbad(struct mtd_info *mtd, loff_t ofs, int allowbbt)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	if (!chip->bbt)
-		return chip->block_bad(mtd, ofs, getchip);
+		return chip->block_bad(mtd, ofs);
 
 	/* Return info from the table */
 	return nand_isbad_bbt(mtd, ofs, allowbbt);
@@ -531,7 +556,7 @@ static int nand_block_checkbad(struct mt
  */
 static void panic_nand_wait_ready(struct mtd_info *mtd, unsigned long timeo)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	int i;
 
 	/* Wait for the device to get ready */
@@ -551,7 +576,7 @@ static void panic_nand_wait_ready(struct
  */
 void nand_wait_ready(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	unsigned long timeo = 400;
 
 	if (in_interrupt() || oops_in_progress)
@@ -566,8 +591,8 @@ void nand_wait_ready(struct mtd_info *mt
 		cond_resched();
 	} while (time_before(jiffies, timeo));
 
-	pr_warn_ratelimited(
-		"timeout while waiting for chip to become ready\n");
+	if (!chip->dev_ready(mtd))
+		pr_warn_ratelimited("timeout while waiting for chip to become ready\n");
 out:
 	led_trigger_event(nand_led_trigger, LED_OFF);
 }
@@ -582,7 +607,7 @@ EXPORT_SYMBOL_GPL(nand_wait_ready);
  */
 static void nand_wait_status_ready(struct mtd_info *mtd, unsigned long timeo)
 {
-	register struct nand_chip *chip = mtd->priv;
+	register struct nand_chip *chip = mtd_to_nand(mtd);
 
 	timeo = jiffies + msecs_to_jiffies(timeo);
 	do {
@@ -605,7 +630,7 @@ static void nand_wait_status_ready(struc
 static void nand_command(struct mtd_info *mtd, unsigned int command,
 			 int column, int page_addr)
 {
-	register struct nand_chip *chip = mtd->priv;
+	register struct nand_chip *chip = mtd_to_nand(mtd);
 	int ctrl = NAND_CTRL_CLE | NAND_CTRL_CHANGE;
 
 	/* Write out the command to the device */
@@ -708,7 +733,7 @@ static void nand_command(struct mtd_info
 static void nand_command_lp(struct mtd_info *mtd, unsigned int command,
 			    int column, int page_addr)
 {
-	register struct nand_chip *chip = mtd->priv;
+	register struct nand_chip *chip = mtd_to_nand(mtd);
 
 	/* Emulate NAND_CMD_READOOB */
 	if (command == NAND_CMD_READOOB) {
@@ -832,7 +857,7 @@ static void panic_nand_get_device(struct
 static int
 nand_get_device(struct mtd_info *mtd, int new_state)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	spinlock_t *lock = &chip->controller->lock;
 	wait_queue_head_t *wq = &chip->controller->wq;
 	DECLARE_WAITQUEUE(wait, current);
@@ -952,7 +977,7 @@ static int __nand_unlock(struct mtd_info
 {
 	int ret = 0;
 	int status, page;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	/* Submit address of first page to unlock */
 	page = ofs >> chip->page_shift;
@@ -987,7 +1012,7 @@ int nand_unlock(struct mtd_info *mtd, lo
 {
 	int ret = 0;
 	int chipnr;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	pr_debug("%s: start = 0x%012llx, len = %llu\n",
 			__func__, (unsigned long long)ofs, len);
@@ -1050,7 +1075,7 @@ int nand_lock(struct mtd_info *mtd, loff
 {
 	int ret = 0;
 	int chipnr, status, page;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	pr_debug("%s: start = 0x%012llx, len = %llu\n",
 			__func__, (unsigned long long)ofs, len);
@@ -1309,13 +1334,12 @@ static int nand_read_page_raw_syndrome(s
 static int nand_read_page_swecc(struct mtd_info *mtd, struct nand_chip *chip,
 				uint8_t *buf, int oob_required, int page)
 {
-	int i, eccsize = chip->ecc.size;
+	int i, eccsize = chip->ecc.size, ret;
 	int eccbytes = chip->ecc.bytes;
 	int eccsteps = chip->ecc.steps;
 	uint8_t *p = buf;
 	uint8_t *ecc_calc = chip->buffers->ecccalc;
 	uint8_t *ecc_code = chip->buffers->ecccode;
-	uint32_t *eccpos = chip->ecc.layout->eccpos;
 	unsigned int max_bitflips = 0;
 
 	chip->ecc.read_page_raw(mtd, chip, buf, 1, page);
@@ -1323,8 +1347,10 @@ static int nand_read_page_swecc(struct m
 	for (i = 0; eccsteps; eccsteps--, i += eccbytes, p += eccsize)
 		chip->ecc.calculate(mtd, p, &ecc_calc[i]);
 
-	for (i = 0; i < chip->ecc.total; i++)
-		ecc_code[i] = chip->oob_poi[eccpos[i]];
+	ret = mtd_ooblayout_get_eccbytes(mtd, ecc_code, chip->oob_poi, 0,
+					 chip->ecc.total);
+	if (ret)
+		return ret;
 
 	eccsteps = chip->ecc.steps;
 	p = buf;
@@ -1356,14 +1382,14 @@ static int nand_read_subpage(struct mtd_
 			uint32_t data_offs, uint32_t readlen, uint8_t *bufpoi,
 			int page)
 {
-	int start_step, end_step, num_steps;
-	uint32_t *eccpos = chip->ecc.layout->eccpos;
+	int start_step, end_step, num_steps, ret;
 	uint8_t *p;
 	int data_col_addr, i, gaps = 0;
 	int datafrag_len, eccfrag_len, aligned_len, aligned_pos;
 	int busw = (chip->options & NAND_BUSWIDTH_16) ? 2 : 1;
-	int index;
+	int index, section = 0;
 	unsigned int max_bitflips = 0;
+	struct mtd_oob_region oobregion = { };
 
 	/* Column address within the page aligned to ECC size (256bytes) */
 	start_step = data_offs / chip->ecc.size;
@@ -1391,12 +1417,13 @@ static int nand_read_subpage(struct mtd_
 	 * The performance is faster if we position offsets according to
 	 * ecc.pos. Let's make sure that there are no gaps in ECC positions.
 	 */
-	for (i = 0; i < eccfrag_len - 1; i++) {
-		if (eccpos[i + index] + 1 != eccpos[i + index + 1]) {
-			gaps = 1;
-			break;
-		}
-	}
+	ret = mtd_ooblayout_find_eccregion(mtd, index, &section, &oobregion);
+	if (ret)
+		return ret;
+
+	if (oobregion.length < eccfrag_len)
+		gaps = 1;
+
 	if (gaps) {
 		chip->cmdfunc(mtd, NAND_CMD_RNDOUT, mtd->writesize, -1);
 		chip->read_buf(mtd, chip->oob_poi, mtd->oobsize);
@@ -1405,20 +1432,23 @@ static int nand_read_subpage(struct mtd_
 		 * Send the command to read the particular ECC bytes take care
 		 * about buswidth alignment in read_buf.
 		 */
-		aligned_pos = eccpos[index] & ~(busw - 1);
+		aligned_pos = oobregion.offset & ~(busw - 1);
 		aligned_len = eccfrag_len;
-		if (eccpos[index] & (busw - 1))
+		if (oobregion.offset & (busw - 1))
 			aligned_len++;
-		if (eccpos[index + (num_steps * chip->ecc.bytes)] & (busw - 1))
+		if ((oobregion.offset + (num_steps * chip->ecc.bytes)) &
+		    (busw - 1))
 			aligned_len++;
 
 		chip->cmdfunc(mtd, NAND_CMD_RNDOUT,
-					mtd->writesize + aligned_pos, -1);
+			      mtd->writesize + aligned_pos, -1);
 		chip->read_buf(mtd, &chip->oob_poi[aligned_pos], aligned_len);
 	}
 
-	for (i = 0; i < eccfrag_len; i++)
-		chip->buffers->ecccode[i] = chip->oob_poi[eccpos[i + index]];
+	ret = mtd_ooblayout_get_eccbytes(mtd, chip->buffers->ecccode,
+					 chip->oob_poi, index, eccfrag_len);
+	if (ret)
+		return ret;
 
 	p = bufpoi + data_col_addr;
 	for (i = 0; i < eccfrag_len ; i += chip->ecc.bytes, p += chip->ecc.size) {
@@ -1426,6 +1456,16 @@ static int nand_read_subpage(struct mtd_
 
 		stat = chip->ecc.correct(mtd, p,
 			&chip->buffers->ecccode[i], &chip->buffers->ecccalc[i]);
+		if (stat == -EBADMSG &&
+		    (chip->ecc.options & NAND_ECC_GENERIC_ERASED_CHECK)) {
+			/* check for empty pages with bitflips */
+			stat = nand_check_erased_ecc_chunk(p, chip->ecc.size,
+						&chip->buffers->ecccode[i],
+						chip->ecc.bytes,
+						NULL, 0,
+						chip->ecc.strength);
+		}
+
 		if (stat < 0) {
 			mtd->ecc_stats.failed++;
 		} else {
@@ -1449,13 +1489,12 @@ static int nand_read_subpage(struct mtd_
 static int nand_read_page_hwecc(struct mtd_info *mtd, struct nand_chip *chip,
 				uint8_t *buf, int oob_required, int page)
 {
-	int i, eccsize = chip->ecc.size;
+	int i, eccsize = chip->ecc.size, ret;
 	int eccbytes = chip->ecc.bytes;
 	int eccsteps = chip->ecc.steps;
 	uint8_t *p = buf;
 	uint8_t *ecc_calc = chip->buffers->ecccalc;
 	uint8_t *ecc_code = chip->buffers->ecccode;
-	uint32_t *eccpos = chip->ecc.layout->eccpos;
 	unsigned int max_bitflips = 0;
 
 	for (i = 0; eccsteps; eccsteps--, i += eccbytes, p += eccsize) {
@@ -1465,8 +1504,10 @@ static int nand_read_page_hwecc(struct m
 	}
 	chip->read_buf(mtd, chip->oob_poi, mtd->oobsize);
 
-	for (i = 0; i < chip->ecc.total; i++)
-		ecc_code[i] = chip->oob_poi[eccpos[i]];
+	ret = mtd_ooblayout_get_eccbytes(mtd, ecc_code, chip->oob_poi, 0,
+					 chip->ecc.total);
+	if (ret)
+		return ret;
 
 	eccsteps = chip->ecc.steps;
 	p = buf;
@@ -1475,6 +1516,15 @@ static int nand_read_page_hwecc(struct m
 		int stat;
 
 		stat = chip->ecc.correct(mtd, p, &ecc_code[i], &ecc_calc[i]);
+		if (stat == -EBADMSG &&
+		    (chip->ecc.options & NAND_ECC_GENERIC_ERASED_CHECK)) {
+			/* check for empty pages with bitflips */
+			stat = nand_check_erased_ecc_chunk(p, eccsize,
+						&ecc_code[i], eccbytes,
+						NULL, 0,
+						chip->ecc.strength);
+		}
+
 		if (stat < 0) {
 			mtd->ecc_stats.failed++;
 		} else {
@@ -1502,12 +1552,11 @@ static int nand_read_page_hwecc(struct m
 static int nand_read_page_hwecc_oob_first(struct mtd_info *mtd,
 	struct nand_chip *chip, uint8_t *buf, int oob_required, int page)
 {
-	int i, eccsize = chip->ecc.size;
+	int i, eccsize = chip->ecc.size, ret;
 	int eccbytes = chip->ecc.bytes;
 	int eccsteps = chip->ecc.steps;
 	uint8_t *p = buf;
 	uint8_t *ecc_code = chip->buffers->ecccode;
-	uint32_t *eccpos = chip->ecc.layout->eccpos;
 	uint8_t *ecc_calc = chip->buffers->ecccalc;
 	unsigned int max_bitflips = 0;
 
@@ -1516,8 +1565,10 @@ static int nand_read_page_hwecc_oob_firs
 	chip->read_buf(mtd, chip->oob_poi, mtd->oobsize);
 	chip->cmdfunc(mtd, NAND_CMD_READ0, 0, page);
 
-	for (i = 0; i < chip->ecc.total; i++)
-		ecc_code[i] = chip->oob_poi[eccpos[i]];
+	ret = mtd_ooblayout_get_eccbytes(mtd, ecc_code, chip->oob_poi, 0,
+					 chip->ecc.total);
+	if (ret)
+		return ret;
 
 	for (i = 0; eccsteps; eccsteps--, i += eccbytes, p += eccsize) {
 		int stat;
@@ -1527,6 +1578,15 @@ static int nand_read_page_hwecc_oob_firs
 		chip->ecc.calculate(mtd, p, &ecc_calc[i]);
 
 		stat = chip->ecc.correct(mtd, p, &ecc_code[i], NULL);
+		if (stat == -EBADMSG &&
+		    (chip->ecc.options & NAND_ECC_GENERIC_ERASED_CHECK)) {
+			/* check for empty pages with bitflips */
+			stat = nand_check_erased_ecc_chunk(p, eccsize,
+						&ecc_code[i], eccbytes,
+						NULL, 0,
+						chip->ecc.strength);
+		}
+
 		if (stat < 0) {
 			mtd->ecc_stats.failed++;
 		} else {
@@ -1554,6 +1614,7 @@ static int nand_read_page_syndrome(struc
 	int i, eccsize = chip->ecc.size;
 	int eccbytes = chip->ecc.bytes;
 	int eccsteps = chip->ecc.steps;
+	int eccpadbytes = eccbytes + chip->ecc.prepad + chip->ecc.postpad;
 	uint8_t *p = buf;
 	uint8_t *oob = chip->oob_poi;
 	unsigned int max_bitflips = 0;
@@ -1573,19 +1634,29 @@ static int nand_read_page_syndrome(struc
 		chip->read_buf(mtd, oob, eccbytes);
 		stat = chip->ecc.correct(mtd, p, oob, NULL);
 
-		if (stat < 0) {
-			mtd->ecc_stats.failed++;
-		} else {
-			mtd->ecc_stats.corrected += stat;
-			max_bitflips = max_t(unsigned int, max_bitflips, stat);
-		}
-
 		oob += eccbytes;
 
 		if (chip->ecc.postpad) {
 			chip->read_buf(mtd, oob, chip->ecc.postpad);
 			oob += chip->ecc.postpad;
 		}
+
+		if (stat == -EBADMSG &&
+		    (chip->ecc.options & NAND_ECC_GENERIC_ERASED_CHECK)) {
+			/* check for empty pages with bitflips */
+			stat = nand_check_erased_ecc_chunk(p, chip->ecc.size,
+							   oob - eccpadbytes,
+							   eccpadbytes,
+							   NULL, 0,
+							   chip->ecc.strength);
+		}
+
+		if (stat < 0) {
+			mtd->ecc_stats.failed++;
+		} else {
+			mtd->ecc_stats.corrected += stat;
+			max_bitflips = max_t(unsigned int, max_bitflips, stat);
+		}
 	}
 
 	/* Calculate remaining oob bytes */
@@ -1598,14 +1669,17 @@ static int nand_read_page_syndrome(struc
 
 /**
  * nand_transfer_oob - [INTERN] Transfer oob to client buffer
- * @chip: nand chip structure
+ * @mtd: mtd info structure
  * @oob: oob destination address
  * @ops: oob ops structure
  * @len: size of oob to transfer
  */
-static uint8_t *nand_transfer_oob(struct nand_chip *chip, uint8_t *oob,
+static uint8_t *nand_transfer_oob(struct mtd_info *mtd, uint8_t *oob,
 				  struct mtd_oob_ops *ops, size_t len)
 {
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	int ret;
+
 	switch (ops->mode) {
 
 	case MTD_OPS_PLACE_OOB:
@@ -1613,31 +1687,12 @@ static uint8_t *nand_transfer_oob(struct
 		memcpy(oob, chip->oob_poi + ops->ooboffs, len);
 		return oob + len;
 
-	case MTD_OPS_AUTO_OOB: {
-		struct nand_oobfree *free = chip->ecc.layout->oobfree;
-		uint32_t boffs = 0, roffs = ops->ooboffs;
-		size_t bytes = 0;
-
-		for (; free->length && len; free++, len -= bytes) {
-			/* Read request not from offset 0? */
-			if (unlikely(roffs)) {
-				if (roffs >= free->length) {
-					roffs -= free->length;
-					continue;
-				}
-				boffs = free->offset + roffs;
-				bytes = min_t(size_t, len,
-					      (free->length - roffs));
-				roffs = 0;
-			} else {
-				bytes = min_t(size_t, len, free->length);
-				boffs = free->offset;
-			}
-			memcpy(oob, chip->oob_poi + boffs, bytes);
-			oob += bytes;
-		}
-		return oob;
-	}
+	case MTD_OPS_AUTO_OOB:
+		ret = mtd_ooblayout_get_databytes(mtd, oob, chip->oob_poi,
+						  ops->ooboffs, len);
+		BUG_ON(ret);
+		return oob + len;
+
 	default:
 		BUG();
 	}
@@ -1655,7 +1710,7 @@ static uint8_t *nand_transfer_oob(struct
  */
 static int nand_setup_read_retry(struct mtd_info *mtd, int retry_mode)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	pr_debug("setting READ RETRY mode %d\n", retry_mode);
 
@@ -1680,12 +1735,11 @@ static int nand_do_read_ops(struct mtd_i
 			    struct mtd_oob_ops *ops)
 {
 	int chipnr, page, realpage, col, bytes, aligned, oob_required;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	int ret = 0;
 	uint32_t readlen = ops->len;
 	uint32_t oobreadlen = ops->ooblen;
-	uint32_t max_oobsize = ops->mode == MTD_OPS_AUTO_OOB ?
-		mtd->oobavail : mtd->oobsize;
+	uint32_t max_oobsize = mtd_oobavail(mtd, ops);
 
 	uint8_t *bufpoi, *oob, *buf;
 	int use_bufpoi;
@@ -1772,7 +1826,7 @@ read_retry:
 				int toread = min(oobreadlen, max_oobsize);
 
 				if (toread) {
-					oob = nand_transfer_oob(chip,
+					oob = nand_transfer_oob(mtd,
 						oob, ops, toread);
 					oobreadlen -= toread;
 				}
@@ -2024,7 +2078,7 @@ static int nand_do_read_oob(struct mtd_i
 			    struct mtd_oob_ops *ops)
 {
 	int page, realpage, chipnr;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	struct mtd_ecc_stats stats;
 	int readlen = ops->ooblen;
 	int len;
@@ -2036,10 +2090,7 @@ static int nand_do_read_oob(struct mtd_i
 
 	stats = mtd->ecc_stats;
 
-	if (ops->mode == MTD_OPS_AUTO_OOB)
-		len = chip->ecc.layout->oobavail;
-	else
-		len = mtd->oobsize;
+	len = mtd_oobavail(mtd, ops);
 
 	if (unlikely(ops->ooboffs >= len)) {
 		pr_debug("%s: attempt to start read outside oob\n",
@@ -2073,7 +2124,7 @@ static int nand_do_read_oob(struct mtd_i
 			break;
 
 		len = min(len, readlen);
-		buf = nand_transfer_oob(chip, buf, ops, len);
+		buf = nand_transfer_oob(mtd, buf, ops, len);
 
 		if (chip->options & NAND_NEED_READRDY) {
 			/* Apply delay or wait for ready/busy pin */
@@ -2232,19 +2283,20 @@ static int nand_write_page_swecc(struct
 				 const uint8_t *buf, int oob_required,
 				 int page)
 {
-	int i, eccsize = chip->ecc.size;
+	int i, eccsize = chip->ecc.size, ret;
 	int eccbytes = chip->ecc.bytes;
 	int eccsteps = chip->ecc.steps;
 	uint8_t *ecc_calc = chip->buffers->ecccalc;
 	const uint8_t *p = buf;
-	uint32_t *eccpos = chip->ecc.layout->eccpos;
 
 	/* Software ECC calculation */
 	for (i = 0; eccsteps; eccsteps--, i += eccbytes, p += eccsize)
 		chip->ecc.calculate(mtd, p, &ecc_calc[i]);
 
-	for (i = 0; i < chip->ecc.total; i++)
-		chip->oob_poi[eccpos[i]] = ecc_calc[i];
+	ret = mtd_ooblayout_set_eccbytes(mtd, ecc_calc, chip->oob_poi, 0,
+					 chip->ecc.total);
+	if (ret)
+		return ret;
 
 	return chip->ecc.write_page_raw(mtd, chip, buf, 1, page);
 }
@@ -2261,12 +2313,11 @@ static int nand_write_page_hwecc(struct
 				  const uint8_t *buf, int oob_required,
 				  int page)
 {
-	int i, eccsize = chip->ecc.size;
+	int i, eccsize = chip->ecc.size, ret;
 	int eccbytes = chip->ecc.bytes;
 	int eccsteps = chip->ecc.steps;
 	uint8_t *ecc_calc = chip->buffers->ecccalc;
 	const uint8_t *p = buf;
-	uint32_t *eccpos = chip->ecc.layout->eccpos;
 
 	for (i = 0; eccsteps; eccsteps--, i += eccbytes, p += eccsize) {
 		chip->ecc.hwctl(mtd, NAND_ECC_WRITE);
@@ -2274,8 +2325,10 @@ static int nand_write_page_hwecc(struct
 		chip->ecc.calculate(mtd, p, &ecc_calc[i]);
 	}
 
-	for (i = 0; i < chip->ecc.total; i++)
-		chip->oob_poi[eccpos[i]] = ecc_calc[i];
+	ret = mtd_ooblayout_set_eccbytes(mtd, ecc_calc, chip->oob_poi, 0,
+					 chip->ecc.total);
+	if (ret)
+		return ret;
 
 	chip->write_buf(mtd, chip->oob_poi, mtd->oobsize);
 
@@ -2303,11 +2356,10 @@ static int nand_write_subpage_hwecc(stru
 	int ecc_size      = chip->ecc.size;
 	int ecc_bytes     = chip->ecc.bytes;
 	int ecc_steps     = chip->ecc.steps;
-	uint32_t *eccpos  = chip->ecc.layout->eccpos;
 	uint32_t start_step = offset / ecc_size;
 	uint32_t end_step   = (offset + data_len - 1) / ecc_size;
 	int oob_bytes       = mtd->oobsize / ecc_steps;
-	int step, i;
+	int step, ret;
 
 	for (step = 0; step < ecc_steps; step++) {
 		/* configure controller for WRITE access */
@@ -2335,8 +2387,10 @@ static int nand_write_subpage_hwecc(stru
 	/* copy calculated ECC for whole page to chip->buffer->oob */
 	/* this include masked-value(0xFF) for unwritten subpages */
 	ecc_calc = chip->buffers->ecccalc;
-	for (i = 0; i < chip->ecc.total; i++)
-		chip->oob_poi[eccpos[i]] = ecc_calc[i];
+	ret = mtd_ooblayout_set_eccbytes(mtd, ecc_calc, chip->oob_poi, 0,
+					 chip->ecc.total);
+	if (ret)
+		return ret;
 
 	/* write OOB buffer to NAND device */
 	chip->write_buf(mtd, chip->oob_poi, mtd->oobsize);
@@ -2472,7 +2526,8 @@ static int nand_write_page(struct mtd_in
 static uint8_t *nand_fill_oob(struct mtd_info *mtd, uint8_t *oob, size_t len,
 			      struct mtd_oob_ops *ops)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	int ret;
 
 	/*
 	 * Initialise to all 0xFF, to avoid the possibility of left over OOB
@@ -2487,31 +2542,12 @@ static uint8_t *nand_fill_oob(struct mtd
 		memcpy(chip->oob_poi + ops->ooboffs, oob, len);
 		return oob + len;
 
-	case MTD_OPS_AUTO_OOB: {
-		struct nand_oobfree *free = chip->ecc.layout->oobfree;
-		uint32_t boffs = 0, woffs = ops->ooboffs;
-		size_t bytes = 0;
-
-		for (; free->length && len; free++, len -= bytes) {
-			/* Write request not from offset 0? */
-			if (unlikely(woffs)) {
-				if (woffs >= free->length) {
-					woffs -= free->length;
-					continue;
-				}
-				boffs = free->offset + woffs;
-				bytes = min_t(size_t, len,
-					      (free->length - woffs));
-				woffs = 0;
-			} else {
-				bytes = min_t(size_t, len, free->length);
-				boffs = free->offset;
-			}
-			memcpy(chip->oob_poi + boffs, oob, bytes);
-			oob += bytes;
-		}
-		return oob;
-	}
+	case MTD_OPS_AUTO_OOB:
+		ret = mtd_ooblayout_set_databytes(mtd, oob, chip->oob_poi,
+						  ops->ooboffs, len);
+		BUG_ON(ret);
+		return oob + len;
+
 	default:
 		BUG();
 	}
@@ -2532,12 +2568,11 @@ static int nand_do_write_ops(struct mtd_
 			     struct mtd_oob_ops *ops)
 {
 	int chipnr, realpage, page, blockmask, column;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	uint32_t writelen = ops->len;
 
 	uint32_t oobwritelen = ops->ooblen;
-	uint32_t oobmaxlen = ops->mode == MTD_OPS_AUTO_OOB ?
-				mtd->oobavail : mtd->oobsize;
+	uint32_t oobmaxlen = mtd_oobavail(mtd, ops);
 
 	uint8_t *oob = ops->oobbuf;
 	uint8_t *buf = ops->datbuf;
@@ -2662,7 +2697,7 @@ err_out:
 static int panic_nand_write(struct mtd_info *mtd, loff_t to, size_t len,
 			    size_t *retlen, const uint8_t *buf)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	struct mtd_oob_ops ops;
 	int ret;
 
@@ -2722,15 +2757,12 @@ static int nand_do_write_oob(struct mtd_
 			     struct mtd_oob_ops *ops)
 {
 	int chipnr, page, status, len;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	pr_debug("%s: to = 0x%08x, len = %i\n",
 			 __func__, (unsigned int)to, (int)ops->ooblen);
 
-	if (ops->mode == MTD_OPS_AUTO_OOB)
-		len = chip->ecc.layout->oobavail;
-	else
-		len = mtd->oobsize;
+	len = mtd_oobavail(mtd, ops);
 
 	/* Do not allow write past end of page */
 	if ((ops->ooboffs + ops->ooblen) > len) {
@@ -2847,7 +2879,7 @@ out:
  */
 static int single_erase(struct mtd_info *mtd, int page)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	/* Send commands to erase a block */
 	chip->cmdfunc(mtd, NAND_CMD_ERASE1, -1, page);
 	chip->cmdfunc(mtd, NAND_CMD_ERASE2, -1, -1);
@@ -2879,7 +2911,7 @@ int nand_erase_nand(struct mtd_info *mtd
 		    int allowbbt)
 {
 	int page, status, pages_per_block, ret, chipnr;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	loff_t len;
 
 	pr_debug("%s: start = 0x%012llx, len = %llu\n",
@@ -2918,7 +2950,7 @@ int nand_erase_nand(struct mtd_info *mtd
 	while (len) {
 		/* Check if we have a bad block, we do not erase bad blocks! */
 		if (nand_block_checkbad(mtd, ((loff_t) page) <<
-					chip->page_shift, 0, allowbbt)) {
+					chip->page_shift, allowbbt)) {
 			pr_warn("%s: attempt to erase a bad block at page 0x%08x\n",
 				    __func__, page);
 			instr->state = MTD_ERASE_FAILED;
@@ -3005,7 +3037,20 @@ static void nand_sync(struct mtd_info *m
  */
 static int nand_block_isbad(struct mtd_info *mtd, loff_t offs)
 {
-	return nand_block_checkbad(mtd, offs, 1, 0);
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	int chipnr = (int)(offs >> chip->chip_shift);
+	int ret;
+
+	/* Select the NAND device */
+	nand_get_device(mtd, FL_READING);
+	chip->select_chip(mtd, chipnr);
+
+	ret = nand_block_checkbad(mtd, offs, 0);
+
+	chip->select_chip(mtd, -1);
+	nand_release_device(mtd);
+
+	return ret;
 }
 
 /**
@@ -3094,7 +3139,7 @@ static int nand_suspend(struct mtd_info
  */
 static void nand_resume(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	if (chip->state == FL_PM_SUSPENDED)
 		nand_release_device(mtd);
@@ -3266,7 +3311,7 @@ ext_out:
 
 static int nand_setup_read_retry_micron(struct mtd_info *mtd, int retry_mode)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	uint8_t feature[ONFI_SUBFEATURE_PARAM_LEN] = {retry_mode};
 
 	return chip->onfi_set_features(mtd, chip, ONFI_FEATURE_ADDR_READ_RETRY,
@@ -3937,10 +3982,13 @@ ident_done:
 	return type;
 }
 
-static int nand_dt_init(struct mtd_info *mtd, struct nand_chip *chip,
-			struct device_node *dn)
+static int nand_dt_init(struct nand_chip *chip)
 {
-	int ecc_mode, ecc_strength, ecc_step;
+	struct device_node *dn = nand_get_flash_node(chip);
+	int ecc_mode, ecc_algo, ecc_strength, ecc_step;
+
+	if (!dn)
+		return 0;
 
 	if (of_get_nand_bus_width(dn) == 16)
 		chip->options |= NAND_BUSWIDTH_16;
@@ -3949,6 +3997,7 @@ static int nand_dt_init(struct mtd_info
 		chip->bbt_options |= NAND_BBT_USE_FLASH;
 
 	ecc_mode = of_get_nand_ecc_mode(dn);
+	ecc_algo = of_get_nand_ecc_algo(dn);
 	ecc_strength = of_get_nand_ecc_strength(dn);
 	ecc_step = of_get_nand_ecc_step_size(dn);
 
@@ -3961,6 +4010,9 @@ static int nand_dt_init(struct mtd_info
 	if (ecc_mode >= 0)
 		chip->ecc.mode = ecc_mode;
 
+	if (ecc_algo >= 0)
+		chip->ecc.algo = ecc_algo;
+
 	if (ecc_strength >= 0)
 		chip->ecc.strength = ecc_strength;
 
@@ -3984,15 +4036,16 @@ int nand_scan_ident(struct mtd_info *mtd
 		    struct nand_flash_dev *table)
 {
 	int i, nand_maf_id, nand_dev_id;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	struct nand_flash_dev *type;
 	int ret;
 
-	if (chip->flash_node) {
-		ret = nand_dt_init(mtd, chip, chip->flash_node);
-		if (ret)
-			return ret;
-	}
+	ret = nand_dt_init(chip);
+	if (ret)
+		return ret;
+
+	if (!mtd->name && mtd->dev.parent)
+		mtd->name = dev_name(mtd->dev.parent);
 
 	if (!mtd->name && mtd->dev.parent)
 		mtd->name = dev_name(mtd->dev.parent);
@@ -4055,7 +4108,7 @@ EXPORT_SYMBOL(nand_scan_ident);
  */
 static bool nand_ecc_strength_good(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	struct nand_ecc_ctrl *ecc = &chip->ecc;
 	int corr, ds_corr;
 
@@ -4083,10 +4136,10 @@ static bool nand_ecc_strength_good(struc
  */
 int nand_scan_tail(struct mtd_info *mtd)
 {
-	int i;
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 	struct nand_ecc_ctrl *ecc = &chip->ecc;
 	struct nand_buffers *nbuf;
+	int ret;
 
 	/* New bad blocks should be marked in OOB, flash-based BBT, or both */
 	BUG_ON((chip->bbt_options & NAND_BBT_NO_OOB_BBM) &&
@@ -4113,19 +4166,15 @@ int nand_scan_tail(struct mtd_info *mtd)
 	/*
 	 * If no default placement scheme is given, select an appropriate one.
 	 */
-	if (!ecc->layout && (ecc->mode != NAND_ECC_SOFT_BCH)) {
+	if (!mtd->ooblayout && (ecc->mode != NAND_ECC_SOFT_BCH)) {
 		switch (mtd->oobsize) {
 		case 8:
-			ecc->layout = &nand_oob_8;
-			break;
 		case 16:
-			ecc->layout = &nand_oob_16;
+			mtd_set_ooblayout(mtd, &nand_ooblayout_sp_ops);
 			break;
 		case 64:
-			ecc->layout = &nand_oob_64;
-			break;
 		case 128:
-			ecc->layout = &nand_oob_128;
+			mtd_set_ooblayout(mtd, &nand_ooblayout_lp_ops);
 			break;
 		default:
 			pr_warn("No oob scheme defined for oobsize %d\n",
@@ -4168,7 +4217,7 @@ int nand_scan_tail(struct mtd_info *mtd)
 			ecc->write_oob = nand_write_oob_std;
 		if (!ecc->read_subpage)
 			ecc->read_subpage = nand_read_subpage;
-		if (!ecc->write_subpage)
+		if (!ecc->write_subpage && ecc->hwctl && ecc->calculate)
 			ecc->write_subpage = nand_write_subpage_hwecc;
 
 	case NAND_ECC_HW_SYNDROME:
@@ -4246,10 +4295,8 @@ int nand_scan_tail(struct mtd_info *mtd)
 		}
 
 		/* See nand_bch_init() for details. */
-		ecc->bytes = DIV_ROUND_UP(
-				ecc->strength * fls(8 * ecc->size), 8);
-		ecc->priv = nand_bch_init(mtd, ecc->size, ecc->bytes,
-					       &ecc->layout);
+		ecc->bytes = 0;
+		ecc->priv = nand_bch_init(mtd);
 		if (!ecc->priv) {
 			pr_warn("BCH ECC initialization failed!\n");
 			BUG();
@@ -4280,20 +4327,9 @@ int nand_scan_tail(struct mtd_info *mtd)
 	if (!ecc->write_oob_raw)
 		ecc->write_oob_raw = ecc->write_oob;
 
-	/*
-	 * The number of bytes available for a client to place data into
-	 * the out of band area.
-	 */
-	ecc->layout->oobavail = 0;
-	for (i = 0; ecc->layout->oobfree[i].length
-			&& i < ARRAY_SIZE(ecc->layout->oobfree); i++)
-		ecc->layout->oobavail += ecc->layout->oobfree[i].length;
-	mtd->oobavail = ecc->layout->oobavail;
-
-	/* ECC sanity check: warn if it's too weak */
-	if (!nand_ecc_strength_good(mtd))
-		pr_warn("WARNING: %s: the ECC used on your system is too weak compared to the one required by the NAND chip\n",
-			mtd->name);
+	/* propagate ecc info to mtd_info */
+	mtd->ecc_strength = ecc->strength;
+	mtd->ecc_step_size = ecc->size;
 
 	/*
 	 * Set the number of read / write steps for one page depending on ECC
@@ -4306,6 +4342,21 @@ int nand_scan_tail(struct mtd_info *mtd)
 	}
 	ecc->total = ecc->steps * ecc->bytes;
 
+	/*
+	 * The number of bytes available for a client to place data into
+	 * the out of band area.
+	 */
+	ret = mtd_ooblayout_count_freebytes(mtd);
+	if (ret < 0)
+		ret = 0;
+
+	mtd->oobavail = ret;
+
+	/* ECC sanity check: warn if it's too weak */
+	if (!nand_ecc_strength_good(mtd))
+		pr_warn("WARNING: %s: the ECC used on your system is too weak compared to the one required by the NAND chip\n",
+			mtd->name);
+
 	/* Allow subpage writes up to ecc.steps. Not possible for MLC flash */
 	if (!(chip->options & NAND_NO_SUBPAGE_WRITE) && nand_is_slc(chip)) {
 		switch (ecc->steps) {
@@ -4362,10 +4413,6 @@ int nand_scan_tail(struct mtd_info *mtd)
 	mtd->_block_markbad = nand_block_markbad;
 	mtd->writebufsize = mtd->writesize;
 
-	/* propagate ecc info to mtd_info */
-	mtd->ecclayout = ecc->layout;
-	mtd->ecc_strength = ecc->strength;
-	mtd->ecc_step_size = ecc->size;
 	/*
 	 * Initialize bitflip_threshold to its default prior scan_bbt() call.
 	 * scan_bbt() might invoke mtd_read(), thus bitflip_threshold must be
@@ -4421,7 +4468,7 @@ EXPORT_SYMBOL(nand_scan);
  */
 void nand_release(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	if (chip->ecc.mode == NAND_ECC_SOFT_BCH)
 		nand_bch_free((struct nand_bch_control *)chip->ecc.priv);
--- a/drivers/mtd/nand/nand_bbt.c
+++ b/drivers/mtd/nand/nand_bbt.c
@@ -172,7 +172,7 @@ static int read_bbt(struct mtd_info *mtd
 		struct nand_bbt_descr *td, int offs)
 {
 	int res, ret = 0, i, j, act = 0;
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	size_t retlen, len, totlen;
 	loff_t from;
 	int bits = td->options & NAND_BBT_NRBITS_MSK;
@@ -263,7 +263,7 @@ static int read_bbt(struct mtd_info *mtd
  */
 static int read_abs_bbt(struct mtd_info *mtd, uint8_t *buf, struct nand_bbt_descr *td, int chip)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int res = 0, i;
 
 	if (td->options & NAND_BBT_PERCHIP) {
@@ -388,7 +388,7 @@ static u32 bbt_get_ver_offs(struct mtd_i
 static void read_abs_bbts(struct mtd_info *mtd, uint8_t *buf,
 			  struct nand_bbt_descr *td, struct nand_bbt_descr *md)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 
 	/* Read the primary version, if available */
 	if (td->options & NAND_BBT_VERSION) {
@@ -454,7 +454,7 @@ static int scan_block_fast(struct mtd_in
 static int create_bbt(struct mtd_info *mtd, uint8_t *buf,
 	struct nand_bbt_descr *bd, int chip)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int i, numblocks, numpages;
 	int startblock;
 	loff_t from;
@@ -523,7 +523,7 @@ static int create_bbt(struct mtd_info *m
  */
 static int search_bbt(struct mtd_info *mtd, uint8_t *buf, struct nand_bbt_descr *td)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int i, chips;
 	int startblock, block, dir;
 	int scanlen = mtd->writesize + mtd->oobsize;
@@ -618,7 +618,7 @@ static int write_bbt(struct mtd_info *mt
 		     struct nand_bbt_descr *td, struct nand_bbt_descr *md,
 		     int chipsel)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	struct erase_info einfo;
 	int i, res, chip = 0;
 	int bits, startblock, dir, page, offs, numblocks, sft, sftmsk;
@@ -819,7 +819,7 @@ static int write_bbt(struct mtd_info *mt
  */
 static inline int nand_memory_bbt(struct mtd_info *mtd, struct nand_bbt_descr *bd)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 
 	return create_bbt(mtd, this->buffers->databuf, bd, -1);
 }
@@ -838,7 +838,7 @@ static inline int nand_memory_bbt(struct
 static int check_create(struct mtd_info *mtd, uint8_t *buf, struct nand_bbt_descr *bd)
 {
 	int i, chips, writeops, create, chipsel, res, res2;
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	struct nand_bbt_descr *td = this->bbt_td;
 	struct nand_bbt_descr *md = this->bbt_md;
 	struct nand_bbt_descr *rd, *rd2;
@@ -962,7 +962,7 @@ static int check_create(struct mtd_info
  */
 static void mark_bbt_region(struct mtd_info *mtd, struct nand_bbt_descr *td)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int i, j, chips, block, nrblocks, update;
 	uint8_t oldval;
 
@@ -1022,7 +1022,7 @@ static void mark_bbt_region(struct mtd_i
  */
 static void verify_bbt_descr(struct mtd_info *mtd, struct nand_bbt_descr *bd)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	u32 pattern_len;
 	u32 bits;
 	u32 table_size;
@@ -1074,7 +1074,7 @@ static void verify_bbt_descr(struct mtd_
  */
 static int nand_scan_bbt(struct mtd_info *mtd, struct nand_bbt_descr *bd)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int len, res;
 	uint8_t *buf;
 	struct nand_bbt_descr *td = this->bbt_td;
@@ -1147,7 +1147,7 @@ err:
  */
 static int nand_update_bbt(struct mtd_info *mtd, loff_t offs)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int len, res = 0;
 	int chip, chipsel;
 	uint8_t *buf;
@@ -1281,7 +1281,7 @@ static int nand_create_badblock_pattern(
  */
 int nand_default_bbt(struct mtd_info *mtd)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int ret;
 
 	/* Is a flash based bad block table requested? */
@@ -1317,7 +1317,7 @@ int nand_default_bbt(struct mtd_info *mt
  */
 int nand_isreserved_bbt(struct mtd_info *mtd, loff_t offs)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int block;
 
 	block = (int)(offs >> this->bbt_erase_shift);
@@ -1332,7 +1332,7 @@ int nand_isreserved_bbt(struct mtd_info
  */
 int nand_isbad_bbt(struct mtd_info *mtd, loff_t offs, int allowbbt)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int block, res;
 
 	block = (int)(offs >> this->bbt_erase_shift);
@@ -1359,7 +1359,7 @@ int nand_isbad_bbt(struct mtd_info *mtd,
  */
 int nand_markbad_bbt(struct mtd_info *mtd, loff_t offs)
 {
-	struct nand_chip *this = mtd->priv;
+	struct nand_chip *this = mtd_to_nand(mtd);
 	int block, ret = 0;
 
 	block = (int)(offs >> this->bbt_erase_shift);
@@ -1373,5 +1373,3 @@ int nand_markbad_bbt(struct mtd_info *mt
 
 	return ret;
 }
-
-EXPORT_SYMBOL(nand_scan_bbt);
--- a/drivers/mtd/nand/nand_bch.c
+++ b/drivers/mtd/nand/nand_bch.c
@@ -32,13 +32,11 @@
 /**
  * struct nand_bch_control - private NAND BCH control structure
  * @bch:       BCH control structure
- * @ecclayout: private ecc layout for this BCH configuration
  * @errloc:    error location array
  * @eccmask:   XOR ecc mask, allows erased pages to be decoded as valid
  */
 struct nand_bch_control {
 	struct bch_control   *bch;
-	struct nand_ecclayout ecclayout;
 	unsigned int         *errloc;
 	unsigned char        *eccmask;
 };
@@ -52,7 +50,7 @@ struct nand_bch_control {
 int nand_bch_calculate_ecc(struct mtd_info *mtd, const unsigned char *buf,
 			   unsigned char *code)
 {
-	const struct nand_chip *chip = mtd->priv;
+	const struct nand_chip *chip = mtd_to_nand(mtd);
 	struct nand_bch_control *nbc = chip->ecc.priv;
 	unsigned int i;
 
@@ -79,7 +77,7 @@ EXPORT_SYMBOL(nand_bch_calculate_ecc);
 int nand_bch_correct_data(struct mtd_info *mtd, unsigned char *buf,
 			  unsigned char *read_ecc, unsigned char *calc_ecc)
 {
-	const struct nand_chip *chip = mtd->priv;
+	const struct nand_chip *chip = mtd_to_nand(mtd);
 	struct nand_bch_control *nbc = chip->ecc.priv;
 	unsigned int *errloc = nbc->errloc;
 	int i, count;
@@ -98,7 +96,7 @@ int nand_bch_correct_data(struct mtd_inf
 		}
 	} else if (count < 0) {
 		printk(KERN_ERR "ecc unrecoverable error\n");
-		count = -1;
+		count = -EBADMSG;
 	}
 	return count;
 }
@@ -107,9 +105,6 @@ EXPORT_SYMBOL(nand_bch_correct_data);
 /**
  * nand_bch_init - [NAND Interface] Initialize NAND BCH error correction
  * @mtd:	MTD block structure
- * @eccsize:	ecc block size in bytes
- * @eccbytes:	ecc length in bytes
- * @ecclayout:	output default layout
  *
  * Returns:
  *  a pointer to a new NAND BCH control structure, or NULL upon failure
@@ -123,14 +118,20 @@ EXPORT_SYMBOL(nand_bch_correct_data);
  * @eccsize = 512  (thus, m=13 is the smallest integer such that 2^m-1 > 512*8)
  * @eccbytes = 7   (7 bytes are required to store m*t = 13*4 = 52 bits)
  */
-struct nand_bch_control *
-nand_bch_init(struct mtd_info *mtd, unsigned int eccsize, unsigned int eccbytes,
-	      struct nand_ecclayout **ecclayout)
+struct nand_bch_control *nand_bch_init(struct mtd_info *mtd)
 {
+	struct nand_chip *nand = mtd_to_nand(mtd);
 	unsigned int m, t, eccsteps, i;
-	struct nand_ecclayout *layout;
 	struct nand_bch_control *nbc = NULL;
 	unsigned char *erased_page;
+	unsigned int eccsize = nand->ecc.size;
+	unsigned int eccbytes = nand->ecc.bytes;
+	unsigned int eccstrength = nand->ecc.strength;
+
+	if (!eccbytes && eccstrength) {
+		eccbytes = DIV_ROUND_UP(eccstrength * fls(8 * eccsize), 8);
+		nand->ecc.bytes = eccbytes;
+	}
 
 	if (!eccsize || !eccbytes) {
 		printk(KERN_WARNING "ecc parameters not supplied\n");
@@ -158,7 +159,7 @@ nand_bch_init(struct mtd_info *mtd, unsi
 	eccsteps = mtd->writesize/eccsize;
 
 	/* if no ecc placement scheme was provided, build one */
-	if (!*ecclayout) {
+	if (!mtd->ooblayout) {
 
 		/* handle large page devices only */
 		if (mtd->oobsize < 64) {
@@ -167,24 +168,7 @@ nand_bch_init(struct mtd_info *mtd, unsi
 			goto fail;
 		}
 
-		layout = &nbc->ecclayout;
-		layout->eccbytes = eccsteps*eccbytes;
-
-		/* reserve 2 bytes for bad block marker */
-		if (layout->eccbytes+2 > mtd->oobsize) {
-			printk(KERN_WARNING "no suitable oob scheme available "
-			       "for oobsize %d eccbytes %u\n", mtd->oobsize,
-			       eccbytes);
-			goto fail;
-		}
-		/* put ecc bytes at oob tail */
-		for (i = 0; i < layout->eccbytes; i++)
-			layout->eccpos[i] = mtd->oobsize-layout->eccbytes+i;
-
-		layout->oobfree[0].offset = 2;
-		layout->oobfree[0].length = mtd->oobsize-2-layout->eccbytes;
-
-		*ecclayout = layout;
+		mtd_set_ooblayout(mtd, &nand_ooblayout_lp_ops);
 	}
 
 	/* sanity checks */
@@ -192,7 +176,8 @@ nand_bch_init(struct mtd_info *mtd, unsi
 		printk(KERN_WARNING "eccsize %u is too large\n", eccsize);
 		goto fail;
 	}
-	if ((*ecclayout)->eccbytes != (eccsteps*eccbytes)) {
+
+	if (mtd_ooblayout_count_eccbytes(mtd) != (eccsteps*eccbytes)) {
 		printk(KERN_WARNING "invalid ecc layout\n");
 		goto fail;
 	}
@@ -216,6 +201,9 @@ nand_bch_init(struct mtd_info *mtd, unsi
 	for (i = 0; i < eccbytes; i++)
 		nbc->eccmask[i] ^= 0xff;
 
+	if (!eccstrength)
+		nand->ecc.strength = (eccbytes * 8) / fls(8 * eccsize);
+
 	return nbc;
 fail:
 	nand_bch_free(nbc);
--- a/drivers/mtd/nand/nand_ecc.c
+++ b/drivers/mtd/nand/nand_ecc.c
@@ -424,7 +424,7 @@ int nand_calculate_ecc(struct mtd_info *
 		       unsigned char *code)
 {
 	__nand_calculate_ecc(buf,
-			((struct nand_chip *)mtd->priv)->ecc.size, code);
+			mtd_to_nand(mtd)->ecc.size, code);
 
 	return 0;
 }
@@ -524,7 +524,7 @@ int nand_correct_data(struct mtd_info *m
 		      unsigned char *read_ecc, unsigned char *calc_ecc)
 {
 	return __nand_correct_data(buf, read_ecc, calc_ecc,
-				   ((struct nand_chip *)mtd->priv)->ecc.size);
+				   mtd_to_nand(mtd)->ecc.size);
 }
 EXPORT_SYMBOL(nand_correct_data);
 
--- a/drivers/mtd/nand/nand_ids.c
+++ b/drivers/mtd/nand/nand_ids.c
@@ -50,8 +50,8 @@ struct nand_flash_dev nand_flash_ids[] =
 		  SZ_16K, SZ_8K, SZ_4M, 0, 6, 1280, NAND_ECC_INFO(40, SZ_1K) },
 	{"H27UCG8T2ATR-BC 64G 3.3V 8-bit",
 		{ .id = {0xad, 0xde, 0x94, 0xda, 0x74, 0xc4} },
-		  SZ_8K, SZ_8K, SZ_2M, 0, 6, 640, NAND_ECC_INFO(40, SZ_1K),
-		  4 },
+		  SZ_8K, SZ_8K, SZ_2M, NAND_NEED_SCRAMBLING, 6, 640,
+		  NAND_ECC_INFO(40, SZ_1K), 4 },
 
 	LEGACY_ID_NAND("NAND 4MiB 5V 8-bit",   0x6B, 4, SZ_8K, SP_OPTIONS),
 	LEGACY_ID_NAND("NAND 4MiB 3,3V 8-bit", 0xE3, 4, SZ_8K, SP_OPTIONS),
--- a/drivers/mtd/nand/nandsim.c
+++ b/drivers/mtd/nand/nandsim.c
@@ -666,8 +666,8 @@ static char *get_partition_name(int i)
  */
 static int init_nandsim(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = mtd->priv;
-	struct nandsim   *ns   = chip->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nandsim   *ns   = nand_get_controller_data(chip);
 	int i, ret = 0;
 	uint64_t remains;
 	uint64_t next_offset;
@@ -1908,7 +1908,8 @@ static void switch_state(struct nandsim
 
 static u_char ns_nand_read_byte(struct mtd_info *mtd)
 {
-	struct nandsim *ns = ((struct nand_chip *)mtd->priv)->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nandsim *ns = nand_get_controller_data(chip);
 	u_char outb = 0x00;
 
 	/* Sanity and correctness checks */
@@ -1969,7 +1970,8 @@ static u_char ns_nand_read_byte(struct m
 
 static void ns_nand_write_byte(struct mtd_info *mtd, u_char byte)
 {
-	struct nandsim *ns = ((struct nand_chip *)mtd->priv)->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nandsim *ns = nand_get_controller_data(chip);
 
 	/* Sanity and correctness checks */
 	if (!ns->lines.ce) {
@@ -2123,7 +2125,8 @@ static void ns_nand_write_byte(struct mt
 
 static void ns_hwcontrol(struct mtd_info *mtd, int cmd, unsigned int bitmask)
 {
-	struct nandsim *ns = ((struct nand_chip *)mtd->priv)->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nandsim *ns = nand_get_controller_data(chip);
 
 	ns->lines.cle = bitmask & NAND_CLE ? 1 : 0;
 	ns->lines.ale = bitmask & NAND_ALE ? 1 : 0;
@@ -2141,7 +2144,7 @@ static int ns_device_ready(struct mtd_in
 
 static uint16_t ns_nand_read_word(struct mtd_info *mtd)
 {
-	struct nand_chip *chip = (struct nand_chip *)mtd->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
 
 	NS_DBG("read_word\n");
 
@@ -2150,7 +2153,8 @@ static uint16_t ns_nand_read_word(struct
 
 static void ns_nand_write_buf(struct mtd_info *mtd, const u_char *buf, int len)
 {
-	struct nandsim *ns = ((struct nand_chip *)mtd->priv)->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nandsim *ns = nand_get_controller_data(chip);
 
 	/* Check that chip is expecting data input */
 	if (!(ns->state & STATE_DATAIN_MASK)) {
@@ -2177,7 +2181,8 @@ static void ns_nand_write_buf(struct mtd
 
 static void ns_nand_read_buf(struct mtd_info *mtd, u_char *buf, int len)
 {
-	struct nandsim *ns = ((struct nand_chip *)mtd->priv)->priv;
+	struct nand_chip *chip = mtd_to_nand(mtd);
+	struct nandsim *ns = nand_get_controller_data(chip);
 
 	/* Sanity and correctness checks */
 	if (!ns->lines.ce) {
@@ -2198,7 +2203,7 @@ static void ns_nand_read_buf(struct mtd_
 		int i;
 
 		for (i = 0; i < len; i++)
-			buf[i] = ((struct nand_chip *)mtd->priv)->read_byte(mtd);
+			buf[i] = mtd_to_nand(mtd)->read_byte(mtd);
 
 		return;
 	}
@@ -2236,16 +2241,15 @@ static int __init ns_init_module(void)
 	}
 
 	/* Allocate and initialize mtd_info, nand_chip and nandsim structures */
-	nsmtd = kzalloc(sizeof(struct mtd_info) + sizeof(struct nand_chip)
-				+ sizeof(struct nandsim), GFP_KERNEL);
-	if (!nsmtd) {
+	chip = kzalloc(sizeof(struct nand_chip) + sizeof(struct nandsim),
+		       GFP_KERNEL);
+	if (!chip) {
 		NS_ERR("unable to allocate core structures.\n");
 		return -ENOMEM;
 	}
-	chip        = (struct nand_chip *)(nsmtd + 1);
-        nsmtd->priv = (void *)chip;
+	nsmtd       = nand_to_mtd(chip);
 	nand        = (struct nandsim *)(chip + 1);
-	chip->priv  = (void *)nand;
+	nand_set_controller_data(chip, (void *)nand);
 
 	/*
 	 * Register simulator's callbacks.
@@ -2257,6 +2261,7 @@ static int __init ns_init_module(void)
 	chip->read_buf   = ns_nand_read_buf;
 	chip->read_word  = ns_nand_read_word;
 	chip->ecc.mode   = NAND_ECC_SOFT;
+	chip->ecc.algo   = NAND_ECC_HAMMING;
 	/* The NAND_SKIP_BBTSCAN option is necessary for 'overridesize' */
 	/* and 'badblocks' parameters to work */
 	chip->options   |= NAND_SKIP_BBTSCAN;
@@ -2335,6 +2340,7 @@ static int __init ns_init_module(void)
 			goto error;
 		}
 		chip->ecc.mode = NAND_ECC_SOFT_BCH;
+		chip->ecc.algo = NAND_ECC_BCH;
 		chip->ecc.size = 512;
 		chip->ecc.strength = bch;
 		chip->ecc.bytes = eccbytes;
@@ -2392,7 +2398,7 @@ err_exit:
 	for (i = 0;i < ARRAY_SIZE(nand->partitions); ++i)
 		kfree(nand->partitions[i].name);
 error:
-	kfree(nsmtd);
+	kfree(chip);
 	free_lists();
 
 	return retval;
@@ -2405,7 +2411,8 @@ module_init(ns_init_module);
  */
 static void __exit ns_cleanup_module(void)
 {
-	struct nandsim *ns = ((struct nand_chip *)nsmtd->priv)->priv;
+	struct nand_chip *chip = mtd_to_nand(nsmtd);
+	struct nandsim *ns = nand_get_controller_data(chip);
 	int i;
 
 	nandsim_debugfs_remove(ns);
@@ -2413,7 +2420,7 @@ static void __exit ns_cleanup_module(voi
 	nand_release(nsmtd); /* Unregister driver */
 	for (i = 0;i < ARRAY_SIZE(ns->partitions); ++i)
 		kfree(ns->partitions[i].name);
-	kfree(nsmtd);        /* Free other structures */
+	kfree(mtd_to_nand(nsmtd));        /* Free other structures */
 	free_lists();
 }
 
--- a/drivers/mtd/ofpart.c
+++ b/drivers/mtd/ofpart.c
@@ -26,9 +26,10 @@ static bool node_has_compatible(struct d
 }
 
 static int parse_ofpart_partitions(struct mtd_info *master,
-				   struct mtd_partition **pparts,
+				   const struct mtd_partition **pparts,
 				   struct mtd_part_parser_data *data)
 {
+	struct mtd_partition *parts;
 	struct device_node *mtd_node;
 	struct device_node *ofpart_node;
 	const char *partname;
@@ -37,10 +38,8 @@ static int parse_ofpart_partitions(struc
 	bool dedicated = true;
 
 
-	if (!data)
-		return 0;
-
-	mtd_node = data->of_node;
+	/* Pull of_node from the master device node */
+	mtd_node = mtd_get_of_node(master);
 	if (!mtd_node)
 		return 0;
 
@@ -72,8 +71,8 @@ static int parse_ofpart_partitions(struc
 	if (nr_parts == 0)
 		return 0;
 
-	*pparts = kzalloc(nr_parts * sizeof(**pparts), GFP_KERNEL);
-	if (!*pparts)
+	parts = kzalloc(nr_parts * sizeof(*parts), GFP_KERNEL);
+	if (!parts)
 		return -ENOMEM;
 
 	i = 0;
@@ -107,19 +106,19 @@ static int parse_ofpart_partitions(struc
 			goto ofpart_fail;
 		}
 
-		(*pparts)[i].offset = of_read_number(reg, a_cells);
-		(*pparts)[i].size = of_read_number(reg + a_cells, s_cells);
+		parts[i].offset = of_read_number(reg, a_cells);
+		parts[i].size = of_read_number(reg + a_cells, s_cells);
 
 		partname = of_get_property(pp, "label", &len);
 		if (!partname)
 			partname = of_get_property(pp, "name", &len);
-		(*pparts)[i].name = partname;
+		parts[i].name = partname;
 
 		if (of_get_property(pp, "read-only", &len))
-			(*pparts)[i].mask_flags |= MTD_WRITEABLE;
+			parts[i].mask_flags |= MTD_WRITEABLE;
 
 		if (of_get_property(pp, "lock", &len))
-			(*pparts)[i].mask_flags |= MTD_POWERUP_LOCK;
+			parts[i].mask_flags |= MTD_POWERUP_LOCK;
 
 		i++;
 	}
@@ -127,6 +126,7 @@ static int parse_ofpart_partitions(struc
 	if (!nr_parts)
 		goto ofpart_none;
 
+	*pparts = parts;
 	return nr_parts;
 
 ofpart_fail:
@@ -135,21 +135,20 @@ ofpart_fail:
 	ret = -EINVAL;
 ofpart_none:
 	of_node_put(pp);
-	kfree(*pparts);
-	*pparts = NULL;
+	kfree(parts);
 	return ret;
 }
 
 static struct mtd_part_parser ofpart_parser = {
-	.owner = THIS_MODULE,
 	.parse_fn = parse_ofpart_partitions,
 	.name = "ofpart",
 };
 
 static int parse_ofoldpart_partitions(struct mtd_info *master,
-				      struct mtd_partition **pparts,
+				      const struct mtd_partition **pparts,
 				      struct mtd_part_parser_data *data)
 {
+	struct mtd_partition *parts;
 	struct device_node *dp;
 	int i, plen, nr_parts;
 	const struct {
@@ -157,10 +156,8 @@ static int parse_ofoldpart_partitions(st
 	} *part;
 	const char *names;
 
-	if (!data)
-		return 0;
-
-	dp = data->of_node;
+	/* Pull of_node from the master device node */
+	dp = mtd_get_of_node(master);
 	if (!dp)
 		return 0;
 
@@ -173,37 +170,37 @@ static int parse_ofoldpart_partitions(st
 
 	nr_parts = plen / sizeof(part[0]);
 
-	*pparts = kzalloc(nr_parts * sizeof(*(*pparts)), GFP_KERNEL);
-	if (!*pparts)
+	parts = kzalloc(nr_parts * sizeof(*parts), GFP_KERNEL);
+	if (!parts)
 		return -ENOMEM;
 
 	names = of_get_property(dp, "partition-names", &plen);
 
 	for (i = 0; i < nr_parts; i++) {
-		(*pparts)[i].offset = be32_to_cpu(part->offset);
-		(*pparts)[i].size   = be32_to_cpu(part->len) & ~1;
+		parts[i].offset = be32_to_cpu(part->offset);
+		parts[i].size   = be32_to_cpu(part->len) & ~1;
 		/* bit 0 set signifies read only partition */
 		if (be32_to_cpu(part->len) & 1)
-			(*pparts)[i].mask_flags = MTD_WRITEABLE;
+			parts[i].mask_flags = MTD_WRITEABLE;
 
 		if (names && (plen > 0)) {
 			int len = strlen(names) + 1;
 
-			(*pparts)[i].name = names;
+			parts[i].name = names;
 			plen -= len;
 			names += len;
 		} else {
-			(*pparts)[i].name = "unnamed";
+			parts[i].name = "unnamed";
 		}
 
 		part++;
 	}
 
+	*pparts = parts;
 	return nr_parts;
 }
 
 static struct mtd_part_parser ofoldpart_parser = {
-	.owner = THIS_MODULE,
 	.parse_fn = parse_ofoldpart_partitions,
 	.name = "ofoldpart",
 };
--- a/drivers/mtd/spi-nor/Kconfig
+++ b/drivers/mtd/spi-nor/Kconfig
@@ -7,6 +7,14 @@ menuconfig MTD_SPI_NOR
 
 if MTD_SPI_NOR
 
+config MTD_MT81xx_NOR
+	tristate "Mediatek MT81xx SPI NOR flash controller"
+	depends on HAS_IOMEM
+	help
+	  This enables access to SPI NOR flash, using MT81xx SPI NOR flash
+	  controller. This controller does not support generic SPI BUS, it only
+	  supports SPI NOR Flash.
+
 config MTD_SPI_NOR_USE_4K_SECTORS
 	bool "Use small 4096 B erase sectors"
 	default y
@@ -23,7 +31,7 @@ config MTD_SPI_NOR_USE_4K_SECTORS
 
 config SPI_FSL_QUADSPI
 	tristate "Freescale Quad SPI controller"
-	depends on ARCH_MXC || COMPILE_TEST
+	depends on ARCH_MXC || SOC_LS1021A || ARCH_LAYERSCAPE || COMPILE_TEST
 	depends on HAS_IOMEM
 	help
 	  This enables support for the Quad SPI controller in master mode.
--- a/drivers/mtd/spi-nor/Makefile
+++ b/drivers/mtd/spi-nor/Makefile
@@ -1,3 +1,4 @@
 obj-$(CONFIG_MTD_SPI_NOR)	+= spi-nor.o
 obj-$(CONFIG_SPI_FSL_QUADSPI)	+= fsl-quadspi.o
+obj-$(CONFIG_MTD_MT81xx_NOR)    += mtk-quadspi.o
 obj-$(CONFIG_SPI_NXP_SPIFI)	+= nxp-spifi.o
--- /dev/null
+++ b/drivers/mtd/spi-nor/mtk-quadspi.c
@@ -0,0 +1,485 @@
+/*
+ * Copyright (c) 2015 MediaTek Inc.
+ * Author: Bayi Cheng <bayi.cheng@mediatek.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/device.h>
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/iopoll.h>
+#include <linux/ioport.h>
+#include <linux/math64.h>
+#include <linux/module.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mutex.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/pinctrl/consumer.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/spi-nor.h>
+
+#define MTK_NOR_CMD_REG			0x00
+#define MTK_NOR_CNT_REG			0x04
+#define MTK_NOR_RDSR_REG		0x08
+#define MTK_NOR_RDATA_REG		0x0c
+#define MTK_NOR_RADR0_REG		0x10
+#define MTK_NOR_RADR1_REG		0x14
+#define MTK_NOR_RADR2_REG		0x18
+#define MTK_NOR_WDATA_REG		0x1c
+#define MTK_NOR_PRGDATA0_REG		0x20
+#define MTK_NOR_PRGDATA1_REG		0x24
+#define MTK_NOR_PRGDATA2_REG		0x28
+#define MTK_NOR_PRGDATA3_REG		0x2c
+#define MTK_NOR_PRGDATA4_REG		0x30
+#define MTK_NOR_PRGDATA5_REG		0x34
+#define MTK_NOR_SHREG0_REG		0x38
+#define MTK_NOR_SHREG1_REG		0x3c
+#define MTK_NOR_SHREG2_REG		0x40
+#define MTK_NOR_SHREG3_REG		0x44
+#define MTK_NOR_SHREG4_REG		0x48
+#define MTK_NOR_SHREG5_REG		0x4c
+#define MTK_NOR_SHREG6_REG		0x50
+#define MTK_NOR_SHREG7_REG		0x54
+#define MTK_NOR_SHREG8_REG		0x58
+#define MTK_NOR_SHREG9_REG		0x5c
+#define MTK_NOR_CFG1_REG		0x60
+#define MTK_NOR_CFG2_REG		0x64
+#define MTK_NOR_CFG3_REG		0x68
+#define MTK_NOR_STATUS0_REG		0x70
+#define MTK_NOR_STATUS1_REG		0x74
+#define MTK_NOR_STATUS2_REG		0x78
+#define MTK_NOR_STATUS3_REG		0x7c
+#define MTK_NOR_FLHCFG_REG		0x84
+#define MTK_NOR_TIME_REG		0x94
+#define MTK_NOR_PP_DATA_REG		0x98
+#define MTK_NOR_PREBUF_STUS_REG		0x9c
+#define MTK_NOR_DELSEL0_REG		0xa0
+#define MTK_NOR_DELSEL1_REG		0xa4
+#define MTK_NOR_INTRSTUS_REG		0xa8
+#define MTK_NOR_INTREN_REG		0xac
+#define MTK_NOR_CHKSUM_CTL_REG		0xb8
+#define MTK_NOR_CHKSUM_REG		0xbc
+#define MTK_NOR_CMD2_REG		0xc0
+#define MTK_NOR_WRPROT_REG		0xc4
+#define MTK_NOR_RADR3_REG		0xc8
+#define MTK_NOR_DUAL_REG		0xcc
+#define MTK_NOR_DELSEL2_REG		0xd0
+#define MTK_NOR_DELSEL3_REG		0xd4
+#define MTK_NOR_DELSEL4_REG		0xd8
+
+/* commands for mtk nor controller */
+#define MTK_NOR_READ_CMD		0x0
+#define MTK_NOR_RDSR_CMD		0x2
+#define MTK_NOR_PRG_CMD			0x4
+#define MTK_NOR_WR_CMD			0x10
+#define MTK_NOR_PIO_WR_CMD		0x90
+#define MTK_NOR_WRSR_CMD		0x20
+#define MTK_NOR_PIO_READ_CMD		0x81
+#define MTK_NOR_WR_BUF_ENABLE		0x1
+#define MTK_NOR_WR_BUF_DISABLE		0x0
+#define MTK_NOR_ENABLE_SF_CMD		0x30
+#define MTK_NOR_DUAD_ADDR_EN		0x8
+#define MTK_NOR_QUAD_READ_EN		0x4
+#define MTK_NOR_DUAL_ADDR_EN		0x2
+#define MTK_NOR_DUAL_READ_EN		0x1
+#define MTK_NOR_DUAL_DISABLE		0x0
+#define MTK_NOR_FAST_READ		0x1
+
+#define SFLASH_WRBUF_SIZE		128
+
+/* Can shift up to 48 bits (6 bytes) of TX/RX */
+#define MTK_NOR_MAX_RX_TX_SHIFT		6
+/* can shift up to 56 bits (7 bytes) transfer by MTK_NOR_PRG_CMD */
+#define MTK_NOR_MAX_SHIFT		7
+
+/* Helpers for accessing the program data / shift data registers */
+#define MTK_NOR_PRG_REG(n)		(MTK_NOR_PRGDATA0_REG + 4 * (n))
+#define MTK_NOR_SHREG(n)		(MTK_NOR_SHREG0_REG + 4 * (n))
+
+struct mt8173_nor {
+	struct spi_nor nor;
+	struct device *dev;
+	void __iomem *base;	/* nor flash base address */
+	struct clk *spi_clk;
+	struct clk *nor_clk;
+};
+
+static void mt8173_nor_set_read_mode(struct mt8173_nor *mt8173_nor)
+{
+	struct spi_nor *nor = &mt8173_nor->nor;
+
+	switch (nor->flash_read) {
+	case SPI_NOR_FAST:
+		writeb(nor->read_opcode, mt8173_nor->base +
+		       MTK_NOR_PRGDATA3_REG);
+		writeb(MTK_NOR_FAST_READ, mt8173_nor->base +
+		       MTK_NOR_CFG1_REG);
+		break;
+	case SPI_NOR_DUAL:
+		writeb(nor->read_opcode, mt8173_nor->base +
+		       MTK_NOR_PRGDATA3_REG);
+		writeb(MTK_NOR_DUAL_READ_EN, mt8173_nor->base +
+		       MTK_NOR_DUAL_REG);
+		break;
+	case SPI_NOR_QUAD:
+		writeb(nor->read_opcode, mt8173_nor->base +
+		       MTK_NOR_PRGDATA4_REG);
+		writeb(MTK_NOR_QUAD_READ_EN, mt8173_nor->base +
+		       MTK_NOR_DUAL_REG);
+		break;
+	default:
+		writeb(MTK_NOR_DUAL_DISABLE, mt8173_nor->base +
+		       MTK_NOR_DUAL_REG);
+		break;
+	}
+}
+
+static int mt8173_nor_execute_cmd(struct mt8173_nor *mt8173_nor, u8 cmdval)
+{
+	int reg;
+	u8 val = cmdval & 0x1f;
+
+	writeb(cmdval, mt8173_nor->base + MTK_NOR_CMD_REG);
+	return readl_poll_timeout(mt8173_nor->base + MTK_NOR_CMD_REG, reg,
+				  !(reg & val), 100, 10000);
+}
+
+static int mt8173_nor_do_tx_rx(struct mt8173_nor *mt8173_nor, u8 op,
+			       u8 *tx, int txlen, u8 *rx, int rxlen)
+{
+	int len = 1 + txlen + rxlen;
+	int i, ret, idx;
+
+	if (len > MTK_NOR_MAX_SHIFT)
+		return -EINVAL;
+
+	writeb(len * 8, mt8173_nor->base + MTK_NOR_CNT_REG);
+
+	/* start at PRGDATA5, go down to PRGDATA0 */
+	idx = MTK_NOR_MAX_RX_TX_SHIFT - 1;
+
+	/* opcode */
+	writeb(op, mt8173_nor->base + MTK_NOR_PRG_REG(idx));
+	idx--;
+
+	/* program TX data */
+	for (i = 0; i < txlen; i++, idx--)
+		writeb(tx[i], mt8173_nor->base + MTK_NOR_PRG_REG(idx));
+
+	/* clear out rest of TX registers */
+	while (idx >= 0) {
+		writeb(0, mt8173_nor->base + MTK_NOR_PRG_REG(idx));
+		idx--;
+	}
+
+	ret = mt8173_nor_execute_cmd(mt8173_nor, MTK_NOR_PRG_CMD);
+	if (ret)
+		return ret;
+
+	/* restart at first RX byte */
+	idx = rxlen - 1;
+
+	/* read out RX data */
+	for (i = 0; i < rxlen; i++, idx--)
+		rx[i] = readb(mt8173_nor->base + MTK_NOR_SHREG(idx));
+
+	return 0;
+}
+
+/* Do a WRSR (Write Status Register) command */
+static int mt8173_nor_wr_sr(struct mt8173_nor *mt8173_nor, u8 sr)
+{
+	writeb(sr, mt8173_nor->base + MTK_NOR_PRGDATA5_REG);
+	writeb(8, mt8173_nor->base + MTK_NOR_CNT_REG);
+	return mt8173_nor_execute_cmd(mt8173_nor, MTK_NOR_WRSR_CMD);
+}
+
+static int mt8173_nor_write_buffer_enable(struct mt8173_nor *mt8173_nor)
+{
+	u8 reg;
+
+	/* the bit0 of MTK_NOR_CFG2_REG is pre-fetch buffer
+	 * 0: pre-fetch buffer use for read
+	 * 1: pre-fetch buffer use for page program
+	 */
+	writel(MTK_NOR_WR_BUF_ENABLE, mt8173_nor->base + MTK_NOR_CFG2_REG);
+	return readb_poll_timeout(mt8173_nor->base + MTK_NOR_CFG2_REG, reg,
+				  0x01 == (reg & 0x01), 100, 10000);
+}
+
+static int mt8173_nor_write_buffer_disable(struct mt8173_nor *mt8173_nor)
+{
+	u8 reg;
+
+	writel(MTK_NOR_WR_BUF_DISABLE, mt8173_nor->base + MTK_NOR_CFG2_REG);
+	return readb_poll_timeout(mt8173_nor->base + MTK_NOR_CFG2_REG, reg,
+				  MTK_NOR_WR_BUF_DISABLE == (reg & 0x1), 100,
+				  10000);
+}
+
+static void mt8173_nor_set_addr(struct mt8173_nor *mt8173_nor, u32 addr)
+{
+	int i;
+
+	for (i = 0; i < 3; i++) {
+		writeb(addr & 0xff, mt8173_nor->base + MTK_NOR_RADR0_REG + i * 4);
+		addr >>= 8;
+	}
+	/* Last register is non-contiguous */
+	writeb(addr & 0xff, mt8173_nor->base + MTK_NOR_RADR3_REG);
+}
+
+static int mt8173_nor_read(struct spi_nor *nor, loff_t from, size_t length,
+			   size_t *retlen, u_char *buffer)
+{
+	int i, ret;
+	int addr = (int)from;
+	u8 *buf = (u8 *)buffer;
+	struct mt8173_nor *mt8173_nor = nor->priv;
+
+	/* set mode for fast read mode ,dual mode or quad mode */
+	mt8173_nor_set_read_mode(mt8173_nor);
+	mt8173_nor_set_addr(mt8173_nor, addr);
+
+	for (i = 0; i < length; i++, (*retlen)++) {
+		ret = mt8173_nor_execute_cmd(mt8173_nor, MTK_NOR_PIO_READ_CMD);
+		if (ret < 0)
+			return ret;
+		buf[i] = readb(mt8173_nor->base + MTK_NOR_RDATA_REG);
+	}
+	return 0;
+}
+
+static int mt8173_nor_write_single_byte(struct mt8173_nor *mt8173_nor,
+					int addr, int length, u8 *data)
+{
+	int i, ret;
+
+	mt8173_nor_set_addr(mt8173_nor, addr);
+
+	for (i = 0; i < length; i++) {
+		writeb(*data++, mt8173_nor->base + MTK_NOR_WDATA_REG);
+		ret = mt8173_nor_execute_cmd(mt8173_nor, MTK_NOR_PIO_WR_CMD);
+		if (ret < 0)
+			return ret;
+	}
+	return 0;
+}
+
+static int mt8173_nor_write_buffer(struct mt8173_nor *mt8173_nor, int addr,
+				   const u8 *buf)
+{
+	int i, bufidx, data;
+
+	mt8173_nor_set_addr(mt8173_nor, addr);
+
+	bufidx = 0;
+	for (i = 0; i < SFLASH_WRBUF_SIZE; i += 4) {
+		data = buf[bufidx + 3]<<24 | buf[bufidx + 2]<<16 |
+		       buf[bufidx + 1]<<8 | buf[bufidx];
+		bufidx += 4;
+		writel(data, mt8173_nor->base + MTK_NOR_PP_DATA_REG);
+	}
+	return mt8173_nor_execute_cmd(mt8173_nor, MTK_NOR_WR_CMD);
+}
+
+static void mt8173_nor_write(struct spi_nor *nor, loff_t to, size_t len,
+			     size_t *retlen, const u_char *buf)
+{
+	int ret;
+	struct mt8173_nor *mt8173_nor = nor->priv;
+
+	ret = mt8173_nor_write_buffer_enable(mt8173_nor);
+	if (ret < 0)
+		dev_warn(mt8173_nor->dev, "write buffer enable failed!\n");
+
+	while (len >= SFLASH_WRBUF_SIZE) {
+		ret = mt8173_nor_write_buffer(mt8173_nor, to, buf);
+		if (ret < 0)
+			dev_err(mt8173_nor->dev, "write buffer failed!\n");
+		len -= SFLASH_WRBUF_SIZE;
+		to += SFLASH_WRBUF_SIZE;
+		buf += SFLASH_WRBUF_SIZE;
+		(*retlen) += SFLASH_WRBUF_SIZE;
+	}
+	ret = mt8173_nor_write_buffer_disable(mt8173_nor);
+	if (ret < 0)
+		dev_warn(mt8173_nor->dev, "write buffer disable failed!\n");
+
+	if (len) {
+		ret = mt8173_nor_write_single_byte(mt8173_nor, to, (int)len,
+						   (u8 *)buf);
+		if (ret < 0)
+			dev_err(mt8173_nor->dev, "write single byte failed!\n");
+		(*retlen) += len;
+	}
+}
+
+static int mt8173_nor_read_reg(struct spi_nor *nor, u8 opcode, u8 *buf, int len)
+{
+	int ret;
+	struct mt8173_nor *mt8173_nor = nor->priv;
+
+	switch (opcode) {
+	case SPINOR_OP_RDSR:
+		ret = mt8173_nor_execute_cmd(mt8173_nor, MTK_NOR_RDSR_CMD);
+		if (ret < 0)
+			return ret;
+		if (len == 1)
+			*buf = readb(mt8173_nor->base + MTK_NOR_RDSR_REG);
+		else
+			dev_err(mt8173_nor->dev, "len should be 1 for read status!\n");
+		break;
+	default:
+		ret = mt8173_nor_do_tx_rx(mt8173_nor, opcode, NULL, 0, buf, len);
+		break;
+	}
+	return ret;
+}
+
+static int mt8173_nor_write_reg(struct spi_nor *nor, u8 opcode, u8 *buf,
+				int len)
+{
+	int ret;
+	struct mt8173_nor *mt8173_nor = nor->priv;
+
+	switch (opcode) {
+	case SPINOR_OP_WRSR:
+		/* We only handle 1 byte */
+		ret = mt8173_nor_wr_sr(mt8173_nor, *buf);
+		break;
+	default:
+		ret = mt8173_nor_do_tx_rx(mt8173_nor, opcode, buf, len, NULL, 0);
+		if (ret)
+			dev_warn(mt8173_nor->dev, "write reg failure!\n");
+		break;
+	}
+	return ret;
+}
+
+static int mtk_nor_init(struct mt8173_nor *mt8173_nor,
+			struct device_node *flash_node)
+{
+	int ret;
+	struct spi_nor *nor;
+
+	/* initialize controller to accept commands */
+	writel(MTK_NOR_ENABLE_SF_CMD, mt8173_nor->base + MTK_NOR_WRPROT_REG);
+
+	nor = &mt8173_nor->nor;
+	nor->dev = mt8173_nor->dev;
+	nor->priv = mt8173_nor;
+	spi_nor_set_flash_node(nor, flash_node);
+
+	/* fill the hooks to spi nor */
+	nor->read = mt8173_nor_read;
+	nor->read_reg = mt8173_nor_read_reg;
+	nor->write = mt8173_nor_write;
+	nor->write_reg = mt8173_nor_write_reg;
+	nor->mtd.name = "mtk_nor";
+	/* initialized with NULL */
+	ret = spi_nor_scan(nor, NULL, SPI_NOR_DUAL);
+	if (ret)
+		return ret;
+
+	return mtd_device_register(&nor->mtd, NULL, 0);
+}
+
+static int mtk_nor_drv_probe(struct platform_device *pdev)
+{
+	struct device_node *flash_np;
+	struct resource *res;
+	int ret;
+	struct mt8173_nor *mt8173_nor;
+
+	if (!pdev->dev.of_node) {
+		dev_err(&pdev->dev, "No DT found\n");
+		return -EINVAL;
+	}
+
+	mt8173_nor = devm_kzalloc(&pdev->dev, sizeof(*mt8173_nor), GFP_KERNEL);
+	if (!mt8173_nor)
+		return -ENOMEM;
+	platform_set_drvdata(pdev, mt8173_nor);
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	mt8173_nor->base = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(mt8173_nor->base))
+		return PTR_ERR(mt8173_nor->base);
+
+	mt8173_nor->spi_clk = devm_clk_get(&pdev->dev, "spi");
+	if (IS_ERR(mt8173_nor->spi_clk))
+		return PTR_ERR(mt8173_nor->spi_clk);
+
+	mt8173_nor->nor_clk = devm_clk_get(&pdev->dev, "sf");
+	if (IS_ERR(mt8173_nor->nor_clk))
+		return PTR_ERR(mt8173_nor->nor_clk);
+
+	mt8173_nor->dev = &pdev->dev;
+	ret = clk_prepare_enable(mt8173_nor->spi_clk);
+	if (ret)
+		return ret;
+
+	ret = clk_prepare_enable(mt8173_nor->nor_clk);
+	if (ret) {
+		clk_disable_unprepare(mt8173_nor->spi_clk);
+		return ret;
+	}
+	/* only support one attached flash */
+	flash_np = of_get_next_available_child(pdev->dev.of_node, NULL);
+	if (!flash_np) {
+		dev_err(&pdev->dev, "no SPI flash device to configure\n");
+		ret = -ENODEV;
+		goto nor_free;
+	}
+	ret = mtk_nor_init(mt8173_nor, flash_np);
+
+nor_free:
+	if (ret) {
+		clk_disable_unprepare(mt8173_nor->spi_clk);
+		clk_disable_unprepare(mt8173_nor->nor_clk);
+	}
+	return ret;
+}
+
+static int mtk_nor_drv_remove(struct platform_device *pdev)
+{
+	struct mt8173_nor *mt8173_nor = platform_get_drvdata(pdev);
+
+	clk_disable_unprepare(mt8173_nor->spi_clk);
+	clk_disable_unprepare(mt8173_nor->nor_clk);
+	return 0;
+}
+
+static const struct of_device_id mtk_nor_of_ids[] = {
+	{ .compatible = "mediatek,mt8173-nor"},
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, mtk_nor_of_ids);
+
+static struct platform_driver mtk_nor_driver = {
+	.probe = mtk_nor_drv_probe,
+	.remove = mtk_nor_drv_remove,
+	.driver = {
+		.name = "mtk-nor",
+		.of_match_table = mtk_nor_of_ids,
+	},
+};
+
+module_platform_driver(mtk_nor_driver);
+MODULE_LICENSE("GPL v2");
+MODULE_DESCRIPTION("MediaTek SPI NOR Flash Driver");
--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -38,6 +38,7 @@
 #define CHIP_ERASE_2MB_READY_WAIT_JIFFIES	(40UL * HZ)
 
 #define SPI_NOR_MAX_ID_LEN	6
+#define SPI_NOR_MAX_ADDR_WIDTH	4
 
 struct flash_info {
 	char		*name;
@@ -60,14 +61,20 @@ struct flash_info {
 	u16		addr_width;
 
 	u16		flags;
-#define	SECT_4K			0x01	/* SPINOR_OP_BE_4K works uniformly */
-#define	SPI_NOR_NO_ERASE	0x02	/* No erase command needed */
-#define	SST_WRITE		0x04	/* use SST byte programming */
-#define	SPI_NOR_NO_FR		0x08	/* Can't do fastread */
-#define	SECT_4K_PMC		0x10	/* SPINOR_OP_BE_4K_PMC works uniformly */
-#define	SPI_NOR_DUAL_READ	0x20    /* Flash supports Dual Read */
-#define	SPI_NOR_QUAD_READ	0x40    /* Flash supports Quad Read */
-#define	USE_FSR			0x80	/* use flag status register */
+#define SECT_4K			BIT(0)	/* SPINOR_OP_BE_4K works uniformly */
+#define SPI_NOR_NO_ERASE	BIT(1)	/* No erase command needed */
+#define SST_WRITE		BIT(2)	/* use SST byte programming */
+#define SPI_NOR_NO_FR		BIT(3)	/* Can't do fastread */
+#define SECT_4K_PMC		BIT(4)	/* SPINOR_OP_BE_4K_PMC works uniformly */
+#define SPI_NOR_DUAL_READ	BIT(5)	/* Flash supports Dual Read */
+#define SPI_NOR_QUAD_READ	BIT(6)	/* Flash supports Quad Read */
+#define USE_FSR			BIT(7)	/* use flag status register */
+#define SPI_NOR_HAS_LOCK	BIT(8)	/* Flash supports lock/unlock via SR */
+#define SPI_NOR_HAS_TB		BIT(9)	/*
+					 * Flash SR has Top/Bottom (TB) protect
+					 * bit. Must be used with
+					 * SPI_NOR_HAS_LOCK.
+					 */
 };
 
 #define JEDEC_MFR(info)	((info)->id[0])
@@ -313,6 +320,29 @@ static void spi_nor_unlock_and_unprep(st
 }
 
 /*
+ * Initiate the erasure of a single sector
+ */
+static int spi_nor_erase_sector(struct spi_nor *nor, u32 addr)
+{
+	u8 buf[SPI_NOR_MAX_ADDR_WIDTH];
+	int i;
+
+	if (nor->erase)
+		return nor->erase(nor, addr);
+
+	/*
+	 * Default implementation, if driver doesn't have a specialized HW
+	 * control
+	 */
+	for (i = nor->addr_width - 1; i >= 0; i--) {
+		buf[i] = addr & 0xff;
+		addr >>= 8;
+	}
+
+	return nor->write_reg(nor, nor->erase_opcode, buf, nor->addr_width);
+}
+
+/*
  * Erase an address range on the nor chip.  The address range may extend
  * one or more erase sectors.  Return an error is there is a problem erasing.
  */
@@ -371,10 +401,9 @@ static int spi_nor_erase(struct mtd_info
 		while (len) {
 			write_enable(nor);
 
-			if (nor->erase(nor, addr)) {
-				ret = -EIO;
+			ret = spi_nor_erase_sector(nor, addr);
+			if (ret)
 				goto erase_err;
-			}
 
 			addr += mtd->erasesize;
 			len -= mtd->erasesize;
@@ -387,17 +416,13 @@ static int spi_nor_erase(struct mtd_info
 
 	write_disable(nor);
 
+erase_err:
 	spi_nor_unlock_and_unprep(nor, SPI_NOR_OPS_ERASE);
 
-	instr->state = MTD_ERASE_DONE;
+	instr->state = ret ? MTD_ERASE_FAILED : MTD_ERASE_DONE;
 	mtd_erase_callback(instr);
 
 	return ret;
-
-erase_err:
-	spi_nor_unlock_and_unprep(nor, SPI_NOR_OPS_ERASE);
-	instr->state = MTD_ERASE_FAILED;
-	return ret;
 }
 
 static void stm_get_locked_range(struct spi_nor *nor, u8 sr, loff_t *ofs,
@@ -415,32 +440,58 @@ static void stm_get_locked_range(struct
 	} else {
 		pow = ((sr & mask) ^ mask) >> shift;
 		*len = mtd->size >> pow;
-		*ofs = mtd->size - *len;
+		if (nor->flags & SNOR_F_HAS_SR_TB && sr & SR_TB)
+			*ofs = 0;
+		else
+			*ofs = mtd->size - *len;
 	}
 }
 
 /*
- * Return 1 if the entire region is locked, 0 otherwise
+ * Return 1 if the entire region is locked (if @locked is true) or unlocked (if
+ * @locked is false); 0 otherwise
  */
-static int stm_is_locked_sr(struct spi_nor *nor, loff_t ofs, uint64_t len,
-			    u8 sr)
+static int stm_check_lock_status_sr(struct spi_nor *nor, loff_t ofs, uint64_t len,
+				    u8 sr, bool locked)
 {
 	loff_t lock_offs;
 	uint64_t lock_len;
 
+	if (!len)
+		return 1;
+
 	stm_get_locked_range(nor, sr, &lock_offs, &lock_len);
 
-	return (ofs + len <= lock_offs + lock_len) && (ofs >= lock_offs);
+	if (locked)
+		/* Requested range is a sub-range of locked range */
+		return (ofs + len <= lock_offs + lock_len) && (ofs >= lock_offs);
+	else
+		/* Requested range does not overlap with locked range */
+		return (ofs >= lock_offs + lock_len) || (ofs + len <= lock_offs);
+}
+
+static int stm_is_locked_sr(struct spi_nor *nor, loff_t ofs, uint64_t len,
+			    u8 sr)
+{
+	return stm_check_lock_status_sr(nor, ofs, len, sr, true);
+}
+
+static int stm_is_unlocked_sr(struct spi_nor *nor, loff_t ofs, uint64_t len,
+			      u8 sr)
+{
+	return stm_check_lock_status_sr(nor, ofs, len, sr, false);
 }
 
 /*
  * Lock a region of the flash. Compatible with ST Micro and similar flash.
- * Supports only the block protection bits BP{0,1,2} in the status register
+ * Supports the block protection bits BP{0,1,2} in the status register
  * (SR). Does not support these features found in newer SR bitfields:
- *   - TB: top/bottom protect - only handle TB=0 (top protect)
  *   - SEC: sector/block protect - only handle SEC=0 (block protect)
  *   - CMP: complement protect - only support CMP=0 (range is not complemented)
  *
+ * Support for the following is provided conditionally for some flash:
+ *   - TB: top/bottom protect
+ *
  * Sample table portion for 8MB flash (Winbond w25q64fw):
  *
  *   SEC  |  TB   |  BP2  |  BP1  |  BP0  |  Prot Length  | Protected Portion
@@ -453,26 +504,55 @@ static int stm_is_locked_sr(struct spi_n
  *    0   |   0   |   1   |   0   |   1   |  2 MB         | Upper 1/4
  *    0   |   0   |   1   |   1   |   0   |  4 MB         | Upper 1/2
  *    X   |   X   |   1   |   1   |   1   |  8 MB         | ALL
+ *  ------|-------|-------|-------|-------|---------------|-------------------
+ *    0   |   1   |   0   |   0   |   1   |  128 KB       | Lower 1/64
+ *    0   |   1   |   0   |   1   |   0   |  256 KB       | Lower 1/32
+ *    0   |   1   |   0   |   1   |   1   |  512 KB       | Lower 1/16
+ *    0   |   1   |   1   |   0   |   0   |  1 MB         | Lower 1/8
+ *    0   |   1   |   1   |   0   |   1   |  2 MB         | Lower 1/4
+ *    0   |   1   |   1   |   1   |   0   |  4 MB         | Lower 1/2
  *
  * Returns negative on errors, 0 on success.
  */
 static int stm_lock(struct spi_nor *nor, loff_t ofs, uint64_t len)
 {
 	struct mtd_info *mtd = &nor->mtd;
-	u8 status_old, status_new;
+	int status_old, status_new;
 	u8 mask = SR_BP2 | SR_BP1 | SR_BP0;
 	u8 shift = ffs(mask) - 1, pow, val;
+	loff_t lock_len;
+	bool can_be_top = true, can_be_bottom = nor->flags & SNOR_F_HAS_SR_TB;
+	bool use_top;
+	int ret;
 
 	status_old = read_sr(nor);
+	if (status_old < 0)
+		return status_old;
 
-	/* SPI NOR always locks to the end */
-	if (ofs + len != mtd->size) {
-		/* Does combined region extend to end? */
-		if (!stm_is_locked_sr(nor, ofs + len, mtd->size - ofs - len,
-				      status_old))
-			return -EINVAL;
-		len = mtd->size - ofs;
-	}
+	/* If nothing in our range is unlocked, we don't need to do anything */
+	if (stm_is_locked_sr(nor, ofs, len, status_old))
+		return 0;
+
+	/* If anything below us is unlocked, we can't use 'bottom' protection */
+	if (!stm_is_locked_sr(nor, 0, ofs, status_old))
+		can_be_bottom = false;
+
+	/* If anything above us is unlocked, we can't use 'top' protection */
+	if (!stm_is_locked_sr(nor, ofs + len, mtd->size - (ofs + len),
+				status_old))
+		can_be_top = false;
+
+	if (!can_be_bottom && !can_be_top)
+		return -EINVAL;
+
+	/* Prefer top, if both are valid */
+	use_top = can_be_top;
+
+	/* lock_len: length of region that should end up locked */
+	if (use_top)
+		lock_len = mtd->size - ofs;
+	else
+		lock_len = ofs + len;
 
 	/*
 	 * Need smallest pow such that:
@@ -483,7 +563,7 @@ static int stm_lock(struct spi_nor *nor,
 	 *
 	 *   pow = ceil(log2(size / len)) = log2(size) - floor(log2(len))
 	 */
-	pow = ilog2(mtd->size) - ilog2(len);
+	pow = ilog2(mtd->size) - ilog2(lock_len);
 	val = mask - (pow << shift);
 	if (val & ~mask)
 		return -EINVAL;
@@ -491,14 +571,27 @@ static int stm_lock(struct spi_nor *nor,
 	if (!(val & mask))
 		return -EINVAL;
 
-	status_new = (status_old & ~mask) | val;
+	status_new = (status_old & ~mask & ~SR_TB) | val;
+
+	/* Disallow further writes if WP pin is asserted */
+	status_new |= SR_SRWD;
+
+	if (!use_top)
+		status_new |= SR_TB;
+
+	/* Don't bother if they're the same */
+	if (status_new == status_old)
+		return 0;
 
 	/* Only modify protection if it will not unlock other areas */
-	if ((status_new & mask) <= (status_old & mask))
+	if ((status_new & mask) < (status_old & mask))
 		return -EINVAL;
 
 	write_enable(nor);
-	return write_sr(nor, status_new);
+	ret = write_sr(nor, status_new);
+	if (ret)
+		return ret;
+	return spi_nor_wait_till_ready(nor);
 }
 
 /*
@@ -509,17 +602,43 @@ static int stm_lock(struct spi_nor *nor,
 static int stm_unlock(struct spi_nor *nor, loff_t ofs, uint64_t len)
 {
 	struct mtd_info *mtd = &nor->mtd;
-	uint8_t status_old, status_new;
+	int status_old, status_new;
 	u8 mask = SR_BP2 | SR_BP1 | SR_BP0;
 	u8 shift = ffs(mask) - 1, pow, val;
+	loff_t lock_len;
+	bool can_be_top = true, can_be_bottom = nor->flags & SNOR_F_HAS_SR_TB;
+	bool use_top;
+	int ret;
 
 	status_old = read_sr(nor);
+	if (status_old < 0)
+		return status_old;
+
+	/* If nothing in our range is locked, we don't need to do anything */
+	if (stm_is_unlocked_sr(nor, ofs, len, status_old))
+		return 0;
+
+	/* If anything below us is locked, we can't use 'top' protection */
+	if (!stm_is_unlocked_sr(nor, 0, ofs, status_old))
+		can_be_top = false;
+
+	/* If anything above us is locked, we can't use 'bottom' protection */
+	if (!stm_is_unlocked_sr(nor, ofs + len, mtd->size - (ofs + len),
+				status_old))
+		can_be_bottom = false;
 
-	/* Cannot unlock; would unlock larger region than requested */
-	if (stm_is_locked_sr(nor, ofs - mtd->erasesize, mtd->erasesize,
-			     status_old))
+	if (!can_be_bottom && !can_be_top)
 		return -EINVAL;
 
+	/* Prefer top, if both are valid */
+	use_top = can_be_top;
+
+	/* lock_len: length of region that should remain locked */
+	if (use_top)
+		lock_len = mtd->size - (ofs + len);
+	else
+		lock_len = ofs;
+
 	/*
 	 * Need largest pow such that:
 	 *
@@ -529,8 +648,8 @@ static int stm_unlock(struct spi_nor *no
 	 *
 	 *   pow = floor(log2(size / len)) = log2(size) - ceil(log2(len))
 	 */
-	pow = ilog2(mtd->size) - order_base_2(mtd->size - (ofs + len));
-	if (ofs + len == mtd->size) {
+	pow = ilog2(mtd->size) - order_base_2(lock_len);
+	if (lock_len == 0) {
 		val = 0; /* fully unlocked */
 	} else {
 		val = mask - (pow << shift);
@@ -539,14 +658,28 @@ static int stm_unlock(struct spi_nor *no
 			return -EINVAL;
 	}
 
-	status_new = (status_old & ~mask) | val;
+	status_new = (status_old & ~mask & ~SR_TB) | val;
+
+	/* Don't protect status register if we're fully unlocked */
+	if (lock_len == mtd->size)
+		status_new &= ~SR_SRWD;
+
+	if (!use_top)
+		status_new |= SR_TB;
+
+	/* Don't bother if they're the same */
+	if (status_new == status_old)
+		return 0;
 
 	/* Only modify protection if it will not lock other areas */
-	if ((status_new & mask) >= (status_old & mask))
+	if ((status_new & mask) > (status_old & mask))
 		return -EINVAL;
 
 	write_enable(nor);
-	return write_sr(nor, status_new);
+	ret = write_sr(nor, status_new);
+	if (ret)
+		return ret;
+	return spi_nor_wait_till_ready(nor);
 }
 
 /*
@@ -715,9 +848,9 @@ static const struct flash_info spi_nor_i
 	{ "mx25l4005a",  INFO(0xc22013, 0, 64 * 1024,   8, SECT_4K) },
 	{ "mx25l8005",   INFO(0xc22014, 0, 64 * 1024,  16, 0) },
 	{ "mx25l1606e",  INFO(0xc22015, 0, 64 * 1024,  32, SECT_4K) },
-	{ "mx25l3205d",  INFO(0xc22016, 0, 64 * 1024,  64, 0) },
+	{ "mx25l3205d",  INFO(0xc22016, 0, 64 * 1024,  64, SECT_4K) },
 	{ "mx25l3255e",  INFO(0xc29e16, 0, 64 * 1024,  64, SECT_4K) },
-	{ "mx25l6405d",  INFO(0xc22017, 0, 64 * 1024, 128, 0) },
+	{ "mx25l6405d",  INFO(0xc22017, 0, 64 * 1024, 128, SECT_4K) },
 	{ "mx25u6435f",  INFO(0xc22537, 0, 64 * 1024, 128, SECT_4K) },
 	{ "mx25l12805d", INFO(0xc22018, 0, 64 * 1024, 256, 0) },
 	{ "mx25l12855e", INFO(0xc22618, 0, 64 * 1024, 256, 0) },
@@ -732,8 +865,8 @@ static const struct flash_info spi_nor_i
 	{ "n25q032a",	 INFO(0x20bb16, 0, 64 * 1024,   64, SPI_NOR_QUAD_READ) },
 	{ "n25q064",     INFO(0x20ba17, 0, 64 * 1024,  128, SECT_4K | SPI_NOR_QUAD_READ) },
 	{ "n25q064a",    INFO(0x20bb17, 0, 64 * 1024,  128, SECT_4K | SPI_NOR_QUAD_READ) },
-	{ "n25q128a11",  INFO(0x20bb18, 0, 64 * 1024,  256, SPI_NOR_QUAD_READ) },
-	{ "n25q128a13",  INFO(0x20ba18, 0, 64 * 1024,  256, SPI_NOR_QUAD_READ) },
+	{ "n25q128a11",  INFO(0x20bb18, 0, 64 * 1024,  256, SECT_4K | SPI_NOR_QUAD_READ) },
+	{ "n25q128a13",  INFO(0x20ba18, 0, 64 * 1024,  256, SECT_4K | SPI_NOR_QUAD_READ) },
 	{ "n25q256a",    INFO(0x20ba19, 0, 64 * 1024,  512, SECT_4K | SPI_NOR_QUAD_READ) },
 	{ "n25q512a",    INFO(0x20bb20, 0, 64 * 1024, 1024, SECT_4K | USE_FSR | SPI_NOR_QUAD_READ) },
 	{ "n25q512ax3",  INFO(0x20ba20, 0, 64 * 1024, 1024, SECT_4K | USE_FSR | SPI_NOR_QUAD_READ) },
@@ -767,6 +900,7 @@ static const struct flash_info spi_nor_i
 	{ "s25fl008k",  INFO(0xef4014,      0,  64 * 1024,  16, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ "s25fl016k",  INFO(0xef4015,      0,  64 * 1024,  32, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ "s25fl064k",  INFO(0xef4017,      0,  64 * 1024, 128, SECT_4K) },
+	{ "s25fl116k",  INFO(0x014015,      0,  64 * 1024,  32, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ "s25fl132k",  INFO(0x014016,      0,  64 * 1024,  64, SECT_4K) },
 	{ "s25fl164k",  INFO(0x014017,      0,  64 * 1024, 128, SECT_4K) },
 	{ "s25fl204k",  INFO(0x014013,      0,  64 * 1024,   8, SECT_4K | SPI_NOR_DUAL_READ) },
@@ -830,11 +964,23 @@ static const struct flash_info spi_nor_i
 	{ "w25x16", INFO(0xef3015, 0, 64 * 1024,  32, SECT_4K) },
 	{ "w25x32", INFO(0xef3016, 0, 64 * 1024,  64, SECT_4K) },
 	{ "w25q32", INFO(0xef4016, 0, 64 * 1024,  64, SECT_4K) },
-	{ "w25q32dw", INFO(0xef6016, 0, 64 * 1024,  64, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+	{
+		"w25q32dw", INFO(0xef6016, 0, 64 * 1024,  64,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
 	{ "w25x64", INFO(0xef3017, 0, 64 * 1024, 128, SECT_4K) },
 	{ "w25q64", INFO(0xef4017, 0, 64 * 1024, 128, SECT_4K) },
-	{ "w25q64dw", INFO(0xef6017, 0, 64 * 1024, 128, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
-	{ "w25q128fw", INFO(0xef6018, 0, 64 * 1024, 256, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+	{
+		"w25q64dw", INFO(0xef6017, 0, 64 * 1024, 128,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
+	{
+		"w25q128fw", INFO(0xef6018, 0, 64 * 1024, 256,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
 	{ "w25q80", INFO(0xef5014, 0, 64 * 1024,  16, SECT_4K) },
 	{ "w25q80bl", INFO(0xef4014, 0, 64 * 1024,  16, SECT_4K) },
 	{ "w25q128", INFO(0xef4018, 0, 64 * 1024, 256, SECT_4K) },
@@ -857,7 +1003,7 @@ static const struct flash_info *spi_nor_
 
 	tmp = nor->read_reg(nor, SPINOR_OP_RDID, id, SPI_NOR_MAX_ID_LEN);
 	if (tmp < 0) {
-		dev_dbg(nor->dev, " error %d reading JEDEC ID\n", tmp);
+		dev_dbg(nor->dev, "error %d reading JEDEC ID\n", tmp);
 		return ERR_PTR(tmp);
 	}
 
@@ -868,7 +1014,7 @@ static const struct flash_info *spi_nor_
 				return &spi_nor_ids[tmp];
 		}
 	}
-	dev_err(nor->dev, "unrecognized JEDEC id bytes: %02x, %2x, %2x\n",
+	dev_err(nor->dev, "unrecognized JEDEC id bytes: %02x, %02x, %02x\n",
 		id[0], id[1], id[2]);
 	return ERR_PTR(-ENODEV);
 }
@@ -1014,6 +1160,8 @@ static int macronix_quad_enable(struct s
 	int ret, val;
 
 	val = read_sr(nor);
+	if (val < 0)
+		return val;
 	write_enable(nor);
 
 	write_sr(nor, val | SR_QUAD_EN_MX);
@@ -1095,7 +1243,7 @@ static int set_quad_mode(struct spi_nor
 static int spi_nor_check(struct spi_nor *nor)
 {
 	if (!nor->dev || !nor->read || !nor->write ||
-		!nor->read_reg || !nor->write_reg || !nor->erase) {
+		!nor->read_reg || !nor->write_reg) {
 		pr_err("spi-nor: please fill all the necessary fields!\n");
 		return -EINVAL;
 	}
@@ -1108,7 +1256,7 @@ int spi_nor_scan(struct spi_nor *nor, co
 	const struct flash_info *info = NULL;
 	struct device *dev = nor->dev;
 	struct mtd_info *mtd = &nor->mtd;
-	struct device_node *np = nor->flash_node;
+	struct device_node *np = spi_nor_get_flash_node(nor);
 	int ret;
 	int i;
 
@@ -1158,9 +1306,11 @@ int spi_nor_scan(struct spi_nor *nor, co
 	if (JEDEC_MFR(info) == SNOR_MFR_ATMEL ||
 	    JEDEC_MFR(info) == SNOR_MFR_INTEL ||
 	    JEDEC_MFR(info) == SNOR_MFR_MACRONIX ||
-	    JEDEC_MFR(info) == SNOR_MFR_SST) {
+	    JEDEC_MFR(info) == SNOR_MFR_SST ||
+	    info->flags & SPI_NOR_HAS_LOCK) {
 		write_enable(nor);
 		write_sr(nor, 0);
+		spi_nor_wait_till_ready(nor);
 	}
 
 	if (!mtd->name)
@@ -1174,7 +1324,8 @@ int spi_nor_scan(struct spi_nor *nor, co
 	mtd->_read = spi_nor_read;
 
 	/* NOR protection support for STmicro/Micron chips and similar */
-	if (JEDEC_MFR(info) == SNOR_MFR_MICRON) {
+	if (JEDEC_MFR(info) == SNOR_MFR_MICRON ||
+			info->flags & SPI_NOR_HAS_LOCK) {
 		nor->flash_lock = stm_lock;
 		nor->flash_unlock = stm_unlock;
 		nor->flash_is_locked = stm_is_locked;
@@ -1194,6 +1345,8 @@ int spi_nor_scan(struct spi_nor *nor, co
 
 	if (info->flags & USE_FSR)
 		nor->flags |= SNOR_F_USE_FSR;
+	if (info->flags & SPI_NOR_HAS_TB)
+		nor->flags |= SNOR_F_HAS_SR_TB;
 
 #ifdef CONFIG_MTD_SPI_NOR_USE_4K_SECTORS
 	/* prefer "small sector" erase if possible */
@@ -1296,6 +1449,12 @@ int spi_nor_scan(struct spi_nor *nor, co
 		nor->addr_width = 3;
 	}
 
+	if (nor->addr_width > SPI_NOR_MAX_ADDR_WIDTH) {
+		dev_err(dev, "address width is too large: %u\n",
+			nor->addr_width);
+		return -EINVAL;
+	}
+
 	nor->read_dummy = spi_nor_read_dummy_cycles(nor);
 
 	dev_info(dev, "%s (%lld Kbytes)\n", info->name,
--- a/drivers/mtd/tests/mtd_nandecctest.c
+++ b/drivers/mtd/tests/mtd_nandecctest.c
@@ -187,7 +187,7 @@ static int double_bit_error_detect(void
 	__nand_calculate_ecc(error_data, size, calc_ecc);
 	ret = __nand_correct_data(error_data, error_ecc, calc_ecc, size);
 
-	return (ret == -1) ? 0 : -EINVAL;
+	return (ret == -EBADMSG) ? 0 : -EINVAL;
 }
 
 static const struct nand_ecc_test nand_ecc_test[] = {
--- a/drivers/mtd/tests/oobtest.c
+++ b/drivers/mtd/tests/oobtest.c
@@ -215,19 +215,19 @@ static int verify_eraseblock(int ebnum)
 			pr_info("ignoring error as within bitflip_limit\n");
 		}
 
-		if (use_offset != 0 || use_len < mtd->ecclayout->oobavail) {
+		if (use_offset != 0 || use_len < mtd->oobavail) {
 			int k;
 
 			ops.mode      = MTD_OPS_AUTO_OOB;
 			ops.len       = 0;
 			ops.retlen    = 0;
-			ops.ooblen    = mtd->ecclayout->oobavail;
+			ops.ooblen    = mtd->oobavail;
 			ops.oobretlen = 0;
 			ops.ooboffs   = 0;
 			ops.datbuf    = NULL;
 			ops.oobbuf    = readbuf;
 			err = mtd_read_oob(mtd, addr, &ops);
-			if (err || ops.oobretlen != mtd->ecclayout->oobavail) {
+			if (err || ops.oobretlen != mtd->oobavail) {
 				pr_err("error: readoob failed at %#llx\n",
 						(long long)addr);
 				errcnt += 1;
@@ -244,7 +244,7 @@ static int verify_eraseblock(int ebnum)
 			/* verify post-(use_offset + use_len) area for 0xff */
 			k = use_offset + use_len;
 			bitflips += memffshow(addr, k, readbuf + k,
-					      mtd->ecclayout->oobavail - k);
+					      mtd->oobavail - k);
 
 			if (bitflips > bitflip_limit) {
 				pr_err("error: verify failed at %#llx\n",
@@ -269,8 +269,8 @@ static int verify_eraseblock_in_one_go(i
 	struct mtd_oob_ops ops;
 	int err = 0;
 	loff_t addr = (loff_t)ebnum * mtd->erasesize;
-	size_t len = mtd->ecclayout->oobavail * pgcnt;
-	size_t oobavail = mtd->ecclayout->oobavail;
+	size_t len = mtd->oobavail * pgcnt;
+	size_t oobavail = mtd->oobavail;
 	size_t bitflips;
 	int i;
 
@@ -394,8 +394,8 @@ static int __init mtd_oobtest_init(void)
 		goto out;
 
 	use_offset = 0;
-	use_len = mtd->ecclayout->oobavail;
-	use_len_max = mtd->ecclayout->oobavail;
+	use_len = mtd->oobavail;
+	use_len_max = mtd->oobavail;
 	vary_offset = 0;
 
 	/* First test: write all OOB, read it back and verify */
@@ -460,8 +460,8 @@ static int __init mtd_oobtest_init(void)
 
 	/* Write all eraseblocks */
 	use_offset = 0;
-	use_len = mtd->ecclayout->oobavail;
-	use_len_max = mtd->ecclayout->oobavail;
+	use_len = mtd->oobavail;
+	use_len_max = mtd->oobavail;
 	vary_offset = 1;
 	prandom_seed_state(&rnd_state, 5);
 
@@ -471,8 +471,8 @@ static int __init mtd_oobtest_init(void)
 
 	/* Check all eraseblocks */
 	use_offset = 0;
-	use_len = mtd->ecclayout->oobavail;
-	use_len_max = mtd->ecclayout->oobavail;
+	use_len = mtd->oobavail;
+	use_len_max = mtd->oobavail;
 	vary_offset = 1;
 	prandom_seed_state(&rnd_state, 5);
 	err = verify_all_eraseblocks();
@@ -480,8 +480,8 @@ static int __init mtd_oobtest_init(void)
 		goto out;
 
 	use_offset = 0;
-	use_len = mtd->ecclayout->oobavail;
-	use_len_max = mtd->ecclayout->oobavail;
+	use_len = mtd->oobavail;
+	use_len_max = mtd->oobavail;
 	vary_offset = 0;
 
 	/* Fourth test: try to write off end of device */
@@ -501,7 +501,7 @@ static int __init mtd_oobtest_init(void)
 	ops.retlen    = 0;
 	ops.ooblen    = 1;
 	ops.oobretlen = 0;
-	ops.ooboffs   = mtd->ecclayout->oobavail;
+	ops.ooboffs   = mtd->oobavail;
 	ops.datbuf    = NULL;
 	ops.oobbuf    = writebuf;
 	pr_info("attempting to start write past end of OOB\n");
@@ -521,7 +521,7 @@ static int __init mtd_oobtest_init(void)
 	ops.retlen    = 0;
 	ops.ooblen    = 1;
 	ops.oobretlen = 0;
-	ops.ooboffs   = mtd->ecclayout->oobavail;
+	ops.ooboffs   = mtd->oobavail;
 	ops.datbuf    = NULL;
 	ops.oobbuf    = readbuf;
 	pr_info("attempting to start read past end of OOB\n");
@@ -543,7 +543,7 @@ static int __init mtd_oobtest_init(void)
 		ops.mode      = MTD_OPS_AUTO_OOB;
 		ops.len       = 0;
 		ops.retlen    = 0;
-		ops.ooblen    = mtd->ecclayout->oobavail + 1;
+		ops.ooblen    = mtd->oobavail + 1;
 		ops.oobretlen = 0;
 		ops.ooboffs   = 0;
 		ops.datbuf    = NULL;
@@ -563,7 +563,7 @@ static int __init mtd_oobtest_init(void)
 		ops.mode      = MTD_OPS_AUTO_OOB;
 		ops.len       = 0;
 		ops.retlen    = 0;
-		ops.ooblen    = mtd->ecclayout->oobavail + 1;
+		ops.ooblen    = mtd->oobavail + 1;
 		ops.oobretlen = 0;
 		ops.ooboffs   = 0;
 		ops.datbuf    = NULL;
@@ -587,7 +587,7 @@ static int __init mtd_oobtest_init(void)
 		ops.mode      = MTD_OPS_AUTO_OOB;
 		ops.len       = 0;
 		ops.retlen    = 0;
-		ops.ooblen    = mtd->ecclayout->oobavail;
+		ops.ooblen    = mtd->oobavail;
 		ops.oobretlen = 0;
 		ops.ooboffs   = 1;
 		ops.datbuf    = NULL;
@@ -607,7 +607,7 @@ static int __init mtd_oobtest_init(void)
 		ops.mode      = MTD_OPS_AUTO_OOB;
 		ops.len       = 0;
 		ops.retlen    = 0;
-		ops.ooblen    = mtd->ecclayout->oobavail;
+		ops.ooblen    = mtd->oobavail;
 		ops.oobretlen = 0;
 		ops.ooboffs   = 1;
 		ops.datbuf    = NULL;
@@ -638,7 +638,7 @@ static int __init mtd_oobtest_init(void)
 	for (i = 0; i < ebcnt - 1; ++i) {
 		int cnt = 2;
 		int pg;
-		size_t sz = mtd->ecclayout->oobavail;
+		size_t sz = mtd->oobavail;
 		if (bbt[i] || bbt[i + 1])
 			continue;
 		addr = (loff_t)(i + 1) * mtd->erasesize - mtd->writesize;
@@ -673,13 +673,12 @@ static int __init mtd_oobtest_init(void)
 	for (i = 0; i < ebcnt - 1; ++i) {
 		if (bbt[i] || bbt[i + 1])
 			continue;
-		prandom_bytes_state(&rnd_state, writebuf,
-					mtd->ecclayout->oobavail * 2);
+		prandom_bytes_state(&rnd_state, writebuf, mtd->oobavail * 2);
 		addr = (loff_t)(i + 1) * mtd->erasesize - mtd->writesize;
 		ops.mode      = MTD_OPS_AUTO_OOB;
 		ops.len       = 0;
 		ops.retlen    = 0;
-		ops.ooblen    = mtd->ecclayout->oobavail * 2;
+		ops.ooblen    = mtd->oobavail * 2;
 		ops.oobretlen = 0;
 		ops.ooboffs   = 0;
 		ops.datbuf    = NULL;
@@ -688,7 +687,7 @@ static int __init mtd_oobtest_init(void)
 		if (err)
 			goto out;
 		if (memcmpshow(addr, readbuf, writebuf,
-			       mtd->ecclayout->oobavail * 2)) {
+			       mtd->oobavail * 2)) {
 			pr_err("error: verify failed at %#llx\n",
 			       (long long)addr);
 			errcnt += 1;
--- a/drivers/mtd/tests/pagetest.c
+++ b/drivers/mtd/tests/pagetest.c
@@ -127,13 +127,12 @@ static int crosstest(void)
 	unsigned char *pp1, *pp2, *pp3, *pp4;
 
 	pr_info("crosstest\n");
-	pp1 = kmalloc(pgsize * 4, GFP_KERNEL);
+	pp1 = kzalloc(pgsize * 4, GFP_KERNEL);
 	if (!pp1)
 		return -ENOMEM;
 	pp2 = pp1 + pgsize;
 	pp3 = pp2 + pgsize;
 	pp4 = pp3 + pgsize;
-	memset(pp1, 0, pgsize * 4);
 
 	addr0 = 0;
 	for (i = 0; i < ebcnt && bbt[i]; ++i)
--- a/include/linux/mtd/bbm.h
+++ b/include/linux/mtd/bbm.h
@@ -166,7 +166,6 @@ struct bbm_info {
 };
 
 /* OneNAND BBT interface */
-extern int onenand_scan_bbt(struct mtd_info *mtd, struct nand_bbt_descr *bd);
 extern int onenand_default_bbt(struct mtd_info *mtd);
 
 #endif	/* __LINUX_MTD_BBM_H */
--- a/include/linux/mtd/fsmc.h
+++ b/include/linux/mtd/fsmc.h
@@ -103,24 +103,6 @@
 
 #define FSMC_BUSY_WAIT_TIMEOUT	(1 * HZ)
 
-/*
- * There are 13 bytes of ecc for every 512 byte block in FSMC version 8
- * and it has to be read consecutively and immediately after the 512
- * byte data block for hardware to generate the error bit offsets
- * Managing the ecc bytes in the following way is easier. This way is
- * similar to oobfree structure maintained already in u-boot nand driver
- */
-#define MAX_ECCPLACE_ENTRIES	32
-
-struct fsmc_nand_eccplace {
-	uint8_t offset;
-	uint8_t length;
-};
-
-struct fsmc_eccplace {
-	struct fsmc_nand_eccplace eccplace[MAX_ECCPLACE_ENTRIES];
-};
-
 struct fsmc_nand_timings {
 	uint8_t tclr;
 	uint8_t tar;
--- a/include/linux/mtd/inftl.h
+++ b/include/linux/mtd/inftl.h
@@ -44,7 +44,6 @@ struct INFTLrecord {
 	unsigned int nb_blocks;		/* number of physical blocks */
 	unsigned int nb_boot_blocks;	/* number of blocks used by the bios */
 	struct erase_info instr;
-	struct nand_ecclayout oobinfo;
 };
 
 int INFTL_mount(struct INFTLrecord *s);
--- a/include/linux/mtd/map.h
+++ b/include/linux/mtd/map.h
@@ -142,7 +142,9 @@
 #endif
 
 #ifndef map_bankwidth
+#ifdef CONFIG_MTD
 #warning "No CONFIG_MTD_MAP_BANK_WIDTH_xx selected. No NOR chip support can work"
+#endif
 static inline int map_bankwidth(void *map)
 {
 	BUG();
@@ -238,8 +240,11 @@ struct map_info {
 	   If there is no cache to care about this can be set to NULL. */
 	void (*inval_cache)(struct map_info *, unsigned long, ssize_t);
 
-	/* set_vpp() must handle being reentered -- enable, enable, disable
-	   must leave it enabled. */
+	/* This will be called with 1 as parameter when the first map user
+	 * needs VPP, and called with 0 when the last user exits. The map
+	 * core maintains a reference counter, and assumes that VPP is a
+	 * global resource applying to all mapped flash chips on the system.
+	 */
 	void (*set_vpp)(struct map_info *, int);
 
 	unsigned long pfow_base;
--- a/include/linux/mtd/mtd.h
+++ b/include/linux/mtd/mtd.h
@@ -100,17 +100,35 @@ struct mtd_oob_ops {
 
 #define MTD_MAX_OOBFREE_ENTRIES_LARGE	32
 #define MTD_MAX_ECCPOS_ENTRIES_LARGE	640
+/**
+ * struct mtd_oob_region - oob region definition
+ * @offset: region offset
+ * @length: region length
+ *
+ * This structure describes a region of the OOB area, and is used
+ * to retrieve ECC or free bytes sections.
+ * Each section is defined by an offset within the OOB area and a
+ * length.
+ */
+struct mtd_oob_region {
+	u32 offset;
+	u32 length;
+};
+
 /*
- * Internal ECC layout control structure. For historical reasons, there is a
- * similar, smaller struct nand_ecclayout_user (in mtd-abi.h) that is retained
- * for export to user-space via the ECCGETLAYOUT ioctl.
- * nand_ecclayout should be expandable in the future simply by the above macros.
+ * struct mtd_ooblayout_ops - NAND OOB layout operations
+ * @ecc: function returning an ECC region in the OOB area.
+ *	 Should return -ERANGE if %section exceeds the total number of
+ *	 ECC sections.
+ * @free: function returning a free region in the OOB area.
+ *	  Should return -ERANGE if %section exceeds the total number of
+ *	  free sections.
  */
-struct nand_ecclayout {
-	__u32 eccbytes;
-	__u32 eccpos[MTD_MAX_ECCPOS_ENTRIES_LARGE];
-	__u32 oobavail;
-	struct nand_oobfree oobfree[MTD_MAX_OOBFREE_ENTRIES_LARGE];
+struct mtd_ooblayout_ops {
+	int (*ecc)(struct mtd_info *mtd, int section,
+		   struct mtd_oob_region *oobecc);
+	int (*free)(struct mtd_info *mtd, int section,
+		    struct mtd_oob_region *oobfree);
 };
 
 struct module;	/* only needed for owner field in mtd_info */
@@ -171,8 +189,8 @@ struct mtd_info {
 	const char *name;
 	int index;
 
-	/* ECC layout structure pointer - read only! */
-	struct nand_ecclayout *ecclayout;
+	/* OOB layout description */
+	const struct mtd_ooblayout_ops *ooblayout;
 
 	/* the ecc step size. */
 	unsigned int ecc_step_size;
@@ -258,6 +276,46 @@ struct mtd_info {
 	int usecount;
 };
 
+int mtd_ooblayout_ecc(struct mtd_info *mtd, int section,
+		      struct mtd_oob_region *oobecc);
+int mtd_ooblayout_find_eccregion(struct mtd_info *mtd, int eccbyte,
+				 int *section,
+				 struct mtd_oob_region *oobregion);
+int mtd_ooblayout_get_eccbytes(struct mtd_info *mtd, u8 *eccbuf,
+			       const u8 *oobbuf, int start, int nbytes);
+int mtd_ooblayout_set_eccbytes(struct mtd_info *mtd, const u8 *eccbuf,
+			       u8 *oobbuf, int start, int nbytes);
+int mtd_ooblayout_free(struct mtd_info *mtd, int section,
+		       struct mtd_oob_region *oobfree);
+int mtd_ooblayout_get_databytes(struct mtd_info *mtd, u8 *databuf,
+				const u8 *oobbuf, int start, int nbytes);
+int mtd_ooblayout_set_databytes(struct mtd_info *mtd, const u8 *databuf,
+				u8 *oobbuf, int start, int nbytes);
+int mtd_ooblayout_count_freebytes(struct mtd_info *mtd);
+int mtd_ooblayout_count_eccbytes(struct mtd_info *mtd);
+
+static inline void mtd_set_ooblayout(struct mtd_info *mtd,
+				     const struct mtd_ooblayout_ops *ooblayout)
+{
+	mtd->ooblayout = ooblayout;
+}
+
+static inline void mtd_set_of_node(struct mtd_info *mtd,
+				   struct device_node *np)
+{
+	mtd->dev.of_node = np;
+}
+
+static inline struct device_node *mtd_get_of_node(struct mtd_info *mtd)
+{
+	return mtd->dev.of_node;
+}
+
+static inline int mtd_oobavail(struct mtd_info *mtd, struct mtd_oob_ops *ops)
+{
+	return ops->mode == MTD_OPS_AUTO_OOB ? mtd->oobavail : mtd->oobsize;
+}
+
 int mtd_erase(struct mtd_info *mtd, struct erase_info *instr);
 int mtd_point(struct mtd_info *mtd, loff_t from, size_t len, size_t *retlen,
 	      void **virt, resource_size_t *phys);
--- a/include/linux/mtd/nand.h
+++ b/include/linux/mtd/nand.h
@@ -119,6 +119,12 @@ typedef enum {
 	NAND_ECC_SOFT_BCH,
 } nand_ecc_modes_t;
 
+enum nand_ecc_algo {
+	NAND_ECC_UNKNOWN,
+	NAND_ECC_HAMMING,
+	NAND_ECC_BCH,
+};
+
 /*
  * Constants for Hardware ECC
  */
@@ -129,6 +135,14 @@ typedef enum {
 /* Enable Hardware ECC before syndrome is read back from flash */
 #define NAND_ECC_READSYN	2
 
+/*
+ * Enable generic NAND 'page erased' check. This check is only done when
+ * ecc.correct() returns -EBADMSG.
+ * Set this flag if your implementation does not fix bitflips in erased
+ * pages and you want to rely on the default implementation.
+ */
+#define NAND_ECC_GENERIC_ERASED_CHECK	BIT(0)
+
 /* Bit mask for flags passed to do_nand_read_ecc */
 #define NAND_GET_DEVICE		0x80
 
@@ -160,6 +174,12 @@ typedef enum {
 /* Device supports subpage reads */
 #define NAND_SUBPAGE_READ	0x00001000
 
+/*
+ * Some MLC NANDs need data scrambling to limit bitflips caused by repeated
+ * patterns.
+ */
+#define NAND_NEED_SCRAMBLING	0x00002000
+
 /* Options valid for Samsung large page devices */
 #define NAND_SAMSUNG_LP_OPTIONS NAND_CACHEPRG
 
@@ -276,15 +296,15 @@ struct nand_onfi_params {
 	__le16 t_r;
 	__le16 t_ccs;
 	__le16 src_sync_timing_mode;
-	__le16 src_ssync_features;
+	u8 src_ssync_features;
 	__le16 clk_pin_capacitance_typ;
 	__le16 io_pin_capacitance_typ;
 	__le16 input_pin_capacitance_typ;
 	u8 input_pin_capacitance_max;
 	u8 driver_strength_support;
 	__le16 t_int_r;
-	__le16 t_ald;
-	u8 reserved4[7];
+	__le16 t_adl;
+	u8 reserved4[8];
 
 	/* vendor */
 	__le16 vendor_revision;
@@ -407,7 +427,7 @@ struct nand_jedec_params {
 	__le16 input_pin_capacitance_typ;
 	__le16 clk_pin_capacitance_typ;
 	u8 driver_strength_support;
-	__le16 t_ald;
+	__le16 t_adl;
 	u8 reserved4[36];
 
 	/* ECC and endurance block */
@@ -444,6 +464,7 @@ struct nand_hw_control {
 /**
  * struct nand_ecc_ctrl - Control structure for ECC
  * @mode:	ECC mode
+ * @algo:	ECC algorithm
  * @steps:	number of ECC steps per page
  * @size:	data bytes per ECC step
  * @bytes:	ECC bytes per step
@@ -451,12 +472,18 @@ struct nand_hw_control {
  * @total:	total number of ECC bytes per page
  * @prepad:	padding information for syndrome based ECC generators
  * @postpad:	padding information for syndrome based ECC generators
- * @layout:	ECC layout control struct pointer
+ * @options:	ECC specific options (see NAND_ECC_XXX flags defined above)
  * @priv:	pointer to private ECC control data
  * @hwctl:	function to control hardware ECC generator. Must only
  *		be provided if an hardware ECC is available
  * @calculate:	function for ECC calculation or readback from ECC hardware
- * @correct:	function for ECC correction, matching to ECC generator (sw/hw)
+ * @correct:	function for ECC correction, matching to ECC generator (sw/hw).
+ *		Should return a positive number representing the number of
+ *		corrected bitflips, -EBADMSG if the number of bitflips exceed
+ *		ECC strength, or any other error code if the error is not
+ *		directly related to correction.
+ *		If -EBADMSG is returned the input buffers should be left
+ *		untouched.
  * @read_page_raw:	function to read a raw page without ECC. This function
  *			should hide the specific layout used by the ECC
  *			controller and always return contiguous in-band and
@@ -487,6 +514,7 @@ struct nand_hw_control {
  */
 struct nand_ecc_ctrl {
 	nand_ecc_modes_t mode;
+	enum nand_ecc_algo algo;
 	int steps;
 	int size;
 	int bytes;
@@ -494,7 +522,7 @@ struct nand_ecc_ctrl {
 	int strength;
 	int prepad;
 	int postpad;
-	struct nand_ecclayout	*layout;
+	unsigned int options;
 	void *priv;
 	void (*hwctl)(struct mtd_info *mtd, int mode);
 	int (*calculate)(struct mtd_info *mtd, const uint8_t *dat,
@@ -540,11 +568,11 @@ struct nand_buffers {
 
 /**
  * struct nand_chip - NAND Private Flash Chip Data
+ * @mtd:		MTD device registered to the MTD framework
  * @IO_ADDR_R:		[BOARDSPECIFIC] address to read the 8 I/O lines of the
  *			flash device
  * @IO_ADDR_W:		[BOARDSPECIFIC] address to write the 8 I/O lines of the
  *			flash device.
- * @flash_node:		[BOARDSPECIFIC] device node describing this instance
  * @read_byte:		[REPLACEABLE] read one byte from the chip
  * @read_word:		[REPLACEABLE] read one word from the chip
  * @write_byte:		[REPLACEABLE] write a single byte to the chip on the
@@ -640,18 +668,17 @@ struct nand_buffers {
  */
 
 struct nand_chip {
+	struct mtd_info mtd;
 	void __iomem *IO_ADDR_R;
 	void __iomem *IO_ADDR_W;
 
-	struct device_node *flash_node;
-
 	uint8_t (*read_byte)(struct mtd_info *mtd);
 	u16 (*read_word)(struct mtd_info *mtd);
 	void (*write_byte)(struct mtd_info *mtd, uint8_t byte);
 	void (*write_buf)(struct mtd_info *mtd, const uint8_t *buf, int len);
 	void (*read_buf)(struct mtd_info *mtd, uint8_t *buf, int len);
 	void (*select_chip)(struct mtd_info *mtd, int chip);
-	int (*block_bad)(struct mtd_info *mtd, loff_t ofs, int getchip);
+	int (*block_bad)(struct mtd_info *mtd, loff_t ofs);
 	int (*block_markbad)(struct mtd_info *mtd, loff_t ofs);
 	void (*cmd_ctrl)(struct mtd_info *mtd, int dat, unsigned int ctrl);
 	int (*dev_ready)(struct mtd_info *mtd);
@@ -719,6 +746,40 @@ struct nand_chip {
 	void *priv;
 };
 
+extern const struct mtd_ooblayout_ops nand_ooblayout_sp_ops;
+extern const struct mtd_ooblayout_ops nand_ooblayout_lp_ops;
+
+static inline void nand_set_flash_node(struct nand_chip *chip,
+				       struct device_node *np)
+{
+	mtd_set_of_node(&chip->mtd, np);
+}
+
+static inline struct device_node *nand_get_flash_node(struct nand_chip *chip)
+{
+	return mtd_get_of_node(&chip->mtd);
+}
+
+static inline struct nand_chip *mtd_to_nand(struct mtd_info *mtd)
+{
+	return container_of(mtd, struct nand_chip, mtd);
+}
+
+static inline struct mtd_info *nand_to_mtd(struct nand_chip *chip)
+{
+	return &chip->mtd;
+}
+
+static inline void *nand_get_controller_data(struct nand_chip *chip)
+{
+	return chip->priv;
+}
+
+static inline void nand_set_controller_data(struct nand_chip *chip, void *priv)
+{
+	chip->priv = priv;
+}
+
 /*
  * NAND Flash Manufacturer ID Codes
  */
@@ -850,7 +911,6 @@ extern int nand_do_read(struct mtd_info
  * @chip_delay:		R/B delay value in us
  * @options:		Option flags, e.g. 16bit buswidth
  * @bbt_options:	BBT option flags, e.g. NAND_BBT_USE_FLASH
- * @ecclayout:		ECC layout info structure
  * @part_probe_types:	NULL-terminated array of probe types
  */
 struct platform_nand_chip {
@@ -858,7 +918,6 @@ struct platform_nand_chip {
 	int chip_offset;
 	int nr_partitions;
 	struct mtd_partition *partitions;
-	struct nand_ecclayout *ecclayout;
 	int chip_delay;
 	unsigned int options;
 	unsigned int bbt_options;
@@ -908,15 +967,6 @@ struct platform_nand_data {
 	struct platform_nand_ctrl ctrl;
 };
 
-/* Some helpers to access the data structures */
-static inline
-struct platform_nand_chip *get_platform_nandchip(struct mtd_info *mtd)
-{
-	struct nand_chip *chip = mtd->priv;
-
-	return chip->priv;
-}
-
 /* return the supported features. */
 static inline int onfi_feature(struct nand_chip *chip)
 {
--- a/include/linux/mtd/nand_bch.h
+++ b/include/linux/mtd/nand_bch.h
@@ -32,9 +32,7 @@ int nand_bch_correct_data(struct mtd_inf
 /*
  * Initialize BCH encoder/decoder
  */
-struct nand_bch_control *
-nand_bch_init(struct mtd_info *mtd, unsigned int eccsize,
-	      unsigned int eccbytes, struct nand_ecclayout **ecclayout);
+struct nand_bch_control *nand_bch_init(struct mtd_info *mtd);
 /*
  * Release BCH encoder/decoder resources
  */
@@ -55,12 +53,10 @@ static inline int
 nand_bch_correct_data(struct mtd_info *mtd, unsigned char *buf,
 		      unsigned char *read_ecc, unsigned char *calc_ecc)
 {
-	return -1;
+	return -ENOTSUPP;
 }
 
-static inline struct nand_bch_control *
-nand_bch_init(struct mtd_info *mtd, unsigned int eccsize,
-	      unsigned int eccbytes, struct nand_ecclayout **ecclayout)
+static inline struct nand_bch_control *nand_bch_init(struct mtd_info *mtd)
 {
 	return NULL;
 }
--- a/include/linux/mtd/nftl.h
+++ b/include/linux/mtd/nftl.h
@@ -50,7 +50,6 @@ struct NFTLrecord {
         unsigned int nb_blocks;		/* number of physical blocks */
         unsigned int nb_boot_blocks;	/* number of blocks used by the bios */
         struct erase_info instr;
-	struct nand_ecclayout oobinfo;
 };
 
 int NFTL_mount(struct NFTLrecord *s);
--- a/include/linux/mtd/onenand.h
+++ b/include/linux/mtd/onenand.h
@@ -80,7 +80,6 @@ struct onenand_bufferram {
  * @page_buf:		[INTERN] page main data buffer
  * @oob_buf:		[INTERN] page oob data buffer
  * @subpagesize:	[INTERN] holds the subpagesize
- * @ecclayout:		[REPLACEABLE] the default ecc placement scheme
  * @bbm:		[REPLACEABLE] pointer to Bad Block Management
  * @priv:		[OPTIONAL] pointer to private chip date
  */
@@ -134,7 +133,6 @@ struct onenand_chip {
 #endif
 
 	int			subpagesize;
-	struct nand_ecclayout	*ecclayout;
 
 	void			*bbm;
 
--- a/include/linux/mtd/partitions.h
+++ b/include/linux/mtd/partitions.h
@@ -42,7 +42,6 @@ struct mtd_partition {
 	uint64_t size;			/* partition size */
 	uint64_t offset;		/* offset within the master MTD space */
 	uint32_t mask_flags;		/* master MTD flags to mask out for this partition */
-	struct nand_ecclayout *ecclayout;	/* out of band layout for this partition (NAND only) */
 };
 
 #define MTDPART_OFS_RETAIN	(-3)
@@ -56,11 +55,9 @@ struct device_node;
 /**
  * struct mtd_part_parser_data - used to pass data to MTD partition parsers.
  * @origin: for RedBoot, start address of MTD device
- * @of_node: for OF parsers, device node containing partitioning information
  */
 struct mtd_part_parser_data {
 	unsigned long origin;
-	struct device_node *of_node;
 };
 
 
@@ -78,14 +75,34 @@ struct mtd_part_parser {
 	struct list_head list;
 	struct module *owner;
 	const char *name;
-	int (*parse_fn)(struct mtd_info *, struct mtd_partition **,
+	int (*parse_fn)(struct mtd_info *, const struct mtd_partition **,
 			struct mtd_part_parser_data *);
+	void (*cleanup)(const struct mtd_partition *pparts, int nr_parts);
 	enum mtd_parser_type type;
 };
 
-extern void register_mtd_parser(struct mtd_part_parser *parser);
+/* Container for passing around a set of parsed partitions */
+struct mtd_partitions {
+	const struct mtd_partition *parts;
+	int nr_parts;
+	const struct mtd_part_parser *parser;
+};
+
+extern int __register_mtd_parser(struct mtd_part_parser *parser,
+				 struct module *owner);
+#define register_mtd_parser(parser) __register_mtd_parser(parser, THIS_MODULE)
+
 extern void deregister_mtd_parser(struct mtd_part_parser *parser);
 
+/*
+ * module_mtd_part_parser() - Helper macro for MTD partition parsers that don't
+ * do anything special in module init/exit. Each driver may only use this macro
+ * once, and calling it replaces module_init() and module_exit().
+ */
+#define module_mtd_part_parser(__mtd_part_parser) \
+	module_driver(__mtd_part_parser, register_mtd_parser, \
+		      deregister_mtd_parser)
+
 int mtd_is_partition(const struct mtd_info *mtd);
 int mtd_add_partition(struct mtd_info *master, const char *name,
 		      long long offset, long long length);
--- a/include/linux/mtd/sh_flctl.h
+++ b/include/linux/mtd/sh_flctl.h
@@ -143,11 +143,11 @@ enum flctl_ecc_res_t {
 struct dma_chan;
 
 struct sh_flctl {
-	struct mtd_info		mtd;
 	struct nand_chip	chip;
 	struct platform_device	*pdev;
 	struct dev_pm_qos_request pm_qos;
 	void __iomem		*reg;
+	resource_size_t		fifo;
 
 	uint8_t	done_buff[2048 + 64];	/* max size 2048 + 64 */
 	int	read_bytes;
@@ -186,7 +186,7 @@ struct sh_flctl_platform_data {
 
 static inline struct sh_flctl *mtd_to_flctl(struct mtd_info *mtdinfo)
 {
-	return container_of(mtdinfo, struct sh_flctl, mtd);
+	return container_of(mtd_to_nand(mtdinfo), struct sh_flctl, chip);
 }
 
 #endif	/* __SH_FLCTL_H__ */
--- a/include/linux/mtd/sharpsl.h
+++ b/include/linux/mtd/sharpsl.h
@@ -14,7 +14,7 @@
 
 struct sharpsl_nand_platform_data {
 	struct nand_bbt_descr	*badblock_pattern;
-	struct nand_ecclayout	*ecc_layout;
+	const struct mtd_ooblayout_ops *ecc_layout;
 	struct mtd_partition	*partitions;
 	unsigned int		nr_partitions;
 };
--- a/include/uapi/mtd/mtd-abi.h
+++ b/include/uapi/mtd/mtd-abi.h
@@ -228,7 +228,7 @@ struct nand_oobfree {
  * complete set of ECC information. The ioctl truncates the larger internal
  * structure to retain binary compatibility with the static declaration of the
  * ioctl. Note that the "MTD_MAX_..._ENTRIES" macros represent the max size of
- * the user struct, not the MAX size of the internal struct nand_ecclayout.
+ * the user struct, not the MAX size of the internal OOB layout representation.
  */
 struct nand_ecclayout_user {
 	__u32 eccbytes;
--- a/fs/jffs2/wbuf.c
+++ b/fs/jffs2/wbuf.c
@@ -1153,7 +1153,7 @@ static struct jffs2_sb_info *work_to_sb(
 {
 	struct delayed_work *dwork;
 
-	dwork = container_of(work, struct delayed_work, work);
+	dwork = to_delayed_work(work);
 	return container_of(dwork, struct jffs2_sb_info, wbuf_dwork);
 }
 
@@ -1183,22 +1183,20 @@ void jffs2_dirty_trigger(struct jffs2_sb
 
 int jffs2_nand_flash_setup(struct jffs2_sb_info *c)
 {
-	struct nand_ecclayout *oinfo = c->mtd->ecclayout;
-
 	if (!c->mtd->oobsize)
 		return 0;
 
 	/* Cleanmarker is out-of-band, so inline size zero */
 	c->cleanmarker_size = 0;
 
-	if (!oinfo || oinfo->oobavail == 0) {
+	if (c->mtd->oobavail == 0) {
 		pr_err("inconsistent device description\n");
 		return -EINVAL;
 	}
 
 	jffs2_dbg(1, "using OOB on NAND\n");
 
-	c->oobavail = oinfo->oobavail;
+	c->oobavail = c->mtd->oobavail;
 
 	/* Initialise write buffer */
 	init_rwsem(&c->wbuf_sem);
--- a/include/linux/mtd/spi-nor.h
+++ b/include/linux/mtd/spi-nor.h
@@ -85,6 +85,7 @@
 #define SR_BP0			BIT(2)	/* Block protect 0 */
 #define SR_BP1			BIT(3)	/* Block protect 1 */
 #define SR_BP2			BIT(4)	/* Block protect 2 */
+#define SR_TB			BIT(5)	/* Top/Bottom protect */
 #define SR_SRWD			BIT(7)	/* SR write protect */
 
 #define SR_QUAD_EN_MX		BIT(6)	/* Macronix Quad I/O */
@@ -116,6 +117,7 @@ enum spi_nor_ops {
 
 enum spi_nor_option_flags {
 	SNOR_F_USE_FSR		= BIT(0),
+	SNOR_F_HAS_SR_TB	= BIT(1),
 };
 
 /**
@@ -123,7 +125,6 @@ enum spi_nor_option_flags {
  * @mtd:		point to a mtd_info structure
  * @lock:		the lock for the read/write/erase/lock/unlock operations
  * @dev:		point to a spi device, or a spi nor controller device.
- * @flash_node:		point to a device node describing this flash instance.
  * @page_size:		the page size of the SPI NOR
  * @addr_width:		number of address bytes
  * @erase_opcode:	the opcode for erasing a sector
@@ -143,7 +144,8 @@ enum spi_nor_option_flags {
  * @read:		[DRIVER-SPECIFIC] read data from the SPI NOR
  * @write:		[DRIVER-SPECIFIC] write data to the SPI NOR
  * @erase:		[DRIVER-SPECIFIC] erase a sector of the SPI NOR
- *			at the offset @offs
+ *			at the offset @offs; if not provided by the driver,
+ *			spi-nor will send the erase opcode via write_reg()
  * @flash_lock:		[FLASH-SPECIFIC] lock a region of the SPI NOR
  * @flash_unlock:	[FLASH-SPECIFIC] unlock a region of the SPI NOR
  * @flash_is_locked:	[FLASH-SPECIFIC] check if a region of the SPI NOR is
@@ -154,7 +156,6 @@ struct spi_nor {
 	struct mtd_info		mtd;
 	struct mutex		lock;
 	struct device		*dev;
-	struct device_node	*flash_node;
 	u32			page_size;
 	u8			addr_width;
 	u8			erase_opcode;
@@ -184,6 +185,17 @@ struct spi_nor {
 	void *priv;
 };
 
+static inline void spi_nor_set_flash_node(struct spi_nor *nor,
+					  struct device_node *np)
+{
+	mtd_set_of_node(&nor->mtd, np);
+}
+
+static inline struct device_node *spi_nor_get_flash_node(struct spi_nor *nor)
+{
+	return mtd_get_of_node(&nor->mtd);
+}
+
 /**
  * spi_nor_scan() - scan the SPI NOR
  * @nor:	the spi_nor structure
