From 56a753118a1446feedb1845f37f3e5d3cc4f31a1 Mon Sep 17 00:00:00 2001
From: Waldemar Brodkorb <wbrodkorb@conet.de>
Date: Wed, 25 Mar 2015 09:26:17 +0100
Subject: [PATCH 075/381] Add driver for rpi-proto

Forward port of 3.10.x driver from https://github.com/koalo
We are using a custom board and would like to use rpi 3.18.x
kernel. Patch works fine for our embedded system.

URL to the audio chip:
http://www.mikroe.com/add-on-boards/audio-voice/audio-codec-proto/

Playback tested with devicetree enabled.

Signed-off-by: Waldemar Brodkorb <wbrodkorb@conet.de>
---
 sound/soc/bcm/Kconfig     |   7 +++
 sound/soc/bcm/Makefile    |   2 +
 sound/soc/bcm/rpi-proto.c | 153 ++++++++++++++++++++++++++++++++++++++++++++++
 3 files changed, 162 insertions(+)
 create mode 100644 sound/soc/bcm/rpi-proto.c

--- a/sound/soc/bcm/Kconfig
+++ b/sound/soc/bcm/Kconfig
@@ -43,6 +43,13 @@ config SND_BCM2708_SOC_RPI_DAC
         help
          Say Y or M if you want to add support for RPi-DAC.
 
+config SND_BCM2708_SOC_RPI_PROTO
+	tristate "Support for Rpi-PROTO"
+	depends on SND_BCM2708_SOC_I2S || SND_BCM2835_SOC_I2S
+	select SND_SOC_WM8731
+	help
+	  Say Y or M if you want to add support for Audio Codec Board PROTO (WM8731).
+
 config SND_BCM2708_SOC_IQAUDIO_DAC
 	tristate "Support for IQaudIO-DAC"
 	depends on SND_BCM2708_SOC_I2S || SND_BCM2835_SOC_I2S
--- a/sound/soc/bcm/Makefile
+++ b/sound/soc/bcm/Makefile
@@ -9,6 +9,7 @@ snd-soc-hifiberry-dacplus-objs := hifibe
 snd-soc-hifiberry-digi-objs := hifiberry_digi.o
 snd-soc-hifiberry-amp-objs := hifiberry_amp.o
 snd-soc-rpi-dac-objs := rpi-dac.o
+snd-soc-rpi-proto-objs := rpi-proto.o
 snd-soc-iqaudio-dac-objs := iqaudio-dac.o
 
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC) += snd-soc-hifiberry-dac.o
@@ -16,4 +17,5 @@ obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_D
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DIGI) += snd-soc-hifiberry-digi.o
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP) += snd-soc-hifiberry-amp.o
 obj-$(CONFIG_SND_BCM2708_SOC_RPI_DAC) += snd-soc-rpi-dac.o
+obj-$(CONFIG_SND_BCM2708_SOC_RPI_PROTO) += snd-soc-rpi-proto.o
 obj-$(CONFIG_SND_BCM2708_SOC_IQAUDIO_DAC) += snd-soc-iqaudio-dac.o
--- /dev/null
+++ b/sound/soc/bcm/rpi-proto.c
@@ -0,0 +1,153 @@
+/*
+ * ASoC driver for PROTO AudioCODEC (with a WM8731)
+ * connected to a Raspberry Pi
+ *
+ * Author:      Florian Meier, <koalo@koalo.de>
+ *	      Copyright 2013
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <sound/core.h>
+#include <sound/pcm.h>
+#include <sound/soc.h>
+#include <sound/jack.h>
+
+#include "../codecs/wm8731.h"
+
+static const unsigned int wm8731_rates_12288000[] = {
+	8000, 32000, 48000, 96000,
+};
+
+static struct snd_pcm_hw_constraint_list wm8731_constraints_12288000 = {
+	.list = wm8731_rates_12288000,
+	.count = ARRAY_SIZE(wm8731_rates_12288000),
+};
+
+static int snd_rpi_proto_startup(struct snd_pcm_substream *substream)
+{
+	/* Setup constraints, because there is a 12.288 MHz XTAL on the board */
+	snd_pcm_hw_constraint_list(substream->runtime, 0,
+				SNDRV_PCM_HW_PARAM_RATE,
+				&wm8731_constraints_12288000);
+	return 0;
+}
+
+static int snd_rpi_proto_hw_params(struct snd_pcm_substream *substream,
+				       struct snd_pcm_hw_params *params)
+{
+	struct snd_soc_pcm_runtime *rtd = substream->private_data;
+	struct snd_soc_codec *codec = rtd->codec;
+	struct snd_soc_dai *codec_dai = rtd->codec_dai;
+	struct snd_soc_dai *cpu_dai = rtd->cpu_dai;
+	int sysclk = 12288000; /* This is fixed on this board */
+
+	/* Set proto bclk */
+	int ret = snd_soc_dai_set_bclk_ratio(cpu_dai,32*2);
+	if (ret < 0){
+		dev_err(codec->dev,
+				"Failed to set BCLK ratio %d\n", ret);
+		return ret;
+	}
+
+	/* Set proto sysclk */
+	ret = snd_soc_dai_set_sysclk(codec_dai, WM8731_SYSCLK_XTAL,
+			sysclk, SND_SOC_CLOCK_IN);
+	if (ret < 0) {
+		dev_err(codec->dev,
+				"Failed to set WM8731 SYSCLK: %d\n", ret);
+		return ret;
+	}
+
+	return 0;
+}
+
+/* machine stream operations */
+static struct snd_soc_ops snd_rpi_proto_ops = {
+	.startup = snd_rpi_proto_startup,
+	.hw_params = snd_rpi_proto_hw_params,
+};
+
+static struct snd_soc_dai_link snd_rpi_proto_dai[] = {
+{
+	.name		= "WM8731",
+	.stream_name	= "WM8731 HiFi",
+	.cpu_dai_name	= "bcm2708-i2s.0",
+	.codec_dai_name	= "wm8731-hifi",
+	.platform_name	= "bcm2708-i2s.0",
+	.codec_name	= "wm8731.1-001a",
+	.dai_fmt	= SND_SOC_DAIFMT_I2S
+				| SND_SOC_DAIFMT_NB_NF
+				| SND_SOC_DAIFMT_CBM_CFM,
+	.ops		= &snd_rpi_proto_ops,
+},
+};
+
+/* audio machine driver */
+static struct snd_soc_card snd_rpi_proto = {
+	.name		= "snd_rpi_proto",
+	.dai_link	= snd_rpi_proto_dai,
+	.num_links	= ARRAY_SIZE(snd_rpi_proto_dai),
+};
+
+static int snd_rpi_proto_probe(struct platform_device *pdev)
+{
+	int ret = 0;
+
+	snd_rpi_proto.dev = &pdev->dev;
+
+	if (pdev->dev.of_node) {
+		struct device_node *i2s_node;
+		struct snd_soc_dai_link *dai = &snd_rpi_proto_dai[0];
+		i2s_node = of_parse_phandle(pdev->dev.of_node,
+				            "i2s-controller", 0);
+
+		if (i2s_node) {
+			dai->cpu_dai_name = NULL;
+			dai->cpu_of_node = i2s_node;
+			dai->platform_name = NULL;
+			dai->platform_of_node = i2s_node;
+		}
+	}
+
+	ret = snd_soc_register_card(&snd_rpi_proto);
+	if (ret) {
+		dev_err(&pdev->dev,
+				"snd_soc_register_card() failed: %d\n", ret);
+	}
+
+	return ret;
+}
+
+
+static int snd_rpi_proto_remove(struct platform_device *pdev)
+{
+	return snd_soc_unregister_card(&snd_rpi_proto);
+}
+
+static const struct of_device_id snd_rpi_proto_of_match[] = {
+	{ .compatible = "rpi,rpi-proto", },
+	{},
+};
+MODULE_DEVICE_TABLE(of, snd_rpi_proto_of_match);
+
+static struct platform_driver snd_rpi_proto_driver = {
+	.driver = {
+		.name   = "snd-rpi-proto",
+		.owner  = THIS_MODULE,
+		.of_match_table = snd_rpi_proto_of_match,
+	},
+	.probe	  = snd_rpi_proto_probe,
+	.remove	 = snd_rpi_proto_remove,
+};
+
+module_platform_driver(snd_rpi_proto_driver);
+
+MODULE_AUTHOR("Florian Meier");
+MODULE_DESCRIPTION("ASoC Driver for Raspberry Pi connected to PROTO board (WM8731)");
+MODULE_LICENSE("GPL");
