From d6a71e3caae07fb2d98e93ee62477273abaceb27 Mon Sep 17 00:00:00 2001
From: Reinder de Haan <patchesrdh@mveas.com>
Date: Tue, 3 Nov 2015 15:13:00 +0100
Subject: [PATCH] ARM: dts: sun8i: Add support for H3 usb clocks

Add a node describing the usb-clks found on the H3.

Signed-off-by: Reinder de Haan <patchesrdh@mveas.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun8i-h3.dtsi | 12 ++++++++++++
 1 file changed, 12 insertions(+)

--- a/arch/arm/boot/dts/sun8i-h3.dtsi
+++ b/arch/arm/boot/dts/sun8i-h3.dtsi
@@ -269,6 +269,18 @@
 					     "mmc2_sample";
 		};
 
+		usb_clk: clk@01c200cc {
+			#clock-cells = <1>;
+			#reset-cells = <1>;
+			compatible = "allwinner,sun8i-h3-usb-clk";
+			reg = <0x01c200cc 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "usb_phy0", "usb_phy1",
+					     "usb_phy2", "usb_phy3",
+					     "usb_ohci0", "usb_ohci1",
+					     "usb_ohci2", "usb_ohci3";
+		};
+
 		mbus_clk: clk@01c2015c {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun8i-a23-mbus-clk";
