/dts-v1/;

#include "rt3050.dtsi"

/ {
	compatible = "JHR-N926R", "ralink,rt3052-soc";
	model = "JCG JHR-N926R";

	cfi@1f000000 {
		compatible = "cfi-flash";
		reg = <0x1f000000 0x800000>;
		bank-width = <2>;
		device-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x30000>;
			read-only;
		};

		partition@30000 {
			label = "u-boot-env";
			reg = <0x30000 0x10000>;
			read-only;
		};

		factory: partition@40000 {
			label = "factory";
			reg = <0x40000 0x10000>;
			read-only;
		};

		partition@50000 {
			label = "firmware";
			reg = <0x50000 0x3b0000>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		wlan1 {
			label = "jhr-n926r:red:wlan";
			gpios = <&gpio0 20 1>;
		};

		wlan2 {
			label = "jhr-n926r:yellow:wlan";
			gpios = <&gpio0 19 1>;
		};

		wlan3 {
			label = "jhr-n926r:green:wlan";
			gpios = <&gpio0 17 1>;
		};

		system {
			label = "jhr-n926r:blue:system";
			gpios = <&gpio0 13 1>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		display_data {
			gpio-export,name = "display_data";
			gpio-export,output = <1>;
			gpios = <&gpio0 7 1>;
		};

		display_clock {
			gpio-export,name = "display_clock";
			gpio-export,output = <1>;
			gpios = <&gpio0 8 0>;
		};

		display_blank {
			gpio-export,name = "display_blank";
			gpio-export,output = <1>;
			gpios = <&gpio0 11 0>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset_wps {
			label = "reset_wps";
			gpios = <&gpio0 10 1>;
			linux,code = <0x198>;
		};

		wlan {
			label = "wlan";
			gpios = <&gpio0 1 1>;
			linux,code = <0x100>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "spi", "i2c", "jtag", "rgmii", "mdio", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x2e>;
};

&esw {
	mediatek,portmap = <0x3e>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
