From 48c22040d540d47c1dd4496a9587b0f3139fc8f0 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Fri, 6 May 2016 13:18:09 -0700
Subject: [PATCH 342/381] BCM270X_DT: Add the disabled-by-default DPI device
 node.

This will be enabled and connected to a particular panel by DT
overlays.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm2708_common.dtsi | 11 +++++++++++
 1 file changed, 11 insertions(+)

--- a/arch/arm/boot/dts/bcm2708_common.dtsi
+++ b/arch/arm/boot/dts/bcm2708_common.dtsi
@@ -179,6 +179,17 @@
 			status = "disabled";
 		};
 
+		dpi: dpi@7e208000 {
+			compatible = "brcm,bcm2835-dpi";
+			reg = <0x7e208000 0x8c>;
+			clocks = <&cprman BCM2835_CLOCK_VPU>,
+				 <&cprman BCM2835_CLOCK_DPI>;
+			clock-names = "core", "pixel";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
 		pixelvalve1: pixelvalve@7e207000 {
 			compatible = "brcm,bcm2835-pixelvalve1";
 			reg = <0x7e207000 0x100>;
