From 337a299edf74d3866636363b675f1b48e01cf842 Mon Sep 17 00:00:00 2001
From: campag <dave-lowe@ntlworld.com>
Date: Wed, 24 Feb 2016 16:45:42 +0000
Subject: [PATCH 199/381] BCM270X_DT: Add 1-bit SDIO using minimal pins...

... for that mode: GPIOs 22-25.
---
 arch/arm/boot/dts/overlays/README                | 21 ++++++++++++++
 arch/arm/boot/dts/overlays/sdio-1bit-overlay.dts | 36 ++++++++++++++++++++++++
 2 files changed, 57 insertions(+)
 create mode 100644 arch/arm/boot/dts/overlays/sdio-1bit-overlay.dts

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -709,6 +709,27 @@ Params: overclock_50            SD Clock
         bus_width               Set the SDIO host bus width (default 4 bits)
 
 
+Name:   sdio-1bit
+Info:   Selects the bcm2835-sdhost SD/MMC driver, optionally with overclock,
+        and enables 1-bit SDIO via GPIOs 22-25.
+Load:   dtoverlay=sdio-1bit,<param>=<val>
+Params: overclock_50            SD Clock (in MHz) to use when the MMC framework
+                                requests 50MHz
+
+        sdio_overclock          SDIO Clock (in MHz) to use when the MMC
+                                framework requests 50MHz
+
+        force_pio               Disable DMA support (default off)
+
+        pio_limit               Number of blocks above which to use DMA
+                                (default 1)
+
+        debug                   Enable debug output (default off)
+
+        poll_once               Disable SDIO-device polling every second
+                                (default on: polling once at boot-time)
+
+
 Name:   sdtweak
 Info:   Tunes the bcm2835-sdhost SD/MMC driver
 Load:   dtoverlay=sdtweak,<param>=<val>
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sdio-1bit-overlay.dts
@@ -0,0 +1,36 @@
+/* Enable 1-bit SDIO from MMC interface via GPIOs 22-25. Includes sdhost overlay. */
+
+/include/ "sdhost-overlay.dts"
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@3 {
+		target = <&mmc>;
+		sdio_mmc: __overlay__ {
+			compatible = "brcm,bcm2835-mmc";
+			pinctrl-names = "default";
+			pinctrl-0 = <&sdio_pins>;
+			non-removable;
+			bus-width = <1>;
+			brcm,overclock-50 = <0>;
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target = <&gpio>;
+		__overlay__ {
+			sdio_pins: sdio_pins {
+				brcm,pins = <22 23 24 25>;
+				brcm,function = <7 7 7 7>; /* ALT3 = SD1 */
+				brcm,pull = <0 2 2 2>;
+			};
+		};
+	};
+
+	__overrides__ {
+		poll_once = <&sdio_mmc>,"non-removable?";
+		sdio_overclock = <&sdio_mmc>,"brcm,overclock-50:0";
+	};
+};
