From f76d188586952fcd3b55916f30c484c62c8fabab Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 7 Mar 2016 16:46:39 +0000
Subject: [PATCH 167/381] bcm2835-sdhost: Only claim one DMA channel

With both MMC controllers enabled there are few DMA channels left. The
bcm2835-sdhost driver only uses DMA in one direction at a time, so it
doesn't need to claim two channels.

See: https://github.com/raspberrypi/linux/issues/1327

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2708_common.dtsi |  5 +--
 drivers/mmc/host/bcm2835-sdhost.c     | 70 ++++++++++++++++++++++++-----------
 2 files changed, 50 insertions(+), 25 deletions(-)

--- a/arch/arm/boot/dts/bcm2708_common.dtsi
+++ b/arch/arm/boot/dts/bcm2708_common.dtsi
@@ -136,9 +136,8 @@
 			reg = <0x7e202000 0x100>;
 			interrupts = <2 24>;
 			clocks = <&clk_core>;
-			dmas = <&dma 13>,
-			       <&dma 13>;
-			dma-names = "tx", "rx";
+			dmas = <&dma 13>;
+			dma-names = "rx-tx";
 			brcm,overclock-50 = <0>;
 			brcm,pio-limit = <1>;
 			status = "disabled";
--- a/drivers/mmc/host/bcm2835-sdhost.c
+++ b/drivers/mmc/host/bcm2835-sdhost.c
@@ -185,9 +185,10 @@ struct bcm2835_host {
 	unsigned int			debug:1;		/* Enable debug output */
 
 	/*DMA part*/
-	struct dma_chan			*dma_chan_rx;		/* DMA channel for reads */
-	struct dma_chan			*dma_chan_tx;		/* DMA channel for writes */
-	struct dma_chan			*dma_chan;		/* Channel in used */
+	struct dma_chan			*dma_chan_rxtx;		/* DMA channel for reads and writes */
+	struct dma_chan			*dma_chan;		/* Channel in use */
+	struct dma_slave_config		dma_cfg_rx;
+	struct dma_slave_config		dma_cfg_tx;
 	struct dma_async_tx_descriptor	*dma_desc;
 	u32				dma_dir;
 	u32				drain_words;
@@ -771,12 +772,11 @@ static void bcm2835_sdhost_prepare_dma(s
 	log_event("PRD<", (u32)data, 0);
 	pr_debug("bcm2835_sdhost_prepare_dma()\n");
 
+	dma_chan = host->dma_chan_rxtx;
 	if (data->flags & MMC_DATA_READ) {
-		dma_chan = host->dma_chan_rx;
 		dir_data = DMA_FROM_DEVICE;
 		dir_slave = DMA_DEV_TO_MEM;
 	} else {
-		dma_chan = host->dma_chan_tx;
 		dir_data = DMA_TO_DEVICE;
 		dir_slave = DMA_MEM_TO_DEV;
 	}
@@ -813,6 +813,12 @@ static void bcm2835_sdhost_prepare_dma(s
 		host->drain_words = len/4;
 	}
 
+	/* The parameters have already been validated, so this will not fail */
+	(void)dmaengine_slave_config(dma_chan,
+				     (dir_data == DMA_FROM_DEVICE) ?
+				     &host->dma_cfg_rx :
+				     &host->dma_cfg_tx);
+
 	len = dma_map_sg(dma_chan->device->dev, data->sg, data->sg_len,
 			 dir_data);
 
@@ -1805,28 +1811,46 @@ int bcm2835_sdhost_add_host(struct bcm28
 	spin_lock_init(&host->lock);
 
 	if (host->allow_dma) {
-		if (IS_ERR_OR_NULL(host->dma_chan_tx) ||
-		    IS_ERR_OR_NULL(host->dma_chan_rx)) {
-			pr_err("%s: unable to initialise DMA channels. "
+		if (IS_ERR_OR_NULL(host->dma_chan_rxtx)) {
+			pr_err("%s: unable to initialise DMA channel. "
 			       "Falling back to PIO\n",
 			       mmc_hostname(mmc));
 			host->use_dma = false;
 		} else {
-			host->use_dma = true;
-
 			cfg.src_addr_width = DMA_SLAVE_BUSWIDTH_4_BYTES;
 			cfg.dst_addr_width = DMA_SLAVE_BUSWIDTH_4_BYTES;
 			cfg.slave_id = 13;		/* DREQ channel */
 
+			/* Validate the slave configurations */
+
 			cfg.direction = DMA_MEM_TO_DEV;
 			cfg.src_addr = 0;
 			cfg.dst_addr = host->bus_addr + SDDATA;
-			ret = dmaengine_slave_config(host->dma_chan_tx, &cfg);
 
-			cfg.direction = DMA_DEV_TO_MEM;
-			cfg.src_addr = host->bus_addr + SDDATA;
-			cfg.dst_addr = 0;
-			ret = dmaengine_slave_config(host->dma_chan_rx, &cfg);
+			ret = dmaengine_slave_config(host->dma_chan_rxtx, &cfg);
+
+			if (ret == 0) {
+				host->dma_cfg_tx = cfg;
+
+				cfg.direction = DMA_DEV_TO_MEM;
+				cfg.src_addr = host->bus_addr + SDDATA;
+				cfg.dst_addr = 0;
+
+				ret = dmaengine_slave_config(host->dma_chan_rxtx, &cfg);
+			}
+
+			if (ret == 0) {
+				host->dma_cfg_rx = cfg;
+
+				host->use_dma = true;
+			} else {
+				pr_err("%s: unable to configure DMA channel. "
+				       "Falling back to PIO\n",
+				       mmc_hostname(mmc));
+				dma_release_channel(host->dma_chan_rxtx);
+				host->dma_chan_rxtx = NULL;
+				host->use_dma = false;
+			}
 		}
 	} else {
 		host->use_dma = false;
@@ -1948,19 +1972,21 @@ static int bcm2835_sdhost_probe(struct p
 
 	if (host->allow_dma) {
 		if (node) {
-			host->dma_chan_tx =
-				dma_request_slave_channel(dev, "tx");
-			host->dma_chan_rx =
-				dma_request_slave_channel(dev, "rx");
+			host->dma_chan_rxtx =
+				dma_request_slave_channel(dev, "rx-tx");
+			if (!host->dma_chan_rxtx)
+				host->dma_chan_rxtx =
+					dma_request_slave_channel(dev, "tx");
+			if (!host->dma_chan_rxtx)
+				host->dma_chan_rxtx =
+					dma_request_slave_channel(dev, "rx");
 		} else {
 			dma_cap_mask_t mask;
 
 			dma_cap_zero(mask);
 			/* we don't care about the channel, any would work */
 			dma_cap_set(DMA_SLAVE, mask);
-			host->dma_chan_tx =
-				dma_request_channel(mask, NULL, NULL);
-			host->dma_chan_rx =
+			host->dma_chan_rxtx =
 				dma_request_channel(mask, NULL, NULL);
 		}
 	}
