From 2cbf3f95a49925317ef4138ceaf7f7f30f353f0f Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Tue, 3 May 2016 03:17:53 +0200
Subject: [PATCH 089/102] net-next: mediatek: increase watchdog_timeo

During stress testing, after reducing the threshold value, we have seen
TX timeouts that were caused by the watchdog_timeo value being too low.
Increase the value to 5 * HZ which is a value commonly used by many other
drivers.

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1720,7 +1720,7 @@ static int mtk_add_mac(struct mtk_eth *e
 	mac->hw_stats->reg_offset = id * MTK_STAT_OFFSET;
 
 	SET_NETDEV_DEV(eth->netdev[id], eth->dev);
-	eth->netdev[id]->watchdog_timeo = HZ;
+	eth->netdev[id]->watchdog_timeo = 5 * HZ;
 	eth->netdev[id]->netdev_ops = &mtk_netdev_ops;
 	eth->netdev[id]->base_addr = (unsigned long)eth->base;
 	eth->netdev[id]->vlan_features = MTK_HW_FEATURES &
