From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Subject: [PATCH] ARM: BCM5301X: Add DT for Linksys EA6300 V1
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -65,6 +65,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm4708-asus-rt-ac56u.dtb \
 	bcm4708-asus-rt-ac68u.dtb \
 	bcm4708-buffalo-wzr-1750dhp.dtb \
+	bcm4708-linksys-ea6300-v1.dtb \
 	bcm4708-luxul-xwc-1000.dtb \
 	bcm4708-netgear-r6250.dtb \
 	bcm4708-netgear-r6300-v2.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm4708-linksys-ea6300-v1.dts
@@ -0,0 +1,48 @@
+/*
+ * Broadcom BCM470X / BCM5301X ARM platform code.
+ * DTS for Linksys EA6300 V1
+ *
+ * Copyright (C) 2015 Rafał Miłecki <zajec5@gmail.com>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+/dts-v1/;
+
+#include "bcm4708.dtsi"
+#include "bcm5301x-nand-cs0-bch8.dtsi"
+
+/ {
+	compatible = "linksys,ea6300v1", "brcm,bcm4708";
+	model = "Linksys EA6300 V1";
+
+	chosen {
+		bootargs = "console=ttyS0,115200";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		wps {
+			label = "WPS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&chipcommon 7 GPIO_ACTIVE_LOW>;
+		};
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
