From f0f6dd227bbb171ad6b0dbe1d394de71d78eae21 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 17 Mar 2016 10:16:16 +0000
Subject: [PATCH 203/381] pi3-miniuart-bt-overlay: Correct and clarify info

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/README                      | 6 ++++--
 arch/arm/boot/dts/overlays/pi3-miniuart-bt-overlay.dts | 6 ++++--
 2 files changed, 8 insertions(+), 4 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -511,8 +511,10 @@ Name:   pi3-miniuart-bt
 Info:   Switch Pi3 Bluetooth function to use the mini-UART (ttyS0) and restore
         UART0/ttyAMA0 over GPIOs 14 & 15. Note that this may reduce the maximum
         usable baudrate.
-        N.B. It is also necessary to edit /lib/systemd/system/hciuart.server
-        and replace ttyAMA0 with ttyS0.
+        N.B. It is also necessary to edit /lib/systemd/system/hciuart.service
+        and replace ttyAMA0 with ttyS0, unless you have a system with udev rules
+        that create /dev/serial0 and /dev/serial1, in which case use
+        /dev/serial1 instead because it will always be correct.
 Load:   dtoverlay=pi3-miniuart-bt
 Params: <None>
 
--- a/arch/arm/boot/dts/overlays/pi3-miniuart-bt-overlay.dts
+++ b/arch/arm/boot/dts/overlays/pi3-miniuart-bt-overlay.dts
@@ -5,8 +5,10 @@
    UART0/ttyAMA0 over GPIOs 14 & 15. Note that this may reduce the maximum
    usable baudrate.
 
-   It is also necessary to edit /lib/systemd/system/hciuart.server and
-   replace ttyAMA0 with ttyS0.
+   It is also necessary to edit /lib/systemd/system/hciuart.service and
+   replace ttyAMA0 with ttyS0, unless you have a system with udev rules
+   that create /dev/serial0 and /dev/serial1, in which case use /dev/serial1
+   instead because it will always be correct.
 
    If cmdline.txt uses the alias serial0 to refer to the user-accessable port
    then the firmware will replace with the appropriate port whether or not
