From c9f294ff6584782d20b4a766901a9cff7398bb20 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 4 Jan 2016 22:27:57 +0100
Subject: [PATCH] pinctrl: lantiq: 2 pins have the wrong mux list

The latest vendor SDK contained this patch.

Signed-off-by: John Crispin <blogic@openwrt.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 drivers/pinctrl/pinctrl-xway.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/pinctrl/pinctrl-xway.c
+++ b/drivers/pinctrl/pinctrl-xway.c
@@ -160,10 +160,10 @@ static const struct ltq_mfp_pin xway_mfp
 	MFP_XWAY(GPIO41, GPIO,	NONE,	NONE,	NONE),
 	MFP_XWAY(GPIO42, GPIO,	MDIO,	NONE,	NONE),
 	MFP_XWAY(GPIO43, GPIO,	MDIO,	NONE,	NONE),
-	MFP_XWAY(GPIO44, GPIO,	NONE,	SIN,	GPHY),
+	MFP_XWAY(GPIO44, GPIO,	MII,	SIN,	GPHY),
 	MFP_XWAY(GPIO45, GPIO,	NONE,	GPHY,	SIN),
 	MFP_XWAY(GPIO46, GPIO,	NONE,	NONE,	EXIN),
-	MFP_XWAY(GPIO47, GPIO,	NONE,	GPHY,	SIN),
+	MFP_XWAY(GPIO47, GPIO,	MII,	GPHY,	SIN),
 	MFP_XWAY(GPIO48, GPIO,	EBU,	NONE,	NONE),
 	MFP_XWAY(GPIO49, GPIO,	EBU,	NONE,	NONE),
 	MFP_XWAY(GPIO50, GPIO,	NONE,	NONE,	NONE),
