From 6d1609ef815189095a8e44feb38e2c128c3736a5 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Thu, 31 Mar 2016 18:38:20 -0700
Subject: [PATCH 339/381] drm/vc4: Add support for gamma ramps.

We could possibly save a bit of power by not requesting gamma
conversion when the ramp happens to be 1:1, but at least if all the
CRTCs are off the SRAM will be disabled.

This should fix brightness sliders in a lot of fullscreen games.

Signed-off-by: Eric Anholt <eric@anholt.net>
(cherry picked from commit e582b6c7e7f9d0b1e30e8017e4082d3a9ede3310)
---
 drivers/gpu/drm/vc4/vc4_crtc.c | 58 ++++++++++++++++++++++++++++++++++++++++++
 drivers/gpu/drm/vc4/vc4_regs.h |  6 +++++
 2 files changed, 64 insertions(+)

--- a/drivers/gpu/drm/vc4/vc4_crtc.c
+++ b/drivers/gpu/drm/vc4/vc4_crtc.c
@@ -49,6 +49,10 @@ struct vc4_crtc {
 	/* Which HVS channel we're using for our CRTC. */
 	int channel;
 
+	u8 lut_r[256];
+	u8 lut_g[256];
+	u8 lut_b[256];
+
 	struct drm_pending_vblank_event *event;
 };
 
@@ -147,6 +151,46 @@ static void vc4_crtc_destroy(struct drm_
 	drm_crtc_cleanup(crtc);
 }
 
+static void
+vc4_crtc_lut_load(struct drm_crtc *crtc)
+{
+	struct drm_device *dev = crtc->dev;
+	struct vc4_dev *vc4 = to_vc4_dev(dev);
+	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
+	u32 i;
+
+	/* The LUT memory is laid out with each HVS channel in order,
+	 * each of which takes 256 writes for R, 256 for G, then 256
+	 * for B.
+	 */
+	HVS_WRITE(SCALER_GAMADDR,
+		  SCALER_GAMADDR_AUTOINC |
+		  (vc4_crtc->channel * 3 * crtc->gamma_size));
+
+	for (i = 0; i < crtc->gamma_size; i++)
+		HVS_WRITE(SCALER_GAMDATA, vc4_crtc->lut_r[i]);
+	for (i = 0; i < crtc->gamma_size; i++)
+		HVS_WRITE(SCALER_GAMDATA, vc4_crtc->lut_g[i]);
+	for (i = 0; i < crtc->gamma_size; i++)
+		HVS_WRITE(SCALER_GAMDATA, vc4_crtc->lut_b[i]);
+}
+
+static void
+vc4_crtc_gamma_set(struct drm_crtc *crtc, u16 *r, u16 *g, u16 *b,
+		   uint32_t start, uint32_t size)
+{
+	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
+	u32 i;
+
+	for (i = start; i < start + size; i++) {
+		vc4_crtc->lut_r[i] = r[i] >> 8;
+		vc4_crtc->lut_g[i] = g[i] >> 8;
+		vc4_crtc->lut_b[i] = b[i] >> 8;
+	}
+
+	vc4_crtc_lut_load(crtc);
+}
+
 static u32 vc4_get_fifo_full_level(u32 format)
 {
 	static const u32 fifo_len_bytes = 64;
@@ -260,8 +304,14 @@ static void vc4_crtc_mode_set_nofb(struc
 
 	HVS_WRITE(SCALER_DISPBKGNDX(vc4_crtc->channel),
 		  SCALER_DISPBKGND_AUTOHS |
+		  SCALER_DISPBKGND_GAMMA |
 		  (interlace ? SCALER_DISPBKGND_INTERLACE : 0));
 
+	/* Reload the LUT, since the SRAMs would have been disabled if
+	 * all CRTCs had SCALER_DISPBKGND_GAMMA unset at once.
+	 */
+	vc4_crtc_lut_load(crtc);
+
 	if (debug_dump_regs) {
 		DRM_INFO("CRTC %d regs after:\n", drm_crtc_index(crtc));
 		vc4_crtc_dump_regs(vc4_crtc);
@@ -613,6 +663,7 @@ static const struct drm_crtc_funcs vc4_c
 	.reset = drm_atomic_helper_crtc_reset,
 	.atomic_duplicate_state = vc4_crtc_duplicate_state,
 	.atomic_destroy_state = vc4_crtc_destroy_state,
+	.gamma_set = vc4_crtc_gamma_set,
 };
 
 static const struct drm_crtc_helper_funcs vc4_crtc_helper_funcs = {
@@ -731,6 +782,7 @@ static int vc4_crtc_bind(struct device *
 	primary_plane->crtc = crtc;
 	vc4->crtc[drm_crtc_index(crtc)] = vc4_crtc;
 	vc4_crtc->channel = vc4_crtc->data->hvs_channel;
+	drm_mode_crtc_set_gamma_size(crtc, ARRAY_SIZE(vc4_crtc->lut_r));
 
 	/* Set up some arbitrary number of planes.  We're not limited
 	 * by a set number of physical registers, just the space in
@@ -771,6 +823,12 @@ static int vc4_crtc_bind(struct device *
 
 	vc4_set_crtc_possible_masks(drm, crtc);
 
+	for (i = 0; i < crtc->gamma_size; i++) {
+		vc4_crtc->lut_r[i] = i;
+		vc4_crtc->lut_g[i] = i;
+		vc4_crtc->lut_b[i] = i;
+	}
+
 	platform_set_drvdata(pdev, vc4_crtc);
 
 	return 0;
--- a/drivers/gpu/drm/vc4/vc4_regs.h
+++ b/drivers/gpu/drm/vc4/vc4_regs.h
@@ -390,6 +390,12 @@
 #define SCALER_DISPBASE2                        0x0000006c
 #define SCALER_DISPALPHA2                       0x00000070
 #define SCALER_GAMADDR                          0x00000078
+# define SCALER_GAMADDR_AUTOINC			BIT(31)
+/* Enables all gamma ramp SRAMs, not just those of CRTCs with gamma
+ * enabled.
+ */
+# define SCALER_GAMADDR_SRAMENB			BIT(30)
+
 #define SCALER_GAMDATA                          0x000000e0
 #define SCALER_DLIST_START                      0x00002000
 #define SCALER_DLIST_SIZE                       0x00004000
