From 4eb2de8729beeae668d522478da951d1da91c42f Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 19 Apr 2016 14:36:31 -0700
Subject: [PATCH 272/381] bcm2708: Add the power domain driver to the device
 tree.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm2708_common.dtsi | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/arm/boot/dts/bcm2708_common.dtsi
+++ b/arch/arm/boot/dts/bcm2708_common.dtsi
@@ -285,6 +285,12 @@
 			mboxes = <&mailbox>;
 		};
 
+		power: power {
+			compatible = "raspberrypi,bcm2835-power";
+			firmware = <&firmware>;
+			#power-domain-cells = <1>;
+		};
+
 		leds: leds {
 			compatible = "gpio-leds";
 		};
