From 0945d95f5b98b323f6a611e2bb96a3400fd91d41 Mon Sep 17 00:00:00 2001
From: Przemek Rudy <prudy1@o2.pl>
Date: Fri, 11 Mar 2016 22:41:26 +0100
Subject: [PATCH 191/381] dwc-overlay: Use label so overrides can apply.

---
 arch/arm/boot/dts/overlays/dwc2-overlay.dts | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

--- a/arch/arm/boot/dts/overlays/dwc2-overlay.dts
+++ b/arch/arm/boot/dts/overlays/dwc2-overlay.dts
@@ -8,7 +8,7 @@
 		target = <&usb>;
 		#address-cells = <1>;
 		#size-cells = <1>;
-		__overlay__ {
+		dwc2_usb: __overlay__ {
 			compatible = "brcm,bcm2835-usb";
 			reg = <0x7e980000 0x10000>;
 			interrupts = <1 9>;
@@ -21,9 +21,9 @@
 	};
 
 	__overrides__ {
-		dr_mode = <&usb>, "dr_mode";
-		g-np-tx-fifo-size = <&usb>,"g-np-tx-fifo-size:0";
-		g-rx-fifo-size = <&usb>,"g-rx-fifo-size:0";
-		g-tx-fifo-size = <&usb>,"g-tx-fifo-size:0";
+		dr_mode = <&dwc2_usb>, "dr_mode";
+		g-np-tx-fifo-size = <&dwc2_usb>,"g-np-tx-fifo-size:0";
+		g-rx-fifo-size = <&dwc2_usb>,"g-rx-fifo-size:0";
+		g-tx-fifo-size = <&dwc2_usb>,"g-tx-fifo-size:0";
 	};
 };
