From 4dc11d58769fda62ef7cff1ab506d4c68c232270 Mon Sep 17 00:00:00 2001
From: notro <notro@tronnes.org>
Date: Wed, 9 Jul 2014 14:46:08 +0200
Subject: [PATCH 051/381] BCM2708: Add core Device Tree support

Add the bare minimum needed to boot BCM2708 from a Device Tree.

Signed-off-by: Noralf Tronnes <notro@tronnes.org>

BCM2708: DT: change 'axi' nodename to 'soc'

Change DT node named 'axi' to 'soc' so it matches ARCH_BCM2835.
The VC4 bootloader fills in certain properties in the 'axi' subtree,
but since this is part of an upstreaming effort, the name is changed.

Signed-off-by: Noralf Tronnes notro@tronnes.org

BCM2708_DT: Correct length of the peripheral space

Use dts-dirs feature for overlays.

The kernel makefiles have a dts-dirs target that is for vendor subdirectories.

Using this fixes the install_dtbs target, which previously did not install the overlays.

BCM270X_DT: configure I2S DMA channels

Signed-off-by: Matthias Reichl <hias@horus.com>

BCM270X_DT: switch to bcm2835-i2s

I2S soundcard drivers with proper devicetree support (i.e. not linking
to the cpu_dai/platform via name but to cpu/platform via of_node)
will work out of the box without any modifications.

When the kernel is compiled without devicetree support the platform
code will instantiate the bcm2708-i2s driver and I2S soundcard drivers
will link to it via name, as before.

Signed-off-by: Matthias Reichl <hias@horus.com>

SDIO-overlay: add poll_once-boolean parameter

Add paramter to toggle sdio-device-polling
done every second or once at boot-time.

Signed-off-by: Patrick Boettcher <patrick.boettcher@posteo.de>

BCM270X_DT: Make mmc overlay compatible with current firmware

The original DT overlay logic followed a merge-then-patch procedure,
i.e. parameters are applied to the loaded overlay before the overlay
is merged into the base DTB. This sequence has been changed to
patch-then-merge, in order to support parameterised node names, and
to protect against bad overlays. As a result, overrides (parameters)
must only target labels in the overlay, but the overlay can obviously target nodes in the base DTB.

mmc-overlay.dts (that switches back to the original mmc sdcard
driver) is the only overlay violating that rule, and this patch
fixes it.

bcm270x_dt: Use the sdhost MMC controller by default

The "mmc" overlay reverts to using the other controller.

squash: Add cprman to dt

BCM270X_DT: Use clk_core for I2C interfaces
---
 arch/arm/boot/dts/Makefile                         |  30 +
 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts           | 145 +++++
 arch/arm/boot/dts/bcm2708-rpi-b.dts                | 135 +++++
 arch/arm/boot/dts/bcm2708-rpi-cm.dts               | 102 ++++
 arch/arm/boot/dts/bcm2708-rpi-cm.dtsi              |  40 ++
 arch/arm/boot/dts/bcm2708.dtsi                     |  40 ++
 arch/arm/boot/dts/bcm2708_common.dtsi              | 347 +++++++++++
 arch/arm/boot/dts/bcm2709-rpi-2-b.dts              | 145 +++++
 arch/arm/boot/dts/bcm2709.dtsi                     | 102 ++++
 arch/arm/boot/dts/bcm2835-rpi-cm.dts               |  93 +++
 arch/arm/boot/dts/bcm2835-rpi-cm.dtsi              |  30 +
 arch/arm/boot/dts/overlays/Makefile                |  69 +++
 arch/arm/boot/dts/overlays/README                  | 648 +++++++++++++++++++++
 arch/arm/boot/dts/overlays/ads7846-overlay.dts     |  83 +++
 .../dts/overlays/bmp085_i2c-sensor-overlay.dts     |  23 +
 arch/arm/boot/dts/overlays/dht11-overlay.dts       |  39 ++
 arch/arm/boot/dts/overlays/enc28j60-overlay.dts    |  50 ++
 .../boot/dts/overlays/gpio-poweroff-overlay.dts    |  34 ++
 .../boot/dts/overlays/hifiberry-amp-overlay.dts    |  39 ++
 .../boot/dts/overlays/hifiberry-dac-overlay.dts    |  34 ++
 .../dts/overlays/hifiberry-dacplus-overlay.dts     |  39 ++
 .../boot/dts/overlays/hifiberry-digi-overlay.dts   |  39 ++
 arch/arm/boot/dts/overlays/hy28a-overlay.dts       |  87 +++
 arch/arm/boot/dts/overlays/hy28b-overlay.dts       | 142 +++++
 arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts     |  55 ++
 arch/arm/boot/dts/overlays/i2s-mmap-overlay.dts    |  13 +
 arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts |  39 ++
 .../boot/dts/overlays/iqaudio-dacplus-overlay.dts  |  39 ++
 arch/arm/boot/dts/overlays/lirc-rpi-overlay.dts    |  57 ++
 .../arm/boot/dts/overlays/mcp2515-can0-overlay.dts |  69 +++
 .../arm/boot/dts/overlays/mcp2515-can1-overlay.dts |  69 +++
 arch/arm/boot/dts/overlays/mmc-overlay.dts         |  39 ++
 arch/arm/boot/dts/overlays/mz61581-overlay.dts     | 111 ++++
 arch/arm/boot/dts/overlays/piscreen-overlay.dts    |  96 +++
 .../dts/overlays/pitft28-resistive-overlay.dts     | 115 ++++
 arch/arm/boot/dts/overlays/pps-gpio-overlay.dts    |  34 ++
 arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts   |  46 ++
 arch/arm/boot/dts/overlays/pwm-overlay.dts         |  42 ++
 arch/arm/boot/dts/overlays/raspidac3-overlay.dts   |  45 ++
 arch/arm/boot/dts/overlays/rpi-dac-overlay.dts     |  34 ++
 arch/arm/boot/dts/overlays/rpi-display-overlay.dts |  82 +++
 arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts  |  17 +
 arch/arm/boot/dts/overlays/rpi-proto-overlay.dts   |  39 ++
 arch/arm/boot/dts/overlays/rpi-sense-overlay.dts   |  47 ++
 arch/arm/boot/dts/overlays/sdhost-overlay.dts      |  29 +
 arch/arm/boot/dts/overlays/sdio-overlay.dts        |  32 +
 arch/arm/boot/dts/overlays/smi-dev-overlay.dts     |  18 +
 arch/arm/boot/dts/overlays/smi-nand-overlay.dts    |  69 +++
 arch/arm/boot/dts/overlays/smi-overlay.dts         |  37 ++
 .../boot/dts/overlays/spi-gpio35-39-overlay.dts    |  31 +
 arch/arm/boot/dts/overlays/tinylcd35-overlay.dts   | 216 +++++++
 arch/arm/boot/dts/overlays/uart1-overlay.dts       |  38 ++
 arch/arm/boot/dts/overlays/vga666-overlay.dts      |  30 +
 arch/arm/boot/dts/overlays/w1-gpio-overlay.dts     |  39 ++
 .../boot/dts/overlays/w1-gpio-pullup-overlay.dts   |  41 ++
 55 files changed, 4203 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-b.dts
 create mode 100755 arch/arm/boot/dts/bcm2708-rpi-cm.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2708.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2708_common.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2709-rpi-2-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2709.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2835-rpi-cm.dts
 create mode 100644 arch/arm/boot/dts/bcm2835-rpi-cm.dtsi
 create mode 100644 arch/arm/boot/dts/overlays/Makefile
 create mode 100644 arch/arm/boot/dts/overlays/README
 create mode 100644 arch/arm/boot/dts/overlays/ads7846-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/bmp085_i2c-sensor-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dht11-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/enc28j60-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-poweroff-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-amp-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dacplus-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-digi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hy28a-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hy28b-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2s-mmap-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/iqaudio-dacplus-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/lirc-rpi-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/mcp2515-can0-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mcp2515-can1-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mmc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mz61581-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/piscreen-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pitft28-resistive-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pps-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pwm-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/raspidac3-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-display-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-proto-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sdhost-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sdio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/smi-dev-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/smi-nand-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/smi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi-gpio35-39-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/tinylcd35-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/uart1-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/vga666-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/w1-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/w1-gpio-pullup-overlay.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -1,5 +1,25 @@
 ifeq ($(CONFIG_OF),y)
 
+dtb-$(CONFIG_ARCH_BCM2708) += bcm2708-rpi-b.dtb
+dtb-$(CONFIG_ARCH_BCM2708) += bcm2708-rpi-b-plus.dtb
+dtb-$(CONFIG_ARCH_BCM2708) += bcm2708-rpi-cm.dtb
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2835-rpi-cm.dtb
+dtb-$(CONFIG_ARCH_BCM2709) += bcm2709-rpi-2-b.dtb
+
+# Raspberry Pi
+ifeq ($(CONFIG_ARCH_BCM2708),y)
+   RPI_DT_OVERLAYS=y
+endif
+ifeq ($(CONFIG_ARCH_BCM2709),y)
+   RPI_DT_OVERLAYS=y
+endif
+ifeq ($(CONFIG_ARCH_BCM2835),y)
+   RPI_DT_OVERLAYS=y
+endif
+ifeq ($(RPI_DT_OVERLAYS),y)
+    dts-dirs += overlays
+endif
+
 dtb-$(CONFIG_ARCH_ALPINE) += \
 	alpine-db.dtb
 dtb-$(CONFIG_MACH_ASM9260) += \
@@ -777,10 +797,20 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += \
 	mt8127-moose.dtb \
 	mt8135-evbp1.dtb
 dtb-$(CONFIG_ARCH_ZX) += zx296702-ad1.dtb
+
+targets += dtbs dtbs_install
+targets += $(dtb-y)
+
 endif
 
 dtstree		:= $(srctree)/$(src)
 dtb-$(CONFIG_OF_ALL_DTBS) := $(patsubst $(dtstree)/%.dts,%.dtb, $(wildcard $(dtstree)/*.dts))
 
 always		:= $(dtb-y)
+subdir-y	:= $(dts-dirs)
 clean-files	:= *.dtb
+
+# Enable fixups to support overlays on BCM2708 platforms
+ifeq ($(RPI_DT_OVERLAYS),y)
+	DTC_FLAGS ?= -@
+endif
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
@@ -0,0 +1,145 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+
+/ {
+	compatible = "brcm,bcm2708";
+	model = "Raspberry Pi Model B+";
+};
+
+&gpio {
+	sdhost_pins: sdhost_pins {
+		brcm,pins = <48 49 50 51 52 53>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+};
+
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&fb {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&random {
+	status = "okay";
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&gpio 35 0>;
+	};
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-b.dts
@@ -0,0 +1,135 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+
+/ {
+	compatible = "brcm,bcm2708";
+	model = "Raspberry Pi Model B";
+};
+
+&gpio {
+	sdhost_pins: sdhost_pins {
+		brcm,pins = <48 49 50 51 52 53>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <28 29 30 31>;
+		brcm,function = <6>; /* alt2 */
+	};
+};
+
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&fb {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&random {
+	status = "okay";
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 16 1>;
+	};
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
@@ -0,0 +1,102 @@
+/dts-v1/;
+
+#include "bcm2708-rpi-cm.dtsi"
+
+/ {
+	model = "Raspberry Pi Compute Module";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&random {
+	status = "okay";
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
@@ -0,0 +1,40 @@
+#include "bcm2708.dtsi"
+
+&gpio {
+	sdhost_pins: sdhost_pins {
+		brcm,pins = <48 49 50 51 52 53>;
+		brcm,function = <4>; /* alt0 */
+	};
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+};
+
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_pins>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+};
+
+&fb {
+	status = "okay";
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708.dtsi
@@ -0,0 +1,40 @@
+#include "bcm2708_common.dtsi"
+
+/ {
+	compatible = "brcm,bcm2708";
+	model = "BCM2708";
+
+	chosen {
+		/* No padding required - the boot loader can do that. */
+		bootargs = "";
+	};
+
+	soc {
+		ranges = <0x7e000000 0x20000000 0x01000000>;
+
+		timer@7e003000 {
+			compatible = "brcm,bcm2835-system-timer";
+			reg = <0x7e003000 0x1000>;
+			interrupts = <1 0>, <1 1>, <1 2>, <1 3>;
+			clock-frequency = <1000000>;
+		};
+
+		arm-pmu {
+			compatible = "arm,arm1176-pmu";
+		};
+
+		gpiomem {
+			compatible = "brcm,bcm2835-gpiomem";
+			reg = <0x7e200000 0x1000>;
+			status = "okay";
+		};
+	};
+};
+
+&intc {
+	compatible = "brcm,bcm2835-armctrl-ic";
+};
+
+&watchdog {
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708_common.dtsi
@@ -0,0 +1,347 @@
+#include "skeleton.dtsi"
+
+/ {
+	interrupt-parent = <&intc>;
+
+	aliases {
+		audio = &audio;
+		sound = &sound;
+		soc = &soc;
+		dma = &dma;
+		intc = &intc;
+		watchdog = &watchdog;
+		random = &random;
+		mailbox = &mailbox;
+		gpio = &gpio;
+		uart0 = &uart0;
+		sdhost = &sdhost;
+		i2s  = &i2s;
+		spi0 = &spi0;
+		i2c0 = &i2c0;
+		uart1 = &uart1;
+		mmc = &mmc;
+		i2c1 = &i2c1;
+		i2c2 = &i2c2;
+		usb = &usb;
+		leds = &leds;
+		fb = &fb;
+		vchiq = &vchiq;
+		thermal = &thermal;
+		clocks = &clocks;
+	};
+
+	/* Onboard audio */
+	audio: audio {
+		compatible = "brcm,bcm2835-audio";
+		brcm,pwm-channels = <8>;
+		status = "disabled";
+	};
+
+	/* External sound card */
+	sound: sound {
+	};
+
+	soc: soc {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+
+		dma: dma@7e007000 {
+			compatible = "brcm,bcm2835-dma";
+			reg = <0x7e007000 0xf00>;
+			interrupts = <1 16>,
+				     <1 17>,
+				     <1 18>,
+				     <1 19>,
+				     <1 20>,
+				     <1 21>,
+				     <1 22>,
+				     <1 23>,
+				     <1 24>,
+				     <1 25>,
+				     <1 26>,
+				     <1 27>;
+
+			#dma-cells = <1>;
+			brcm,dma-channel-mask = <0x0f35>;
+		};
+
+		intc: interrupt-controller@7e00b200 {
+			compatible = "brcm,bcm2708-armctrl-ic";
+			reg = <0x7e00b200 0x200>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		mailbox: mailbox@7e00b800 {
+			compatible = "brcm,bcm2835-mbox";
+			reg = <0x7e00b880 0x40>;
+			interrupts = <0 1>;
+			#mbox-cells = <0>;
+		};
+
+		watchdog: watchdog@7e100000 {
+			compatible = "brcm,bcm2835-pm-wdt";
+			reg = <0x7e100000 0x28>;
+			status = "disabled";
+		};
+
+		cprman: cprman@7e101000 {
+			compatible = "brcm,bcm2835-cprman";
+			#clock-cells = <1>;
+			reg = <0x7e101000 0x2000>;
+
+			/* CPRMAN derives everything from the platform's
+			 * oscillator.
+			 */
+			clocks = <&clk_osc>;
+			status = "disabled";
+		};
+
+		random: rng@7e104000 {
+			compatible = "brcm,bcm2835-rng";
+			reg = <0x7e104000 0x10>;
+			status = "disabled";
+		};
+
+		gpio: gpio@7e200000 {
+			compatible = "brcm,bcm2835-gpio";
+			reg = <0x7e200000 0xb4>;
+			interrupts = <2 17>, <2 18>;
+
+			gpio-controller;
+			#gpio-cells = <2>;
+
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		uart0: uart@7e201000 {
+			compatible = "arm,pl011", "arm,primecell";
+			reg = <0x7e201000 0x1000>;
+			interrupts = <2 25>;
+			clocks = <&clk_uart0 &clk_apb_p>;
+			clock-names = "uartclk","apb_pclk";
+			arm,primecell-periphid = <0x00241011>; // For an explanation, see
+			// https://github.com/raspberrypi/linux/commit/13731d862cf5219216533a3b0de052cee4cc5038
+			status = "disabled";
+		};
+
+		sdhost: sdhost@7e202000 {
+			compatible = "brcm,bcm2835-sdhost";
+			reg = <0x7e202000 0x100>;
+			interrupts = <2 24>;
+			clocks = <&clk_core>;
+			dmas = <&dma 13>,
+			       <&dma 13>;
+			dma-names = "tx", "rx";
+			brcm,pio-limit = <1>;
+			status = "disabled";
+		};
+
+		i2s: i2s@7e203000 {
+			compatible = "brcm,bcm2835-i2s";
+			reg = <0x7e203000 0x24>,
+			      <0x7e101098 0x08>;
+
+			dmas = <&dma 2>, <&dma 3>;
+			dma-names = "tx", "rx";
+			status = "disabled";
+		};
+
+		spi0: spi@7e204000 {
+			compatible = "brcm,bcm2835-spi";
+			reg = <0x7e204000 0x1000>;
+			interrupts = <2 22>;
+			clocks = <&clk_core>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+			/* the dma channels */
+			dmas = <&dma 6>, <&dma 7>;
+			dma-names = "tx", "rx";
+			/* the chipselects used - <0> means native GPIO
+			 * add more gpios if necessary as <&gpio 6 1>
+			 * (but do not forget to make them output!)
+			 */
+			cs-gpios = <0>, <0>;
+		};
+
+		i2c0: i2c@7e205000 {
+			compatible = "brcm,bcm2708-i2c";
+			reg = <0x7e205000 0x1000>;
+			interrupts = <2 21>;
+			clocks = <&clk_core>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		pwm: pwm@7e20c000 {
+			compatible = "brcm,bcm2835-pwm";
+			reg = <0x7e20c000 0x28>;
+			clocks = <&clk_pwm>;
+			#pwm-cells = <2>;
+			status = "disabled";
+		};
+
+		uart1: uart@7e215040 {
+			compatible = "brcm,bcm2835-aux-uart", "ns16550";
+			reg = <0x7e215040 0x40>;
+			interrupts = <1 29>;
+			clocks = <&clk_uart1>;
+			reg-shift = <2>;
+			no-loopback-test;
+			status = "disabled";
+	        };
+
+		mmc: mmc@7e300000 {
+			compatible = "brcm,bcm2835-mmc";
+			reg = <0x7e300000 0x100>;
+			interrupts = <2 30>;
+			clocks = <&clk_mmc>;
+			dmas = <&dma 11>,
+			       <&dma 11>;
+			dma-names = "tx", "rx";
+			status = "disabled";
+		};
+
+		i2c1: i2c@7e804000 {
+			compatible = "brcm,bcm2708-i2c";
+			reg = <0x7e804000 0x1000>;
+			interrupts = <2 21>;
+			clocks = <&clk_core>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c2: i2c@7e805000 {
+			// Beware - this is shared with the HDMI module.
+			// Careless use may break (really) your display.
+			// Caveat emptor.
+			compatible = "brcm,bcm2708-i2c";
+			reg = <0x7e805000 0x1000>;
+			interrupts = <2 21>;
+			clocks = <&clk_core>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		smi: smi@7e600000 {
+			compatible = "brcm,bcm2835-smi";
+			reg = <0x7e600000 0x44>, <0x7e1010b0 0x8>;
+			interrupts = <2 16>;
+			brcm,smi-clock-source = <6>;
+			brcm,smi-clock-divisor = <4>;
+			dmas = <&dma 4>;
+			dma-names = "rx-tx";
+			status = "disabled";
+		};
+
+		usb: usb@7e980000 {
+			compatible = "brcm,bcm2708-usb";
+			reg = <0x7e980000 0x10000>,
+			      <0x7e006000 0x1000>;
+			interrupts = <2 0>,
+				     <1 9>;
+		};
+
+		firmware: firmware {
+			compatible = "raspberrypi,bcm2835-firmware";
+			mboxes = <&mailbox>;
+		};
+
+		leds: leds {
+			compatible = "gpio-leds";
+		};
+
+		fb: fb {
+			compatible = "brcm,bcm2708-fb";
+			firmware = <&firmware>;
+			status = "disabled";
+		};
+
+		vchiq: vchiq {
+			compatible = "brcm,bcm2835-vchiq";
+			reg = <0x7e00b840 0xf>;
+			interrupts = <0 2>;
+			cache-line-size = <32>;
+			firmware = <&firmware>;
+		};
+
+		thermal: thermal {
+			compatible = "brcm,bcm2835-thermal";
+			firmware = <&firmware>;
+		};
+	};
+
+	clocks: clocks {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		clk_core: clock@0 {
+			compatible = "fixed-clock";
+			reg = <0>;
+			#clock-cells = <0>;
+			clock-output-names = "core";
+			clock-frequency = <250000000>;
+		};
+
+		clk_mmc: clock@1 {
+			compatible = "fixed-clock";
+			reg = <1>;
+			#clock-cells = <0>;
+			clock-output-names = "mmc";
+			clock-frequency = <250000000>;
+		};
+
+		clk_uart0: clock@2 {
+			compatible = "fixed-clock";
+			reg = <2>;
+			#clock-cells = <0>;
+			clock-output-names = "uart0_pclk";
+			clock-frequency = <3000000>;
+		};
+
+		clk_apb_p: clock@3 {
+			compatible = "fixed-clock";
+			reg = <3>;
+			#clock-cells = <0>;
+			clock-output-names = "apb_pclk";
+			clock-frequency = <126000000>;
+		};
+
+		clk_pwm: clock@4 {
+			compatible = "fixed-clock";
+			reg = <4>;
+			#clock-cells = <0>;
+			clock-output-names = "pwm";
+			clock-frequency = <100000000>;
+		};
+
+		clk_uart1: clock@5 {
+			compatible = "fixed-factor-clock";
+			reg = <5>;
+			clocks = <&clk_core>;
+			#clock-cells = <0>;
+			clock-div = <1>;
+			clock-mult = <2>;
+		};
+
+		/* The oscillator is the root of the clock tree. */
+		clk_osc: clock@6 {
+			compatible = "fixed-clock";
+			reg = <6>;
+			#clock-cells = <0>;
+			clock-output-names = "osc";
+			clock-frequency = <19200000>;
+		};
+	};
+
+	__overrides__ {
+		cache_line_size = <&vchiq>, "cache-line-size:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
@@ -0,0 +1,145 @@
+/dts-v1/;
+
+#include "bcm2709.dtsi"
+
+/ {
+	compatible = "brcm,bcm2709";
+	model = "Raspberry Pi 2 Model B";
+};
+
+&gpio {
+	sdhost_pins: sdhost_pins {
+		brcm,pins = <48 49 50 51 52 53>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+};
+
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&fb {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&random {
+	status = "okay";
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&gpio 35 0>;
+	};
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2709.dtsi
@@ -0,0 +1,102 @@
+#include "bcm2708_common.dtsi"
+
+/ {
+	compatible = "brcm,bcm2709";
+	model = "BCM2709";
+
+	chosen {
+		/* No padding required - the boot loader can do that. */
+		bootargs = "";
+	};
+
+	soc {
+		ranges = <0x7e000000 0x3f000000 0x01000000>,
+		         <0x40000000 0x40000000 0x00040000>;
+
+		local_intc: local_intc {
+			compatible = "brcm,bcm2836-l1-intc";
+			reg = <0x40000000 0x100>;
+			interrupt-controller;
+			#interrupt-cells = <1>;
+			interrupt-parent = <&local_intc>;
+		};
+
+		arm-pmu {
+			compatible = "arm,cortex-a7-pmu";
+			interrupt-parent = <&local_intc>;
+			interrupts = <9>;
+		};
+
+		gpiomem {
+			compatible = "brcm,bcm2835-gpiomem";
+			reg = <0x7e200000 0x1000>;
+			status = "okay";
+		};
+
+		timer {
+			compatible = "arm,armv7-timer";
+			clock-frequency = <19200000>;
+			interrupt-parent = <&local_intc>;
+			interrupts = <0>, // PHYS_SECURE_PPI
+				     <1>, // PHYS_NONSECURE_PPI
+				     <3>, // VIRT_PPI
+				     <2>; // HYP_PPI
+			always-on;
+		};
+
+		syscon@40000000 {
+			compatible = "brcm,bcm2836-arm-local", "syscon";
+			reg = <0x40000000 0x100>;
+		};
+	};
+
+	cpus: cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		v7_cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf00>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf01>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf02>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf03>;
+			clock-frequency = <800000000>;
+		};
+	};
+
+	__overrides__ {
+		arm_freq = <&v7_cpu0>, "clock-frequency:0",
+		       <&v7_cpu1>, "clock-frequency:0",
+		       <&v7_cpu2>, "clock-frequency:0",
+		       <&v7_cpu3>, "clock-frequency:0";
+	};
+};
+
+&watchdog {
+	status = "okay";
+};
+
+&intc {
+        compatible = "brcm,bcm2836-armctrl-ic";
+        interrupt-parent = <&local_intc>;
+        interrupts = <8>;
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2835-rpi-cm.dts
@@ -0,0 +1,93 @@
+/dts-v1/;
+
+#include "bcm2835-rpi-cm.dtsi"
+
+/ {
+	model = "Raspberry Pi Compute Module";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <7 8 9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		uart1_clkrate = <&uart1>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2835-rpi-cm.dtsi
@@ -0,0 +1,30 @@
+#include "bcm2835.dtsi"
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+};
+
+&mmc {
+	status = "okay";
+	bus-width = <4>;
+};
+
+&fb {
+	status = "okay";
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/Makefile
@@ -0,0 +1,69 @@
+ifeq ($(CONFIG_OF),y)
+
+# Overlays for the Raspberry Pi platform
+
+ifeq ($(CONFIG_ARCH_BCM2708),y)
+   RPI_DT_OVERLAYS=y
+endif
+ifeq ($(CONFIG_ARCH_BCM2709),y)
+   RPI_DT_OVERLAYS=y
+endif
+ifeq ($(CONFIG_ARCH_BCM2835),y)
+   RPI_DT_OVERLAYS=y
+endif
+
+dtb-$(RPI_DT_OVERLAYS) += ads7846-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += bmp085_i2c-sensor-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += dht11-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += enc28j60-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += gpio-poweroff-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += hifiberry-amp-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += hifiberry-dac-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += hifiberry-dacplus-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += hifiberry-digi-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += hy28a-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += hy28b-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += i2c-rtc-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += i2s-mmap-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += iqaudio-dac-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += iqaudio-dacplus-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += lirc-rpi-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += mcp2515-can0-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += mcp2515-can1-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += mmc-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += mz61581-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += piscreen-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += pitft28-resistive-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += pps-gpio-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += pwm-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += pwm-2chan-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += raspidac3-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += rpi-dac-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += rpi-display-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += rpi-ft5406-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += rpi-proto-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += rpi-sense-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += sdhost-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += sdio-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += smi-dev-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += smi-nand-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += smi-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += spi-gpio35-39-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += tinylcd35-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += uart1-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += vga666-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += w1-gpio-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += w1-gpio-pullup-overlay.dtb
+
+targets += dtbs dtbs_install
+targets += $(dtb-y)
+
+endif
+
+always		:= $(dtb-y)
+clean-files	:= *.dtb
+
+# Enable fixups to support overlays on BCM2708 platforms
+ifeq ($(RPI_DT_OVERLAYS),y)
+	DTC_FLAGS ?= -@
+endif
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/README
@@ -0,0 +1,648 @@
+Introduction
+============
+
+This directory contains Device Tree overlays. Device Tree makes it possible
+to support many hardware configurations with a single kernel and without the
+need to explicitly load or blacklist kernel modules. Note that this isn't a
+"pure" Device Tree configuration (c.f. MACH_BCM2835) - some on-board devices
+are still configured by the board support code, but the intention is to
+eventually reach that goal.
+
+On Raspberry Pi, Device Tree usage is controlled from /boot/config.txt. By
+default, the Raspberry Pi kernel boots with device tree enabled. You can
+completely disable DT usage (for now) by adding:
+
+    device_tree=
+
+to your config.txt, which should cause your Pi to revert to the old way of
+doing things after a reboot.
+
+In /boot you will find a .dtb for each base platform. This describes the
+hardware that is part of the Raspberry Pi board. The loader (start.elf and its
+siblings) selects the .dtb file appropriate for the platform by name, and reads
+it into memory. At this point, all of the optional interfaces (i2c, i2s, spi)
+are disabled, but they can be enabled using Device Tree parameters:
+
+    dtparam=i2c=on,i2s=on,spi=on
+
+However, this shouldn't be necessary in many use cases because loading an
+overlay that requires one of those interfaces will cause it to be enabled
+automatically, and it is advisable to only enable interfaces if they are
+needed.
+
+Configuring additional, optional hardware is done using Device Tree overlays
+(see below).
+
+raspi-config
+============
+
+The Advanced Options section of the raspi-config utility can enable and disable
+Device Tree use, as well as toggling the I2C and SPI interfaces. Note that it
+is possible to both enable an interface and blacklist the driver, if for some
+reason you should want to defer the loading.
+
+Modules
+=======
+
+As well as describing the hardware, Device Tree also gives enough information
+to allow suitable driver modules to be located and loaded, with the corollary
+that unneeded modules are not loaded. As a result it should be possible to
+remove lines from /etc/modules, and /etc/modprobe.d/raspi-blacklist.conf can
+have its contents deleted (or commented out).
+
+Using Overlays
+==============
+
+Overlays are loaded using the "dtoverlay" directive. As an example, consider the
+popular lirc-rpi module, the Linux Infrared Remote Control driver. In the
+pre-DT world this would be loaded from /etc/modules, with an explicit
+"modprobe lirc-rpi" command, or programmatically by lircd. With DT enabled,
+this becomes a line in config.txt:
+
+    dtoverlay=lirc-rpi
+
+This causes the file /boot/overlays/lirc-rpi-overlay.dtb to be loaded. By
+default it will use GPIOs 17 (out) and 18 (in), but this can be modified using
+DT parameters:
+
+    dtoverlay=lirc-rpi,gpio_out_pin=17,gpio_in_pin=13
+
+Parameters always have default values, although in some cases (e.g. "w1-gpio")
+it is necessary to provided multiple overlays in order to get the desired
+behaviour. See the list of overlays below for a description of the parameters and their defaults.
+
+The Overlay and Parameter Reference
+===================================
+
+N.B. When editing this file, please preserve the indentation levels to make it simple to parse
+programmatically. NO HARD TABS.
+
+
+Name:   <The base DTB>
+Info:   Configures the base Raspberry Pi hardware
+Load:   <loaded automatically>
+Params:
+        audio                    Set to "on" to enable the onboard ALSA audio
+                                 interface (default "off")
+
+        i2c_arm                  Set to "on" to enable the ARM's i2c interface
+                                 (default "off")
+
+        i2c_vc                   Set to "on" to enable the i2c interface
+                                 usually reserved for the VideoCore processor
+                                 (default "off")
+
+        i2c                      An alias for i2c_arm
+
+        i2c_arm_baudrate         Set the baudrate of the ARM's i2c interface
+                                 (default "100000")
+
+        i2c_vc_baudrate          Set the baudrate of the VideoCore i2c interface
+                                 (default "100000")
+
+        i2c_baudrate             An alias for i2c_arm_baudrate
+
+        i2s                      Set to "on" to enable the i2s interface
+                                 (default "off")
+
+        spi                      Set to "on" to enable the spi interfaces
+                                 (default "off")
+
+        random                   Set to "on" to enable the hardware random
+                                 number generator (default "on")
+
+        uart0                    Set to "off" to disable uart0 (default "on")
+
+        watchdog                 Set to "on" to enable the hardware watchdog
+                                 (default "off")
+
+        act_led_trigger          Choose which activity the LED tracks.
+                                 Use "heartbeat" for a nice load indicator.
+                                 (default "mmc")
+
+        act_led_activelow        Set to "on" to invert the sense of the LED
+                                 (default "off")
+
+        act_led_gpio             Set which GPIO to use for the activity LED
+                                 (in case you want to connect it to an external
+                                 device)
+                                 (default "16" on a non-Plus board, "47" on a
+                                 Plus or Pi 2)
+
+        pwr_led_trigger
+        pwr_led_activelow
+        pwr_led_gpio
+                                 As for act_led_*, but using the PWR LED.
+                                 Not available on Model A/B boards.
+
+        N.B. It is recommended to only enable those interfaces that are needed.
+        Leaving all interfaces enabled can lead to unwanted behaviour (i2c_vc
+        interfering with Pi Camera, I2S and SPI hogging GPIO pins, etc.)
+        Note also that i2c, i2c_arm and i2c_vc are aliases for the physical
+        interfaces i2c0 and i2c1. Use of the numeric variants is still possible
+        but deprecated because the ARM/VC assignments differ between board
+        revisions. The same board-specific mapping applies to i2c_baudrate,
+        and the other i2c baudrate parameters.
+
+
+Name:   ads7846
+Info:   ADS7846 Touch controller
+Load:   dtoverlay=ads7846,<param>=<val>
+Params: cs                       SPI bus Chip Select (default 1)
+        speed                    SPI bus speed (default 2Mhz, max 3.25MHz)
+        penirq                   GPIO used for PENIRQ. REQUIRED
+        penirq_pull              Set GPIO pull (default 0=none, 2=pullup)
+        swapxy                   Swap x and y axis
+        xmin                     Minimum value on the X axis (default 0)
+        ymin                     Minimum value on the Y axis (default 0)
+        xmax                     Maximum value on the X axis (default 4095)
+        ymax                     Maximum value on the Y axis (default 4095)
+        pmin                     Minimum reported pressure value (default 0)
+        pmax                     Maximum reported pressure value (default 65535)
+        xohms                    Touchpanel sensitivity (X-plate resistance)
+                                 (default 400)
+
+        penirq is required and usually xohms (60-100) has to be set as well.
+        Apart from that, pmax (255) and swapxy are also common.
+        The rest of the calibration can be done with xinput-calibrator.
+        See: github.com/notro/fbtft/wiki/FBTFT-on-Raspian
+        Device Tree binding document:
+        www.kernel.org/doc/Documentation/devicetree/bindings/input/ads7846.txt
+
+
+Name:   bmp085_i2c-sensor
+Info:   Configures the BMP085/BMP180 digital barometric pressure and temperature
+        sensors from Bosch Sensortec
+Load:   dtoverlay=bmp085_i2c-sensor
+Params: <None>
+
+
+Name:   dht11
+Info:   Overlay for the DHT11/DHT21/DHT22 humidity/temperature sensors
+        Also sometimes found with the part number(s) AM230x.
+Load:   dtoverlay=dht11,<param>=<val>
+Params: gpiopin                  GPIO connected to the sensor's DATA output.
+                                 (default 4)
+
+
+[ The ds1307-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+Name:   enc28j60
+Info:   Overlay for the Microchip ENC28J60 Ethernet Controller (SPI)
+Load:   dtoverlay=enc28j60,<param>=<val>
+Params: int_pin                  GPIO used for INT (default 25)
+
+        speed                    SPI bus speed (default 12000000)
+
+
+Name:   gpio-poweroff
+Info:   Drives a GPIO high or low on reboot
+Load:   dtoverlay=gpio-poweroff,<param>=<val>
+Params: gpiopin                  GPIO for signalling (default 26)
+
+        active_low               Set if the power control device requires a
+                                 high->low transition to trigger a power-down.
+                                 Note that this will require the support of a
+                                 custom dt-blob.bin to prevent a power-down
+                                 during the boot process, and that a reboot
+                                 will also cause the pin to go low.
+
+
+Name:   hifiberry-amp
+Info:   Configures the HifiBerry Amp and Amp+ audio cards
+Load:   dtoverlay=hifiberry-amp
+Params: <None>
+
+
+Name:   hifiberry-dac
+Info:   Configures the HifiBerry DAC audio card
+Load:   dtoverlay=hifiberry-dac
+Params: <None>
+
+
+Name:   hifiberry-dacplus
+Info:   Configures the HifiBerry DAC+ audio card
+Load:   dtoverlay=hifiberry-dacplus
+Params: <None>
+
+
+Name:   hifiberry-digi
+Info:   Configures the HifiBerry Digi audio card
+Load:   dtoverlay=hifiberry-digi
+Params: <None>
+
+
+Name:   hy28a
+Info:   HY28A - 2.8" TFT LCD Display Module by HAOYU Electronics
+        Default values match Texy's display shield
+Load:   dtoverlay=hy28a,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        debug                    Debug output level {0-7}
+
+        xohms                    Touchpanel sensitivity (X-plate resistance)
+
+        resetgpio                GPIO used to reset controller
+
+        ledgpio                  GPIO used to control backlight
+
+
+Name:   hy28b
+Info:   HY28B - 2.8" TFT LCD Display Module by HAOYU Electronics
+        Default values match Texy's display shield
+Load:   dtoverlay=hy28b,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        debug                    Debug output level {0-7}
+
+        xohms                    Touchpanel sensitivity (X-plate resistance)
+
+        resetgpio                GPIO used to reset controller
+
+        ledgpio                  GPIO used to control backlight
+
+
+Name:   i2c-rtc
+Info:   Adds support for a number of I2C Real Time Clock devices
+Load:   dtoverlay=i2c-rtc,<param>
+Params: ds1307                   Select the DS1307 device
+
+        ds3231                   Select the DS3231 device
+
+        mcp7941x                 Select the MCP7941x device
+
+        pcf2127                  Select the PCF2127 device
+
+        pcf8523                  Select the PCF8523 device
+
+        pcf8563                  Select the PCF8563 device
+
+
+Name:   i2s-mmap
+Info:   Enables mmap support in the bcm2708-i2s driver
+Load:   dtoverlay=i2s-mmap
+Params: <None>
+
+
+Name:   iqaudio-dac
+Info:   Configures the IQaudio DAC audio card
+Load:   dtoverlay=iqaudio-dac
+Params: <None>
+
+
+Name:   iqaudio-dacplus
+Info:   Configures the IQaudio DAC+ audio card
+Load:   dtoverlay=iqaudio-dacplus
+Params: <None>
+
+
+Name:   lirc-rpi
+Info:   Configures lirc-rpi (Linux Infrared Remote Control for Raspberry Pi)
+        Consult the module documentation for more details.
+Load:   dtoverlay=lirc-rpi,<param>=<val>,...
+Params: gpio_out_pin             GPIO for output (default "17")
+
+        gpio_in_pin              GPIO for input (default "18")
+
+        gpio_in_pull             Pull up/down/off on the input pin
+                                 (default "down")
+
+        sense                    Override the IR receive auto-detection logic:
+                                   "0" = force active-high
+                                   "1" = force active-low
+                                   "-1" = use auto-detection
+                                 (default "-1")
+
+        softcarrier              Turn the software carrier "on" or "off"
+                                 (default "on")
+
+        invert                   "on" = invert the output pin (default "off")
+
+        debug                    "on" = enable additional debug messages
+                                 (default "off")
+
+
+Name:   mcp2515-can0
+Info:   Configures the MCP2515 CAN controller on spi0.0
+Load:   dtoverlay=mcp2515-can0,<param>=<val>
+Params: oscillator               Clock frequency for the CAN controller (Hz)
+
+        spimaxfrequency          Maximum SPI frequence (Hz)
+
+        interrupt                GPIO for interrupt signal
+
+
+Name:   mcp2515-can1
+Info:   Configures the MCP2515 CAN controller on spi0.1
+Load:   dtoverlay=mcp2515-can1,<param>=<val>
+Params: oscillator               Clock frequency for the CAN controller (Hz)
+
+        spimaxfrequency          Maximum SPI frequence (Hz)
+
+        interrupt                GPIO for interrupt signal
+
+
+Name:   mmc
+Info:   Selects the bcm2835-mmc SD/MMC driver, optionally with overclock
+Load:   dtoverlay=mmc,<param>=<val>
+Params: overclock_50             Clock (in MHz) to use when the MMC framework
+                                 requests 50MHz
+        force_pio                Disable DMA support
+
+
+Name:   mz61581
+Info:   MZ61581 display by Tontec
+Load:   dtoverlay=mz61581,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        txbuflen                 Transmit buffer length (default 32768)
+
+        debug                    Debug output level {0-7}
+
+        xohms                    Touchpanel sensitivity (X-plate resistance)
+
+
+[ The pcf2127-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+[ The pcf8523-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+[ The pcf8563-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+Name:   piscreen
+Info:   PiScreen display by OzzMaker.com
+Load:   dtoverlay=piscreen,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        debug                    Debug output level {0-7}
+
+        xohms                    Touchpanel sensitivity (X-plate resistance)
+
+
+Name:   pitft28-resistive
+Info:   Adafruit PiTFT 2.8" resistive touch screen
+Load:   dtoverlay=pitft28-resistive,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        debug                    Debug output level {0-7}
+
+
+Name:   pps-gpio
+Info:   Configures the pps-gpio (pulse-per-second time signal via GPIO).
+Load:   dtoverlay=pps-gpio,<param>=<val>
+Params: gpiopin                  Input GPIO (default "18")
+
+
+Name:   pwm
+Info:   Configures a single PWM channel
+        Legal pin,function combinations for each channel:
+          PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+          PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+        N.B.:
+          1) Pin 18 is the only one available on all platforms, and
+             it is the one used by the I2S audio interface.
+             Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+          2) The onboard analogue audio output uses both PWM channels.
+          3) So be careful mixing audio and PWM.
+          4) Currently the clock must have been enabled and configured
+             by other means.
+Load:   dtoverlay=pwm,<param>=<val>
+Params: pin                      Output pin (default 18) - see table
+        func                     Pin function (default 2 = Alt5) - see above
+        clock                    PWM clock frequency (informational)
+
+
+Name:   pwm-2chan
+Info:   Configures both PWM channels
+        Legal pin,function combinations for each channel:
+          PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+          PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+        N.B.:
+          1) Pin 18 is the only one available on all platforms, and
+             it is the one used by the I2S audio interface.
+             Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+          2) The onboard analogue audio output uses both PWM channels.
+          3) So be careful mixing audio and PWM.
+          4) Currently the clock must have been enabled and configured
+             by other means.
+Load:   dtoverlay=pwm-2chan,<param>=<val>
+Params: pin                      Output pin (default 18) - see table
+        pin2                     Output pin for other channel (default 19)
+        func                     Pin function (default 2 = Alt5) - see above
+        func2                    Function for pin2 (default 2 = Alt5)
+        clock                    PWM clock frequency (informational)
+
+
+Name:   raspidac3
+Info:   Configures the RaspiDAV Rev.3x audio card
+Load:   dtoverlay=raspidac3
+Params: <None>
+
+
+Name:   rpi-dac
+Info:   Configures the RPi DAC audio card
+Load:   dtoverlay=rpi-dac
+Params: <None>
+
+
+Name:   rpi-display
+Info:   RPi-Display - 2.8" Touch Display by Watterott
+Load:   dtoverlay=rpi-display,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        debug                    Debug output level {0-7}
+
+        xohms                    Touchpanel sensitivity (X-plate resistance)
+
+
+Name:   rpi-ft5406
+Info:   Official Raspberry Pi display touchscreen
+Load:   dtoverlay=rpi-ft5406
+Params: <None>
+
+
+Name:   rpi-proto
+Info:   Configures the RPi Proto audio card
+Load:   dtoverlay=rpi-proto
+Params: <None>
+
+
+Name:   rpi-sense
+Info:   Raspberry Pi Sense HAT
+Load:   dtoverlay=rpi-sense
+Params: <None>
+
+
+Name:   sdhost
+Info:   Selects the bcm2835-sdhost SD/MMC driver, optionally with overclock
+Load:   dtoverlay=sdhost,<param>=<val>
+Params: overclock_50             Clock (in MHz) to use when the MMC framework
+                                 requests 50MHz
+
+        force_pio                Disable DMA support (default off)
+
+        pio_limit                Number of blocks above which to use DMA
+                                 (default 1)
+
+        debug                    Enable debug output (default off)
+
+
+Name:   sdio
+Info:   Selects the bcm2835-sdhost SD/MMC driver, optionally with overclock,
+        and enables SDIO via GPIOs 22-27.
+Load:   dtoverlay=sdio,<param>=<val>
+Params: overclock_50             Clock (in MHz) to use when the MMC framework
+                                 requests 50MHz
+
+        force_pio                Disable DMA support (default off)
+
+        pio_limit                Number of blocks above which to use DMA
+                                 (default 1)
+
+        debug                    Enable debug output (default off)
+
+        poll_once                Disable SDIO-device polling every second
+                                 (default on: polling once at boot-time)
+
+
+Name:   smi
+Info:   Enables the Secondary Memory Interface peripheral. Uses GPIOs 2-25!
+Load:   dtoverlay=smi
+Params: <None>
+
+
+Name:   smi-dev
+Info:   Enables the userspace interface for the SMI driver
+Load:   dtoverlay=smi-dev
+Params: <None>
+
+
+Name:   smi-nand
+Info:   Enables access to NAND flash via the SMI interface
+Load:   dtoverlay=smi-nand
+Params: <None>
+
+
+Name:   spi-gpio35-39
+Info:   move SPI function block to GPIO 35 to 39
+Load:   dtoverlay=spi-gpio35-39
+Params: <None>
+
+
+Name:   tinylcd35
+Info:   3.5" Color TFT Display by www.tinylcd.com
+        Options: Touch, RTC, keypad
+Load:   dtoverlay=tinylcd35,<param>=<val>
+Params: speed                    Display SPI bus speed
+
+        rotate                   Display rotation {0,90,180,270}
+
+        fps                      Delay between frame updates
+
+        debug                    Debug output level {0-7}
+
+        touch                    Enable touch panel
+
+        touchgpio                Touch controller IRQ GPIO
+
+        xohms                    Touchpanel: Resistance of X-plate in ohms
+
+        rtc-pcf                  PCF8563 Real Time Clock
+
+        rtc-ds                   DS1307 Real Time Clock
+
+        keypad                   Enable keypad
+
+        Examples:
+            Display with touchpanel, PCF8563 RTC and keypad:
+                dtoverlay=tinylcd35,touch,rtc-pcf,keypad
+            Old touch display:
+                dtoverlay=tinylcd35,touch,touchgpio=3
+
+
+Name:   uart1
+Info:   Enable uart1 in place of uart0
+Load:   dtoverlay=uart1,<param>=<val>
+Params: txd1_pin                 GPIO pin for TXD1 (14, 32 or 40 - default 14)
+
+        rxd1_pin                 GPIO pin for RXD1 (15, 33 or 41 - default 15)
+
+
+Name:   vga666
+Info:   Overlay for the Fen Logic VGA666 board
+        This uses GPIOs 2-21 (so no I2C), and activates the output 2-3 seconds
+        after the kernel has started.
+Load:   dtoverlay=vga666
+Params: <None>
+
+
+Name:   w1-gpio
+Info:   Configures the w1-gpio Onewire interface module.
+        Use this overlay if you *don't* need a GPIO to drive an external pullup.
+Load:   dtoverlay=w1-gpio,<param>=<val>
+Params: gpiopin                  GPIO for I/O (default "4")
+
+        pullup                   Non-zero, "on", or "y" to enable the parasitic
+                                 power (2-wire, power-on-data) feature
+
+
+Name:   w1-gpio-pullup
+Info:   Configures the w1-gpio Onewire interface module.
+        Use this overlay if you *do* need a GPIO to drive an external pullup.
+Load:   dtoverlay=w1-gpio-pullup,<param>=<val>
+Params: gpiopin                  GPIO for I/O (default "4")
+
+        pullup                   Non-zero, "on", or "y" to enable the parasitic
+                                 power (2-wire, power-on-data) feature
+
+        extpullup                GPIO for external pullup (default "5")
+
+
+Troubleshooting
+===============
+
+If you are experiencing problems that you think are DT-related, enable DT
+diagnostic output by adding this to /boot/config.txt:
+
+    dtdebug=on
+
+and rebooting. Then run:
+
+    sudo vcdbg log msg
+
+and look for relevant messages.
+
+Further reading
+===============
+
+This is only meant to be a quick introduction to the subject of Device Tree on
+Raspberry Pi. There is a more complete explanation here:
+
+http://www.raspberrypi.org/documentation/configuration/device-tree.md
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ads7846-overlay.dts
@@ -0,0 +1,83 @@
+/*
+ * Generic Device Tree overlay for the ADS7846 touch controller
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			ads7846_pins: ads7846_pins {
+				brcm,pins = <255>; /* illegal default value */
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			ads7846: ads7846@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&ads7846_pins>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <255 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 255 0>;
+
+				/* driver defaults */
+				ti,x-min = /bits/ 16 <0>;
+				ti,y-min = /bits/ 16 <0>;
+				ti,x-max = /bits/ 16 <0x0FFF>;
+				ti,y-max = /bits/ 16 <0x0FFF>;
+				ti,pressure-min = /bits/ 16 <0>;
+				ti,pressure-max = /bits/ 16 <0xFFFF>;
+				ti,x-plate-ohms = /bits/ 16 <400>;
+			};
+		};
+	};
+	__overrides__ {
+		cs =     <&ads7846>,"reg:0";
+		speed =  <&ads7846>,"spi-max-frequency:0";
+		penirq = <&ads7846_pins>,"brcm,pins:0", /* REQUIRED */
+			 <&ads7846>,"interrupts:0",
+			 <&ads7846>,"pendown-gpio:4";
+		penirq_pull = <&ads7846_pins>,"brcm,pull:0";
+		swapxy = <&ads7846>,"ti,swap-xy?";
+		xmin =   <&ads7846>,"ti,x-min;0";
+		ymin =   <&ads7846>,"ti,y-min;0";
+		xmax =   <&ads7846>,"ti,x-max;0";
+		ymax =   <&ads7846>,"ti,y-max;0";
+		pmin =   <&ads7846>,"ti,pressure-min;0";
+		pmax =   <&ads7846>,"ti,pressure-max;0";
+		xohms =  <&ads7846>,"ti,x-plate-ohms;0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/bmp085_i2c-sensor-overlay.dts
@@ -0,0 +1,23 @@
+// Definitions for BMP085/BMP180 digital barometric pressure and temperature sensors from Bosch Sensortec
+/dts-v1/;
+/plugin/;
+
+/ {
+        compatible = "brcm,bcm2708";
+
+        fragment@0 {
+                target = <&i2c_arm>;
+                __overlay__ {
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+                        status = "okay";
+
+                        bmp085@77 {
+                                compatible = "bosch,bmp085";
+                                reg = <0x77>;
+                                default-oversampling = <3>;
+                                status = "okay";
+                        };
+                };
+        };
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dht11-overlay.dts
@@ -0,0 +1,39 @@
+/*
+ * Overlay for the DHT11/21/22 humidity/temperature sensor modules.
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+
+			dht11: dht11@0 {
+				compatible = "dht11";
+				pinctrl-names = "default";
+				pinctrl-0 = <&dht11_pins>;
+				gpios = <&gpio 4 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			dht11_pins: dht11_pins {
+				brcm,pins = <4>;
+				brcm,function = <0>; // in
+				brcm,pull = <0>; // off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin = <&dht11_pins>,"brcm,pins:0",
+			<&dht11>,"gpios:4";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/enc28j60-overlay.dts
@@ -0,0 +1,50 @@
+// Overlay for the Microchip ENC28J60 Ethernet Controller
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			eth1: enc28j60@0{
+				compatible = "microchip,enc28j60";
+				reg = <0>; /* CE0 */
+				pinctrl-names = "default";
+				pinctrl-0 = <&eth1_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <25 0x2>; /* falling edge */
+				spi-max-frequency = <12000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			eth1_pins: eth1_pins {
+				brcm,pins = <25>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&eth1>, "interrupts:0",
+		          <&eth1_pins>, "brcm,pins:0";
+		speed   = <&eth1>, "spi-max-frequency:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-poweroff-overlay.dts
@@ -0,0 +1,34 @@
+// Definitions for gpio-poweroff module
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			power_ctrl: power_ctrl {
+				compatible = "gpio-poweroff";
+				gpios = <&gpio 26 0>;
+				force;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			power_ctrl_pins: power_ctrl_pins {
+				brcm,pins = <26>;
+				brcm,function = <1>; // out
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin =       <&power_ctrl>,"gpios:4",
+				<&power_ctrl_pins>,"brcm,pins:0";
+		active_low =    <&power_ctrl>,"gpios:8";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-amp-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for HiFiBerry Amp/Amp+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-amp";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			tas5713@1b {
+				#sound-dai-cells = <0>;
+				compatible = "ti,tas5713";
+				reg = <0x1b>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
@@ -0,0 +1,34 @@
+// Definitions for HiFiBerry DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			pcm5102a-codec {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5102a";
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dacplus-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for HiFiBerry DAC+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-dacplus";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-digi-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for HiFiBerry Digi
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-digi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hy28a-overlay.dts
@@ -0,0 +1,87 @@
+/*
+ * Device Tree overlay for HY28A display
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			hy28a_pins: hy28a_pins {
+				brcm,pins = <17 25 18>;
+				brcm,function = <0 1 1>; /* in out out */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			hy28a: hy28a@0{
+				compatible = "ilitek,ili9320";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&hy28a_pins>;
+
+				spi-max-frequency = <32000000>;
+				spi-cpol;
+				spi-cpha;
+				rotate = <270>;
+				bgr;
+				fps = <50>;
+				buswidth = <8>;
+				startbyte = <0x70>;
+				reset-gpios = <&gpio 25 0>;
+				led-gpios = <&gpio 18 1>;
+				debug = <0>;
+			};
+
+			hy28a_ts: hy28a-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =		<&hy28a>,"spi-max-frequency:0";
+		rotate =	<&hy28a>,"rotate:0";
+		fps =		<&hy28a>,"fps:0";
+		debug =		<&hy28a>,"debug:0";
+		xohms =		<&hy28a_ts>,"ti,x-plate-ohms;0";
+		resetgpio =	<&hy28a>,"reset-gpios:4",
+				<&hy28a_pins>, "brcm,pins:1";
+		ledgpio =	<&hy28a>,"led-gpios:4",
+				<&hy28a_pins>, "brcm,pins:2";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hy28b-overlay.dts
@@ -0,0 +1,142 @@
+/*
+ * Device Tree overlay for HY28b display shield by Texy
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			hy28b_pins: hy28b_pins {
+				brcm,pins = <17 25 18>;
+				brcm,function = <0 1 1>; /* in out out */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			hy28b: hy28b@0{
+				compatible = "ilitek,ili9325";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&hy28b_pins>;
+
+				spi-max-frequency = <48000000>;
+				spi-cpol;
+				spi-cpha;
+				rotate = <270>;
+				bgr;
+				fps = <50>;
+				buswidth = <8>;
+				startbyte = <0x70>;
+				reset-gpios = <&gpio 25 0>;
+				led-gpios = <&gpio 18 1>;
+
+				gamma = "04 1F 4 7 7 0 7 7 6 0\n0F 00 1 7 4 0 0 0 6 7";
+
+				init = <0x10000e7 0x0010
+					0x1000000 0x0001
+					0x1000001 0x0100
+					0x1000002 0x0700
+				        0x1000003 0x1030
+					0x1000004 0x0000
+					0x1000008 0x0207
+					0x1000009 0x0000
+				        0x100000a 0x0000
+					0x100000c 0x0001
+					0x100000d 0x0000
+					0x100000f 0x0000
+				        0x1000010 0x0000
+					0x1000011 0x0007
+					0x1000012 0x0000
+					0x1000013 0x0000
+				        0x2000032
+					0x1000010 0x1590
+					0x1000011 0x0227
+				        0x2000032
+					0x1000012 0x009c
+				        0x2000032
+				        0x1000013 0x1900
+					0x1000029 0x0023
+					0x100002b 0x000e
+				        0x2000032
+				        0x1000020 0x0000
+					0x1000021 0x0000
+				        0x2000032
+					0x1000050 0x0000
+				        0x1000051 0x00ef
+					0x1000052 0x0000
+					0x1000053 0x013f
+					0x1000060 0xa700
+				        0x1000061 0x0001
+					0x100006a 0x0000
+					0x1000080 0x0000
+					0x1000081 0x0000
+				        0x1000082 0x0000
+					0x1000083 0x0000
+					0x1000084 0x0000
+					0x1000085 0x0000
+				        0x1000090 0x0010
+					0x1000092 0x0000
+					0x1000093 0x0003
+					0x1000095 0x0110
+				        0x1000097 0x0000
+					0x1000098 0x0000
+					0x1000007 0x0133
+					0x1000020 0x0000
+				        0x1000021 0x0000
+				        0x2000064>;
+				debug = <0>;
+			};
+
+			hy28b_ts: hy28b-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed = 	<&hy28b>,"spi-max-frequency:0";
+		rotate = 	<&hy28b>,"rotate:0";
+		fps = 		<&hy28b>,"fps:0";
+		debug = 	<&hy28b>,"debug:0";
+		xohms =		<&hy28b_ts>,"ti,x-plate-ohms;0";
+		resetgpio =	<&hy28b>,"reset-gpios:4",
+				<&hy28b_pins>, "brcm,pins:1";
+		ledgpio =	<&hy28b>,"led-gpios:4",
+				<&hy28b_pins>, "brcm,pins:2";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts
@@ -0,0 +1,55 @@
+// Definitions for several I2C based Real Time Clocks
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds1307: ds1307@68 {
+				compatible = "maxim,ds1307";
+				reg = <0x68>;
+				status = "disable";
+			};
+			mcp7941x: mcp7941x@6f {
+				compatible = "microchip,mcp7941x";
+				reg = <0x6f>;
+				status = "disable";
+			};
+			ds3231: ds3231@68 {
+				compatible = "maxim,ds3231";
+				reg = <0x68>;
+				status = "disable";
+			};
+			pcf2127: pcf2127@51 {
+				compatible = "nxp,pcf2127";
+				reg = <0x51>;
+				status = "disable";
+			};
+			pcf8523: pcf8523@68 {
+				compatible = "nxp,pcf8523";
+				reg = <0x68>;
+				status = "disable";
+			};
+			pcf8563: pcf8563@51 {
+				compatible = "nxp,pcf8563";
+				reg = <0x51>;
+				status = "disable";
+			};
+		};
+	};
+	__overrides__ {
+		ds1307 = <&ds1307>,"status";
+		ds3231 = <&ds3231>,"status";
+		mcp7941x = <&mcp7941x>,"status";
+		pcf2127 = <&pcf2127>,"status";
+		pcf8523 = <&pcf8523>,"status";
+		pcf8563 = <&pcf8563>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2s-mmap-overlay.dts
@@ -0,0 +1,13 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			brcm,enable-mmap;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for IQaudIO DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/iqaudio-dacplus-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for IQaudIO DAC+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/lirc-rpi-overlay.dts
@@ -0,0 +1,57 @@
+// Definitions for lirc-rpi module
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			lirc_rpi: lirc_rpi {
+				compatible = "rpi,lirc-rpi";
+				pinctrl-names = "default";
+				pinctrl-0 = <&lirc_pins>;
+				status = "okay";
+
+				// Override autodetection of IR receiver circuit
+				// (0 = active high, 1 = active low, -1 = no override )
+				rpi,sense = <0xffffffff>;
+
+				// Software carrier
+				// (0 = off, 1 = on)
+				rpi,softcarrier = <1>;
+
+				// Invert output
+				// (0 = off, 1 = on)
+				rpi,invert = <0>;
+
+				// Enable debugging messages
+				// (0 = off, 1 = on)
+				rpi,debug = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			lirc_pins: lirc_pins {
+				brcm,pins = <17 18>;
+				brcm,function = <1 0>; // out in
+				brcm,pull = <0 1>; // off down
+			};
+		};
+	};
+
+	__overrides__ {
+		gpio_out_pin =  <&lirc_pins>,"brcm,pins:0";
+		gpio_in_pin =   <&lirc_pins>,"brcm,pins:4";
+		gpio_in_pull =  <&lirc_pins>,"brcm,pull:4";
+
+		sense =         <&lirc_rpi>,"rpi,sense:0";
+		softcarrier =   <&lirc_rpi>,"rpi,softcarrier:0";
+		invert =        <&lirc_rpi>,"rpi,invert:0";
+		debug =         <&lirc_rpi>,"rpi,debug:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp2515-can0-overlay.dts
@@ -0,0 +1,69 @@
+/*
+ * Device tree overlay for mcp251x/can0 on spi0.0
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835", "brcm,bcm2836", "brcm,bcm2708", "brcm,bcm2709";
+    /* disable spi-dev for spi0.0 */
+    fragment@0 {
+        target = <&spi0>;
+        __overlay__ {
+            status = "okay";
+            spidev@0{
+                status = "disabled";
+            };
+        };
+    };
+
+    /* the interrupt pin of the can-controller */
+    fragment@1 {
+        target = <&gpio>;
+        __overlay__ {
+            can0_pins: can0_pins {
+                brcm,pins = <25>;
+                brcm,function = <0>; /* input */
+            };
+        };
+    };
+
+    /* the clock/oscillator of the can-controller */
+    fragment@2 {
+        target-path = "/clocks";
+        __overlay__ {
+            /* external oscillator of mcp2515 on SPI0.0 */
+            can0_osc: can0_osc {
+                compatible = "fixed-clock";
+                #clock-cells = <0>;
+                clock-frequency  = <16000000>;
+            };
+        };
+    };
+
+    /* the spi config of the can-controller itself binding everything together */
+    fragment@3 {
+        target = <&spi0>;
+        __overlay__ {
+            /* needed to avoid dtc warning */
+            #address-cells = <1>;
+            #size-cells = <0>;
+            can0: mcp2515@0 {
+                reg = <0>;
+                compatible = "microchip,mcp2515";
+                pinctrl-names = "default";
+                pinctrl-0 = <&can0_pins>;
+                spi-max-frequency = <10000000>;
+                interrupt-parent = <&gpio>;
+                interrupts = <25 0x2>;
+                clocks = <&can0_osc>;
+            };
+        };
+    };
+    __overrides__ {
+        oscillator = <&can0_osc>,"clock-frequency:0";
+        spimaxfrequency = <&can0>,"spi-max-frequency:0";
+        interrupt = <&can0_pins>,"brcm,pins:0",<&can0>,"interrupts:0";
+    };
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp2515-can1-overlay.dts
@@ -0,0 +1,69 @@
+/*
+ * Device tree overlay for mcp251x/can1 on spi0.1 edited by petit_miner
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835", "brcm,bcm2836", "brcm,bcm2708", "brcm,bcm2709";
+    /* disable spi-dev for spi0.1 */
+    fragment@0 {
+        target = <&spi0>;
+        __overlay__ {
+            status = "okay";
+            spidev@1{
+                status = "disabled";
+            };
+        };
+    };
+
+    /* the interrupt pin of the can-controller */
+    fragment@1 {
+        target = <&gpio>;
+        __overlay__ {
+            can1_pins: can1_pins {
+                brcm,pins = <25>;
+                brcm,function = <0>; /* input */
+            };
+        };
+    };
+
+    /* the clock/oscillator of the can-controller */
+    fragment@2 {
+        target-path = "/clocks";
+        __overlay__ {
+            /* external oscillator of mcp2515 on spi0.1 */
+            can1_osc: can1_osc {
+                compatible = "fixed-clock";
+                #clock-cells = <0>;
+                clock-frequency  = <16000000>;
+            };
+        };
+    };
+
+    /* the spi config of the can-controller itself binding everything together */
+    fragment@3 {
+        target = <&spi0>;
+        __overlay__ {
+            /* needed to avoid dtc warning */
+            #address-cells = <1>;
+            #size-cells = <0>;
+            can1: mcp2515@1 {
+                reg = <1>;
+                compatible = "microchip,mcp2515";
+                pinctrl-names = "default";
+                pinctrl-0 = <&can1_pins>;
+                spi-max-frequency = <10000000>;
+                interrupt-parent = <&gpio>;
+                interrupts = <25 0x2>;
+                clocks = <&can1_osc>;
+            };
+        };
+    };
+    __overrides__ {
+        oscillator = <&can1_osc>,"clock-frequency:0";
+        spimaxfrequency = <&can1>,"spi-max-frequency:0";
+        interrupt = <&can1_pins>,"brcm,pins:0",<&can1>,"interrupts:0";
+    };
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mmc-overlay.dts
@@ -0,0 +1,39 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&mmc>;
+		frag0: __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&mmc_pins>;
+			bus-width = <4>;
+			brcm,overclock-50 = <0>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			mmc_pins: mmc_pins {
+				brcm,pins = <48 49 50 51 52 53>;
+				brcm,function = <7>; /* alt3 */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sdhost>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	__overrides__ {
+		overclock_50     = <&frag0>,"brcm,overclock-50:0";
+		force_pio        = <&frag0>,"brcm,force-pio?";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mz61581-overlay.dts
@@ -0,0 +1,111 @@
+/*
+ * Device Tree overlay for MZ61581-PI-EXT 2014.12.28 by Tontec
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			mz61581_pins: mz61581_pins {
+				brcm,pins = <4 15 18 25>;
+				brcm,function = <0 1 1 1>; /* in out out out */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mz61581: mz61581@0{
+				compatible = "samsung,s6d02a1";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&mz61581_pins>;
+
+				spi-max-frequency = <128000000>;
+				spi-cpol;
+				spi-cpha;
+
+				width = <320>;
+				height = <480>;
+				rotate = <270>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				txbuflen = <32768>;
+
+				reset-gpios = <&gpio 15 0>;
+				dc-gpios = <&gpio 25 0>;
+				led-gpios = <&gpio 18 0>;
+
+				init = <0x10000b0 00
+					0x1000011
+					0x20000ff
+					0x10000b3 0x02 0x00 0x00 0x00
+					0x10000c0 0x13 0x3b 0x00 0x02 0x00 0x01 0x00 0x43
+					0x10000c1 0x08 0x16 0x08 0x08
+					0x10000c4 0x11 0x07 0x03 0x03
+					0x10000c6 0x00
+					0x10000c8 0x03 0x03 0x13 0x5c 0x03 0x07 0x14 0x08 0x00 0x21 0x08 0x14 0x07 0x53 0x0c 0x13 0x03 0x03 0x21 0x00
+					0x1000035 0x00
+					0x1000036 0xa0
+					0x100003a 0x55
+					0x1000044 0x00 0x01
+					0x10000d0 0x07 0x07 0x1d 0x03
+					0x10000d1 0x03 0x30 0x10
+					0x10000d2 0x03 0x14 0x04
+					0x1000029
+					0x100002c>;
+
+				/* This is a workaround to make sure the init sequence slows down and doesn't fail */
+				debug = <3>;
+			};
+
+			mz61581_ts: mz61581_ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <4 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 4 0>;
+
+				ti,x-plate-ohms = /bits/ 16 <60>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =   <&mz61581>, "spi-max-frequency:0";
+		rotate =  <&mz61581>, "rotate:0";
+		fps =     <&mz61581>, "fps:0";
+		txbuflen = <&mz61581>, "txbuflen:0";
+		debug =   <&mz61581>, "debug:0";
+		xohms =   <&mz61581_ts>,"ti,x-plate-ohms;0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/piscreen-overlay.dts
@@ -0,0 +1,96 @@
+/*
+ * Device Tree overlay for PiScreen 3.5" display shield by Ozzmaker
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			piscreen_pins: piscreen_pins {
+				brcm,pins = <17 25 24 22>;
+				brcm,function = <0 1 1 1>; /* in out out out */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			piscreen: piscreen@0{
+				compatible = "ilitek,ili9486";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&piscreen_pins>;
+
+				spi-max-frequency = <24000000>;
+				rotate = <270>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				regwidth = <16>;
+				reset-gpios = <&gpio 25 0>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 22 1>;
+				debug = <0>;
+
+				init = <0x10000b0 0x00
+				        0x1000011
+					0x20000ff
+					0x100003a 0x55
+					0x1000036 0x28
+					0x10000c2 0x44
+					0x10000c5 0x00 0x00 0x00 0x00
+					0x10000e0 0x0f 0x1f 0x1c 0x0c 0x0f 0x08 0x48 0x98 0x37 0x0a 0x13 0x04 0x11 0x0d 0x00
+					0x10000e1 0x0f 0x32 0x2e 0x0b 0x0d 0x05 0x47 0x75 0x37 0x06 0x10 0x03 0x24 0x20 0x00
+					0x10000e2 0x0f 0x32 0x2e 0x0b 0x0d 0x05 0x47 0x75 0x37 0x06 0x10 0x03 0x24 0x20 0x00
+					0x1000011
+					0x1000029>;
+			};
+
+			piscreen_ts: piscreen-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,swap-xy;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =		<&piscreen>,"spi-max-frequency:0";
+		rotate =	<&piscreen>,"rotate:0";
+		fps =		<&piscreen>,"fps:0";
+		debug =		<&piscreen>,"debug:0";
+		xohms =		<&piscreen_ts>,"ti,x-plate-ohms;0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pitft28-resistive-overlay.dts
@@ -0,0 +1,115 @@
+/*
+ * Device Tree overlay for Adafruit PiTFT 2.8" resistive touch screen
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			pitft_pins: pitft_pins {
+				brcm,pins = <24 25>;
+				brcm,function = <0 1>; /* in out */
+				brcm,pull = <2 0>; /* pullup none */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pitft: pitft@0{
+				compatible = "ilitek,ili9340";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pitft_pins>;
+
+				spi-max-frequency = <32000000>;
+				rotate = <90>;
+				fps = <25>;
+				bgr;
+				buswidth = <8>;
+				dc-gpios = <&gpio 25 0>;
+				debug = <0>;
+			};
+
+			pitft_ts@1 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "st,stmpe610";
+				reg = <1>;
+
+				spi-max-frequency = <500000>;
+				irq-gpio = <&gpio 24 0x2>; /* IRQF_TRIGGER_FALLING */
+				interrupts = <24 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				interrupt-controller;
+
+				stmpe_touchscreen {
+					compatible = "st,stmpe-ts";
+					st,sample-time = <4>;
+					st,mod-12b = <1>;
+					st,ref-sel = <0>;
+					st,adc-freq = <2>;
+					st,ave-ctrl = <3>;
+					st,touch-det-delay = <4>;
+					st,settling = <2>;
+					st,fraction-z = <7>;
+					st,i-drive = <0>;
+				};
+
+				stmpe_gpio: stmpe_gpio {
+					#gpio-cells = <2>;
+					compatible = "st,stmpe-gpio";
+					/*
+					 * only GPIO2 is wired/available
+					 * and it is wired to the backlight
+					 */
+					st,norequest-mask = <0x7b>;
+				};
+			};
+		};
+	};
+
+	fragment@3 {
+		target-path = "/soc";
+		__overlay__ {
+			backlight {
+				compatible = "gpio-backlight";
+				gpios = <&stmpe_gpio 2 0>;
+				default-on;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed =   <&pitft>,"spi-max-frequency:0";
+		rotate =  <&pitft>,"rotate:0";
+		fps =     <&pitft>,"fps:0";
+		debug =   <&pitft>,"debug:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pps-gpio-overlay.dts
@@ -0,0 +1,34 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			pps: pps {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&gpio 18 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			pps_pins: pps_pins {
+				brcm,pins =     <18>;
+				brcm,function = <0>;    // in
+				brcm,pull =     <0>;    // off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin = <&pps>,"gpios:4",
+			  <&pps_pins>,"brcm,pins:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts
@@ -0,0 +1,46 @@
+/dts-v1/;
+/plugin/;
+
+/*
+This is the 2-channel overlay - only use it if you need both channels.
+
+Legal pin,function combinations for each channel:
+  PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+  PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+
+N.B.:
+  1) Pin 18 is the only one available on all platforms, and
+     it is the one used by the I2S audio interface.
+     Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+  2) The onboard analogue audio output uses both PWM channels.
+  3) So be careful mixing audio and PWM.
+*/
+
+/ {
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			pwm_pins: pwm_pins {
+				brcm,pins = <18 19>;
+				brcm,function = <2 2>; /* Alt5 */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm_pins>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		pin   = <&pwm_pins>,"brcm,pins:0";
+		pin2  = <&pwm_pins>,"brcm,pins:4";
+		func  = <&pwm_pins>,"brcm,function:0";
+		func2 = <&pwm_pins>,"brcm,function:4";
+		clock = <&clk_pwm>,"clock-frequency:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pwm-overlay.dts
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/*
+Legal pin,function combinations for each channel:
+  PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+  PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+
+N.B.:
+  1) Pin 18 is the only one available on all platforms, and
+     it is the one used by the I2S audio interface.
+     Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+  2) The onboard analogue audio output uses both PWM channels.
+  3) So be careful mixing audio and PWM.
+*/
+
+/ {
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			pwm_pins: pwm_pins {
+				brcm,pins = <18>;
+				brcm,function = <2>; /* Alt5 */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm_pins>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		pin   = <&pwm_pins>,"brcm,pins:0";
+		func  = <&pwm_pins>,"brcm,function:0";
+		clock = <&clk_pwm>,"clock-frequency:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/raspidac3-overlay.dts
@@ -0,0 +1,45 @@
+// Definitions for RaspiDACv3
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "jg,raspidacv3";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				status = "okay";
+			};
+
+			tpa6130a2: tpa6130a2@60 {
+				compatible = "ti,tpa6130a2";
+				reg = <0x60>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-dac-overlay.dts
@@ -0,0 +1,34 @@
+// Definitions for RPi DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "rpi,rpi-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			pcm1794a-codec {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm1794a";
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-display-overlay.dts
@@ -0,0 +1,82 @@
+/*
+ * Device Tree overlay for rpi-display by Watterott
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			rpi_display_pins: rpi_display_pins {
+				brcm,pins = <18 23 24 25>;
+				brcm,function = <1 1 1 0>; /* out out out in */
+				brcm,pull = <0 0 0 2>; /* - - - up */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rpidisplay: rpi-display@0{
+				compatible = "ilitek,ili9341";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&rpi_display_pins>;
+
+				spi-max-frequency = <32000000>;
+				rotate = <270>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				reset-gpios = <&gpio 23 0>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 18 1>;
+				debug = <0>;
+			};
+
+			rpidisplay_ts: rpi-display-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <25 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 25 0>;
+				ti,x-plate-ohms = /bits/ 16 <60>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =   <&rpidisplay>,"spi-max-frequency:0";
+		rotate =  <&rpidisplay>,"rotate:0";
+		fps =     <&rpidisplay>,"fps:0";
+		debug =   <&rpidisplay>,"debug:0";
+		xohms =   <&rpidisplay_ts>,"ti,x-plate-ohms;0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts
@@ -0,0 +1,17 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			rpi_ft5406: rpi_ft5406 {
+				compatible = "rpi,rpi-ft5406";
+				firmware = <&firmware>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-proto-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for Rpi-Proto
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "rpi,rpi-proto";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8731@1a {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8731";
+				reg = <0x1a>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
@@ -0,0 +1,47 @@
+// rpi-sense HAT
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rpi-sense@46 {
+				compatible = "rpi,rpi-sense";
+				reg = <0x46>;
+				keys-int-gpios = <&gpio 23 1>;
+				status = "okay";
+			};
+
+			lsm9ds1-magn@1c {
+				compatible = "st,lsm9ds1-magn";
+				reg = <0x1c>;
+				status = "okay";
+			};
+
+			lsm9ds1-accel6a {
+				compatible = "st,lsm9ds1-accel";
+				reg = <0x6a>;
+				status = "okay";
+			};
+
+			lps25h-press@5c {
+				compatible = "st,lps25h-press";
+				reg = <0x5c>;
+				status = "okay";
+			};
+
+			hts221-humid@5f {
+				compatible = "st,hts221-humid";
+				reg = <0x5f>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sdhost-overlay.dts
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&mmc>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&sdhost>;
+		frag1: __overlay__ {
+			brcm,overclock-50 = <0>;
+			brcm,pio-limit = <1>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		overclock_50     = <&frag1>,"brcm,overclock-50:0";
+		force_pio        = <&frag1>,"brcm,force-pio?";
+		pio_limit        = <&frag1>,"brcm,pio-limit:0";
+		debug            = <&frag1>,"brcm,debug?";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sdio-overlay.dts
@@ -0,0 +1,32 @@
+/* Enable SDIO from MMC interface via GPIOs 22-27. Includes sdhost overlay. */
+
+/include/ "sdhost-overlay.dts"
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@3 {
+		target = <&mmc>;
+		sdio_mmc: __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&sdio_pins>;
+			non-removable;
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target = <&gpio>;
+		__overlay__ {
+			sdio_pins: sdio_pins {
+				brcm,pins = <22 23 24 25 26 27>;
+				brcm,function = <7 7 7 7 7 7>; /* ALT3 = SD1 */
+				brcm,pull = <0 2 2 2 2 2>;
+			};
+		};
+	};
+
+	__overrides__ {
+		poll_once = <&sdio_mmc>,"non-removable?";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/smi-dev-overlay.dts
@@ -0,0 +1,18 @@
+// Description: Overlay to enable character device interface for SMI.
+// Author:	Luke Wren <luke@raspberrypi.org>
+
+/dts-v1/;
+/plugin/;
+
+/{
+	fragment@0 {
+		target = <&soc>;
+		__overlay__ {
+			smi_dev {
+				compatible = "brcm,bcm2835-smi-dev";
+				smi_handle = <&smi>;
+				status = "okay";
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/smi-nand-overlay.dts
@@ -0,0 +1,69 @@
+// Description: Overlay to enable NAND flash through
+// the secondary memory interface
+// Author:	Luke Wren
+
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&smi>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&smi_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&soc>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			nand: flash@0 {
+				compatible = "brcm,bcm2835-smi-nand";
+				smi_handle = <&smi>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				status = "okay";
+
+				partition@0 {
+					label = "stage2";
+					// 128k
+					reg = <0 0x20000>;
+					read-only;
+				};
+				partition@1 {
+					label = "firmware";
+					// 16M
+					reg = <0x20000 0x1000000>;
+					read-only;
+				};
+				partition@2 {
+					label = "root";
+					// 2G (will need to use 64 bit for >=4G)
+					reg = <0x1020000 0x80000000>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			smi_pins: smi_pins {
+				brcm,pins = <0 1 2 3 4 5 6 7 8 9 10 11
+					12 13 14 15>;
+				/* Alt 1: SMI */
+				brcm,function = <5 5 5 5 5 5 5 5 5 5 5
+					5 5 5 5 5>;
+				/* /CS, /WE and /OE are pulled high, as they are
+				   generally active low signals */
+				brcm,pull = <2 2 2 2 2 2 2 2 0 0 0 0 0 0 0 0>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/smi-overlay.dts
@@ -0,0 +1,37 @@
+// Description:	Overlay to enable the secondary memory interface peripheral
+// Author:	Luke Wren
+
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&smi>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&smi_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			smi_pins: smi_pins {
+				/* Don't configure the top two address bits, as
+				   these are already used as ID_SD and ID_SC */
+				brcm,pins = <2 3 4 5 6 7 8 9 10 11 12 13 14 15
+					     16 17 18 19 20 21 22 23 24 25>;
+				/* Alt 0: SMI */
+				brcm,function = <5 5 5 5 5 5 5 5 5 5 5 5 5 5 5
+						 5 5 5 5 5 5 5 5 5>;
+				/* /CS, /WE and /OE are pulled high, as they are
+				   generally active low signals */
+				brcm,pull = <2 2 2 2 2 2 0 0 0 0 0 0 0 0 0 0 0
+					     0 0 0 0 0 0 0>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi-gpio35-39-overlay.dts
@@ -0,0 +1,31 @@
+/*
+ * Device tree overlay to move spi0 to gpio 35 to 39 on CM
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2836", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			cs-gpios = <&gpio 36 1>, <&gpio 35 1>;
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0_cs_pins>;
+		__overlay__ {
+			bcrm,pins = <36 35>;
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0_pins>;
+		__overlay__ {
+			bcrm,pins = <37 38 39>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/tinylcd35-overlay.dts
@@ -0,0 +1,216 @@
+/*
+ * tinylcd35-overlay.dts
+ *
+ * -------------------------------------------------
+ * www.tinlylcd.com
+ * -------------------------------------------------
+ * Device---Driver-----BUS       GPIO's
+ * display  tinylcd35  spi0.0    25 24 18
+ * touch    ads7846    spi0.1    5
+ * rtc      ds1307     i2c1-0068
+ * rtc      pcf8563    i2c1-0051
+ * keypad   gpio-keys  --------- 17 22 27 23 28
+ *
+ *
+ * TinyLCD.com 3.5 inch TFT
+ *
+ *  Version 001
+ *  5/3/2015  -- Noralf Trønnes     Initial Device tree framework
+ *  10/3/2015 -- tinylcd@gmail.com  added ds1307 support.
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835", "brcm,bcm2708", "brcm,bcm2709";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			tinylcd35_pins: tinylcd35_pins {
+				brcm,pins = <25 24 18>;
+				brcm,function = <1>; /* out */
+			};
+			tinylcd35_ts_pins: tinylcd35_ts_pins {
+				brcm,pins = <5>;
+				brcm,function = <0>; /* in */
+			};
+			keypad_pins: keypad_pins {
+				brcm,pins = <4 17 22 23 27>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <1>; /* down */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			tinylcd35: tinylcd35@0{
+				compatible = "neosec,tinylcd";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&tinylcd35_pins>,
+					    <&tinylcd35_ts_pins>;
+
+				spi-max-frequency = <48000000>;
+				rotate = <270>;
+				fps = <20>;
+				bgr;
+				buswidth = <8>;
+				reset-gpios = <&gpio 25 0>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 18 1>;
+				debug = <0>;
+
+				init = <0x10000B0 0x80
+					0x10000C0 0x0A 0x0A
+					0x10000C1 0x01 0x01
+					0x10000C2 0x33
+					0x10000C5 0x00 0x42 0x80
+					0x10000B1 0xD0 0x11
+					0x10000B4 0x02
+					0x10000B6 0x00 0x22 0x3B
+					0x10000B7 0x07
+					0x1000036 0x58
+					0x10000F0 0x36 0xA5 0xD3
+					0x10000E5 0x80
+					0x10000E5 0x01
+					0x10000B3 0x00
+					0x10000E5 0x00
+					0x10000F0 0x36 0xA5 0x53
+					0x10000E0 0x00 0x35 0x33 0x00 0x00 0x00 0x00 0x35 0x33 0x00 0x00 0x00
+					0x100003A 0x55
+					0x1000011
+					0x2000001
+					0x1000029>;
+			};
+
+			tinylcd35_ts: tinylcd35_ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+				status = "disabled";
+
+				spi-max-frequency = <2000000>;
+				interrupts = <5 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 5 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+
+	/*  RTC    */
+
+	fragment@3 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pcf8563: pcf8563@51 {
+				compatible = "nxp,pcf8563";
+				reg = <0x51>;
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			ds1307: ds1307@68 {
+				compatible = "maxim,ds1307";
+				reg = <0x68>;
+				status = "disabled";
+			};
+		};
+	};
+
+	/*
+	 * Values for input event code is found under the
+	 * 'Keys and buttons' heading in include/uapi/linux/input.h
+	 */
+	fragment@5 {
+		target-path = "/soc";
+		__overlay__ {
+			keypad: keypad {
+				compatible = "gpio-keys";
+				#address-cells = <1>;
+				#size-cells = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&keypad_pins>;
+				status = "disabled";
+				autorepeat;
+
+				button@17 {
+					label = "GPIO KEY_UP";
+					linux,code = <103>;
+					gpios = <&gpio 17 0>;
+				};
+				button@22 {
+					label = "GPIO KEY_DOWN";
+					linux,code = <108>;
+					gpios = <&gpio 22 0>;
+				};
+				button@27 {
+					label = "GPIO KEY_LEFT";
+					linux,code = <105>;
+					gpios = <&gpio 27 0>;
+				};
+				button@23 {
+					label = "GPIO KEY_RIGHT";
+					linux,code = <106>;
+					gpios = <&gpio 23 0>;
+				};
+				button@4 {
+					label = "GPIO KEY_ENTER";
+					linux,code = <28>;
+					gpios = <&gpio 4 0>;
+				};
+			};
+		};
+	};
+
+	__overrides__ {
+		speed =      <&tinylcd35>,"spi-max-frequency:0";
+		rotate =     <&tinylcd35>,"rotate:0";
+		fps =        <&tinylcd35>,"fps:0";
+		debug =      <&tinylcd35>,"debug:0";
+		touch =      <&tinylcd35_ts>,"status";
+		touchgpio =  <&tinylcd35_ts_pins>,"brcm,pins:0",
+			     <&tinylcd35_ts>,"interrupts:0",
+			     <&tinylcd35_ts>,"pendown-gpio:4";
+		xohms =      <&tinylcd35_ts>,"ti,x-plate-ohms;0";
+		rtc-pcf =    <&i2c1>,"status",
+			     <&pcf8563>,"status";
+		rtc-ds =     <&i2c1>,"status",
+			     <&ds1307>,"status";
+		keypad =     <&keypad>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart1-overlay.dts
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&uart1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			uart1_pins: uart1_pins {
+				brcm,pins = <14 15>;
+				brcm,function = <2>; /* alt5 */
+				brcm,pull = <0 2>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target-path = "/chosen";
+		__overlay__ {
+			bootargs = "8250.nr_uarts=1";
+		};
+	};
+
+	__overrides__ {
+		txd1_pin = <&uart1_pins>,"brcm,pins:0";
+		rxd1_pin = <&uart1_pins>,"brcm,pins:4";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/vga666-overlay.dts
@@ -0,0 +1,30 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2708";
+
+	// There is no VGA driver module, but we need a platform device
+	// node (that doesn't already use pinctrl) to hang the pinctrl
+	// reference on - leds will do
+
+	fragment@0 {
+		target = <&leds>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&vga666_pins>;
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			vga666_pins: vga666_pins {
+				brcm,pins = <2 3 4 5 6 7 8 9 10 11 12
+					     13 14 15 16 17 18 19 20 21>;
+				brcm,function = <6>; /* alt2 */
+				brcm,pull = <0>; /* no pull */
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/w1-gpio-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for w1-gpio module (without external pullup)
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+
+			w1: onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&gpio 4 0>;
+				rpi,parasitic-power = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				brcm,pins = <4>;
+				brcm,function = <0>; // in (initially)
+				brcm,pull = <0>; // off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin =       <&w1>,"gpios:4",
+				<&w1_pins>,"brcm,pins:0";
+		pullup =        <&w1>,"rpi,parasitic-power:0";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/w1-gpio-pullup-overlay.dts
@@ -0,0 +1,41 @@
+// Definitions for w1-gpio module (with external pullup)
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+
+			w1: onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&gpio 4 0>, <&gpio 5 1>;
+				rpi,parasitic-power = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				brcm,pins = <4 5>;
+				brcm,function = <0 1>; // in out
+				brcm,pull = <0 0>; // off off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin =       <&w1>,"gpios:4",
+				<&w1_pins>,"brcm,pins:0";
+		extpullup =     <&w1>,"gpios:16",
+				<&w1_pins>,"brcm,pins:4";
+		pullup =        <&w1>,"rpi,parasitic-power:0";
+	};
+};
