From a5b8204a864f7f9a5a30c6b673e735138c3bdba3 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 15 Mar 2016 15:49:16 +0000
Subject: [PATCH 186/381] BCM270X_DT: Add labels to spidev nodes

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts | 4 ++--
 arch/arm/boot/dts/bcm2708-rpi-b.dts      | 4 ++--
 arch/arm/boot/dts/bcm2708-rpi-cm.dts     | 4 ++--
 arch/arm/boot/dts/bcm2709-rpi-2-b.dts    | 4 ++--
 arch/arm/boot/dts/bcm2710-rpi-3-b.dts    | 4 ++--
 5 files changed, 10 insertions(+), 10 deletions(-)

--- a/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
@@ -59,7 +59,7 @@
 	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
 	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
 
-	spidev@0{
+	spidev0: spidev@0{
 		compatible = "spidev";
 		reg = <0>;	/* CE0 */
 		#address-cells = <1>;
@@ -67,7 +67,7 @@
 		spi-max-frequency = <500000>;
 	};
 
-	spidev@1{
+	spidev1: spidev@1{
 		compatible = "spidev";
 		reg = <1>;	/* CE1 */
 		#address-cells = <1>;
--- a/arch/arm/boot/dts/bcm2708-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b.dts
@@ -59,7 +59,7 @@
 	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
 	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
 
-	spidev@0{
+	spidev0: spidev@0{
 		compatible = "spidev";
 		reg = <0>;	/* CE0 */
 		#address-cells = <1>;
@@ -67,7 +67,7 @@
 		spi-max-frequency = <500000>;
 	};
 
-	spidev@1{
+	spidev1: spidev@1{
 		compatible = "spidev";
 		reg = <1>;	/* CE1 */
 		#address-cells = <1>;
--- a/arch/arm/boot/dts/bcm2708-rpi-cm.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
@@ -42,7 +42,7 @@
 	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
 	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
 
-	spidev@0{
+	spidev0: spidev@0{
 		compatible = "spidev";
 		reg = <0>;	/* CE0 */
 		#address-cells = <1>;
@@ -50,7 +50,7 @@
 		spi-max-frequency = <500000>;
 	};
 
-	spidev@1{
+	spidev1: spidev@1{
 		compatible = "spidev";
 		reg = <1>;	/* CE1 */
 		#address-cells = <1>;
--- a/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
+++ b/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
@@ -59,7 +59,7 @@
 	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
 	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
 
-	spidev@0{
+	spidev0: spidev@0{
 		compatible = "spidev";
 		reg = <0>;	/* CE0 */
 		#address-cells = <1>;
@@ -67,7 +67,7 @@
 		spi-max-frequency = <500000>;
 	};
 
-	spidev@1{
+	spidev1: spidev@1{
 		compatible = "spidev";
 		reg = <1>;	/* CE1 */
 		#address-cells = <1>;
--- a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -110,7 +110,7 @@
 	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
 	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
 
-	spidev@0{
+	spidev0: spidev@0{
 		compatible = "spidev";
 		reg = <0>;	/* CE0 */
 		#address-cells = <1>;
@@ -118,7 +118,7 @@
 		spi-max-frequency = <500000>;
 	};
 
-	spidev@1{
+	spidev1: spidev@1{
 		compatible = "spidev";
 		reg = <1>;	/* CE1 */
 		#address-cells = <1>;
