From 84e674b139553b74fa118a3e41ba6ca31e2c0750 Mon Sep 17 00:00:00 2001
From: DigitalDreamtime <clive.messer@digitaldreamtime.co.uk>
Date: Thu, 14 Apr 2016 01:00:58 +0100
Subject: [PATCH 240/381] Add support for the Digital Dreamtime Akkordion music
 player.

Support the Digital Dreamtime Akkordion using the OEM IQAudIO DAC+ or
DACZero modules. Set ALSA card name, ("Akkordion"), from dt config.

Signed-off-by: DigitalDreamtime <clive.messer@digitaldreamtime.co.uk>
---
 arch/arm/boot/dts/overlays/Makefile                |  1 +
 arch/arm/boot/dts/overlays/README                  | 20 ++++++++++
 .../dts/overlays/akkordion-iqdacplus-overlay.dts   | 46 ++++++++++++++++++++++
 3 files changed, 67 insertions(+)
 create mode 100644 arch/arm/boot/dts/overlays/akkordion-iqdacplus-overlay.dts

--- a/arch/arm/boot/dts/overlays/Makefile
+++ b/arch/arm/boot/dts/overlays/Makefile
@@ -13,6 +13,7 @@ ifeq ($(CONFIG_ARCH_BCM2835),y)
 endif
 
 dtbo-$(RPI_DT_OVERLAYS) += ads7846.dtbo
+dtbo-$(RPI_DT_OVERLAYS) += akkordion-iqdacplus.dtbo
 dtbo-$(RPI_DT_OVERLAYS) += at86rf233.dtbo
 dtbo-$(RPI_DT_OVERLAYS) += bmp085_i2c-sensor.dtbo
 dtbo-$(RPI_DT_OVERLAYS) += dpi24.dtbo
--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -186,6 +186,26 @@ Params: cs                      SPI bus
         www.kernel.org/doc/Documentation/devicetree/bindings/input/ads7846.txt
 
 
+Name:   akkordion-iqdacplus
+Info:   Configures the Digital Dreamtime Akkordion Music Player (based on the
+        OEM IQAudIO DAC+ or DAC Zero module).
+Load:   dtoverlay=akkordion-iqdacplus,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                dtoverlay=akkordion-iqdacplus,24db_digital_gain
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
 Name:   at86rf233
 Info:   Configures the Atmel AT86RF233 802.15.4 low-power WPAN transceiver,
         connected to spi0.0
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/akkordion-iqdacplus-overlay.dts
@@ -0,0 +1,46 @@
+// Definitions for Digital Dreamtime Akkordion using IQaudIO DAC+ or DACZero
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&sound>;
+		frag0: __overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			card_name = "Akkordion";
+			dai_name = "IQaudIO DAC";
+			dai_stream_name = "IQaudIO DAC HiFi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&frag0>,"iqaudio,24db_digital_gain?";
+	};
+};
