#!/bin/sh
#
# Copyright (C) 2014-2016 OpenWrt.org
# Copyright (C) 2016 LEDE-Project.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
armada-385-linksys-caiman)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:caiman:white:wan" "eth1"
	ucidef_set_led_usbport "usb1" "USB 1" "pca963x:caiman:white:usb2" "usb1-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "pca963x:caiman:white:usb3_1" "usb2-port1" "usb3-port1"
	ucidef_set_led_usbport "usb2_ss" "USB 2 SS" "pca963x:caiman:white:usb3_2" "usb3-port1"
	;;
armada-385-linksys-cobra)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:cobra:white:wan" "eth1"
	ucidef_set_led_usbport "usb1" "USB 1" "pca963x:cobra:white:usb2" "usb1-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "pca963x:cobra:white:usb3_1" "usb2-port1" "usb3-port1"
	ucidef_set_led_usbport "usb2_ss" "USB 2 SS" "pca963x:cobra:white:usb3_2" "usb3-port1"
	;;
armada-385-linksys-rango)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:rango:white:wan" "eth1"
	ucidef_set_led_usbport "usb1" "USB 1" "pca963x:rango:white:usb2" "usb1-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "pca963x:rango:white:usb3_1" "usb2-port1" "usb3-port1"
	ucidef_set_led_usbport "usb2_ss" "USB 2 SS" "pca963x:rango:white:usb3_2" "usb3-port1"
	;;
armada-385-linksys-shelby)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:shelby:white:wan" "eth1"
	ucidef_set_led_usbport "usb1" "USB 1" "pca963x:shelby:white:usb2" "usb1-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "pca963x:shelby:white:usb3_1" "usb2-port1" "usb3-port1"
	ucidef_set_led_usbport "usb2_ss" "USB 2 SS" "pca963x:shelby:white:usb3_2" "usb3-port1"
	;;
armada-385-linksys-venom)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:venom:blue:wan" "eth1"
	ucidef_set_led_usbport "usb1" "USB 1" "pca963x:venom:blue:usb2" "usb1-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "pca963x:venom:blue:usb3_1" "usb2-port1" "usb3-port1"
	ucidef_set_led_usbport "usb2_ss" "USB 2 SS" "pca963x:venom:blue:usb3_2" "usb3-port1"
	;;
armada-xp-linksys-mamba)
	ucidef_set_led_netdev "wan" "WAN" "mamba:white:wan" "eth1"
	ucidef_set_led_usbport "usb1" "USB 1" "mamba:white:usb2" "usb1-port1"
	ucidef_set_led_usbport "usb2" "USB 2" "mamba:white:usb3_1" "usb2-port1" "usb3-port1"
	ucidef_set_led_usbport "usb2_ss" "USB 2 SS" "mamba:white:usb3_2" "usb3-port2"
	;;

esac

board_config_flush

exit 0
