From e74caf41aec5338b8cbbd0a1483650848f16f532 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Sun, 16 Jul 2017 12:23:47 +0200
Subject: [PATCH V2 1/8] MIPS: BCM63XX: add clkdev lookup support

Enable clkdev lookup support to allow us providing clocks under
different names to devices more easily, so we don't need to care
about clock name clashes anymore.

Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 arch/mips/Kconfig       |   1 +
 arch/mips/bcm63xx/clk.c | 150 +++++++++++++++++++++++++++++++++++++-----------
 2 files changed, 116 insertions(+), 35 deletions(-)

--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -279,6 +279,7 @@ config BCM63XX
 	select GPIOLIB
 	select HAVE_CLK
 	select MIPS_L1_CACHE_SHIFT_4
+	select CLKDEV_LOOKUP
 	help
 	 Support for BCM63XX based boards
 
--- a/arch/mips/bcm63xx/clk.c
+++ b/arch/mips/bcm63xx/clk.c
@@ -11,6 +11,7 @@
 #include <linux/mutex.h>
 #include <linux/err.h>
 #include <linux/clk.h>
+#include <linux/clkdev.h>
 #include <linux/delay.h>
 #include <bcm63xx_cpu.h>
 #include <bcm63xx_io.h>
@@ -359,44 +360,103 @@ long clk_round_rate(struct clk *clk, uns
 }
 EXPORT_SYMBOL_GPL(clk_round_rate);
 
-struct clk *clk_get(struct device *dev, const char *id)
-{
-	if (!strcmp(id, "enet0"))
-		return &clk_enet0;
-	if (!strcmp(id, "enet1"))
-		return &clk_enet1;
-	if (!strcmp(id, "enetsw"))
-		return &clk_enetsw;
-	if (!strcmp(id, "ephy"))
-		return &clk_ephy;
-	if (!strcmp(id, "usbh"))
-		return &clk_usbh;
-	if (!strcmp(id, "usbd"))
-		return &clk_usbd;
-	if (!strcmp(id, "spi"))
-		return &clk_spi;
-	if (!strcmp(id, "hsspi"))
-		return &clk_hsspi;
-	if (!strcmp(id, "xtm"))
-		return &clk_xtm;
-	if (!strcmp(id, "periph"))
-		return &clk_periph;
-	if ((BCMCPU_IS_3368() || BCMCPU_IS_6358()) && !strcmp(id, "pcm"))
-		return &clk_pcm;
-	if ((BCMCPU_IS_6362() || BCMCPU_IS_6368()) && !strcmp(id, "ipsec"))
-		return &clk_ipsec;
-	if ((BCMCPU_IS_6328() || BCMCPU_IS_6362()) && !strcmp(id, "pcie"))
-		return &clk_pcie;
-	return ERR_PTR(-ENOENT);
-}
-
-EXPORT_SYMBOL(clk_get);
-
-void clk_put(struct clk *clk)
-{
-}
-
-EXPORT_SYMBOL(clk_put);
+static struct clk_lookup bcm3368_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enet0", &clk_enet0),
+	CLKDEV_INIT(NULL, "enet1", &clk_enet1),
+	CLKDEV_INIT(NULL, "ephy", &clk_ephy),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+	CLKDEV_INIT(NULL, "pcm", &clk_pcm),
+};
+
+static struct clk_lookup bcm6328_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enetsw", &clk_enetsw),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "hsspi", &clk_hsspi),
+	CLKDEV_INIT(NULL, "pcie", &clk_pcie),
+};
+
+static struct clk_lookup bcm6338_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enet0", &clk_enet0),
+	CLKDEV_INIT(NULL, "enet1", &clk_enet1),
+	CLKDEV_INIT(NULL, "ephy", &clk_ephy),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+};
+
+static struct clk_lookup bcm6345_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enet0", &clk_enet0),
+	CLKDEV_INIT(NULL, "enet1", &clk_enet1),
+	CLKDEV_INIT(NULL, "ephy", &clk_ephy),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+};
+
+static struct clk_lookup bcm6348_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enet0", &clk_enet0),
+	CLKDEV_INIT(NULL, "enet1", &clk_enet1),
+	CLKDEV_INIT(NULL, "ephy", &clk_ephy),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+};
+
+static struct clk_lookup bcm6358_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enet0", &clk_enet0),
+	CLKDEV_INIT(NULL, "enet1", &clk_enet1),
+	CLKDEV_INIT(NULL, "ephy", &clk_ephy),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+	CLKDEV_INIT(NULL, "pcm", &clk_pcm),
+};
+
+static struct clk_lookup bcm6362_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enetsw", &clk_enetsw),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+	CLKDEV_INIT(NULL, "hsspi", &clk_hsspi),
+	CLKDEV_INIT(NULL, "pcie", &clk_pcie),
+	CLKDEV_INIT(NULL, "ipsec", &clk_ipsec),
+};
+
+static struct clk_lookup bcm6368_clks[] = {
+	/* fixed rate clocks */
+	CLKDEV_INIT(NULL, "periph", &clk_periph),
+	/* gated clocks */
+	CLKDEV_INIT(NULL, "enetsw", &clk_enetsw),
+	CLKDEV_INIT(NULL, "usbh", &clk_usbh),
+	CLKDEV_INIT(NULL, "usbd", &clk_usbd),
+	CLKDEV_INIT(NULL, "spi", &clk_spi),
+	CLKDEV_INIT(NULL, "xtm", &clk_xtm),
+	CLKDEV_INIT(NULL, "ipsec", &clk_ipsec),
+};
 
 #define HSSPI_PLL_HZ_6328	133333333
 #define HSSPI_PLL_HZ_6362	400000000
@@ -404,11 +464,31 @@ EXPORT_SYMBOL(clk_put);
 static int __init bcm63xx_clk_init(void)
 {
 	switch (bcm63xx_get_cpu_id()) {
+	case BCM3368_CPU_ID:
+		clkdev_add_table(bcm3368_clks, ARRAY_SIZE(bcm3368_clks));
+		break;
 	case BCM6328_CPU_ID:
 		clk_hsspi.rate = HSSPI_PLL_HZ_6328;
+		clkdev_add_table(bcm6328_clks, ARRAY_SIZE(bcm6328_clks));
+		break;
+	case BCM6338_CPU_ID:
+		clkdev_add_table(bcm6338_clks, ARRAY_SIZE(bcm6338_clks));
+		break;
+	case BCM6345_CPU_ID:
+		clkdev_add_table(bcm6345_clks, ARRAY_SIZE(bcm6345_clks));
+		break;
+	case BCM6348_CPU_ID:
+		clkdev_add_table(bcm6348_clks, ARRAY_SIZE(bcm6348_clks));
+		break;
+	case BCM6358_CPU_ID:
+		clkdev_add_table(bcm6358_clks, ARRAY_SIZE(bcm6358_clks));
 		break;
 	case BCM6362_CPU_ID:
 		clk_hsspi.rate = HSSPI_PLL_HZ_6362;
+		clkdev_add_table(bcm6362_clks, ARRAY_SIZE(bcm6362_clks));
+		break;
+	case BCM6368_CPU_ID:
+		clkdev_add_table(bcm6368_clks, ARRAY_SIZE(bcm6368_clks));
 		break;
 	}
 
